## MMModemCdma MMModemCdma — The CDMA interface |

## Functions

const gchar * | mm_modem_cdma_get_path ()
gchar * | mm_modem_cdma_dup_path ()
const gchar * | mm_modem_cdma_get_esn ()
gchar * | mm_modem_cdma_dup_esn ()
const gchar * | mm_modem_cdma_get_meid ()
gchar * | mm_modem_cdma_dup_meid ()
guint | mm_modem_cdma_get_nid ()
guint | mm_modem_cdma_get_sid ()
MMModemCdmaRegistrationState | mm_modem_cdma_get_cdma1x_registration_state ()
MMModemCdmaRegistrationState | mm_modem_cdma_get_evdo_registration_state ()
MMModemCdmaActivationState | mm_modem_cdma_get_activation_state ()
void | mm_modem_cdma_activate ()
gboolean | mm_modem_cdma_activate_finish ()
gboolean | mm_modem_cdma_activate_sync ()
void | mm_modem_cdma_activate_manual ()
gboolean | mm_modem_cdma_activate_manual_finish ()
gboolean | mm_modem_cdma_activate_manual_sync ()

## Types and Values

struct | MMModemCdma
#define | MM_MODEM_CDMA_NID_UNKNOWN
#define | MM_MODEM_CDMA_SID_UNKNOWN

## Object Hierarchy

        GObject
        ╰── GDBusProxy
            ╰── MmGdbusModemCdmaProxy
                ╰── MMModemCdma

## Implemented Interfaces

MMModemCdma implements GDBusInterface, GInitable, GAsyncInitable and MmGdbusModemCdma.

## Description

The MMModemCdma is an object providing access to the methods, signals and properties of the CDMA interface.

The CDMA interface is exposed whenever a modem has CDMA capabilities (`MM_MODEM_CAPABILITY_CDMA_EVDO`).

## Functions

### mm_modem_cdma_get_path ()

    const gchar *
    mm_modem_cdma_get_path (MMModemCdma *self);

Gets the DBus path of the MMObject which implements this interface.

#### Parameters

self | A MMModemCdma. |

#### Returns

The DBus path of the MMObject object.

[transfer none]

Since: 1.0

### mm_modem_cdma_dup_path ()

    gchar *
    mm_modem_cdma_dup_path (MMModemCdma *self);

Gets a copy of the DBus path of the MMObject object which implements this interface.

#### Parameters

self | A MMModemCdma. |

#### Returns

The DBus path of the MMObject. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_cdma_get_esn ()

    const gchar *
    mm_modem_cdma_get_esn (MMModemCdma *self);

Gets the

Electronic Serial Number,

as reported by this MMModemCdma.

The ESN is superceded by MEID, but still used in older devices.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_cdma_dup_esn()` if on another thread.

#### Parameters

self | A MMModemCdma. |

#### Returns

The ESN, or `NULL` if none available.

[transfer none]

Since: 1.0

### mm_modem_cdma_dup_esn ()

    gchar *
    mm_modem_cdma_dup_esn (MMModemCdma *self);

Gets a copy of the

Electronic Serial Number,

as reported by this MMModemCdma.

The ESN is superceded by MEID, but still used in older devices.

#### Parameters

self | A MMModemCdma. |

#### Returns

The ESN, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_cdma_get_meid ()

    const gchar *
    mm_modem_cdma_get_meid (MMModemCdma *self);

Gets the

Mobile Equipment Identifier,

as reported by this MMModemCdma.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_cdma_dup_meid()` if on another thread.

#### Parameters

self | A MMModemCdma. |

#### Returns

The MEID, or `NULL` if none available.

[transfer none]

Since: 1.0

### mm_modem_cdma_dup_meid ()

    gchar *
    mm_modem_cdma_dup_meid (MMModemCdma *self);

Gets a copy of the

Mobile Equipment Identifier,

as reported by this MMModemCdma.

#### Parameters

self | A MMModemCdma. |

#### Returns

The MEID, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_cdma_get_nid ()

    guint
    mm_modem_cdma_get_nid (MMModemCdma *self);

Gets the

Network Identifier

of the serving CDMA 1x network, if known, and if the modem is registered with a CDMA 1x network.

#### Parameters

self | A MMModemCdma. |

#### Returns

The NID, or `MM_MODEM_CDMA_NID_UNKNOWN`.

Since: 1.0

### mm_modem_cdma_get_sid ()

    guint
    mm_modem_cdma_get_sid (MMModemCdma *self);

Gets the

System Identifier

of the serving CDMA 1x network, if known, and if the modem is registered with a CDMA 1x network.

#### Parameters

self | A MMModemCdma. |

#### Returns

The SID, or `MM_MODEM_CDMA_SID_UNKNOWN`.

Since: 1.0

### mm_modem_cdma_get_cdma1x_registration_state ()

    MMModemCdmaRegistrationState
    mm_modem_cdma_get_cdma1x_registration_state
                                   (MMModemCdma *self);

Gets the state of the registration in the CDMA 1x network.

#### Parameters

self | A MMModemCdma. |

#### Returns

a MMModemCdmaRegistrationState.

Since: 1.0

### mm_modem_cdma_get_evdo_registration_state ()

    MMModemCdmaRegistrationState
    mm_modem_cdma_get_evdo_registration_state
                                   (MMModemCdma *self);

Gets the state of the registration in the EV-DO network.

#### Parameters

self | A MMModemCdma. |

#### Returns

a MMModemCdmaRegistrationState.

Since: 1.0

### mm_modem_cdma_get_activation_state ()

    MMModemCdmaActivationState
    mm_modem_cdma_get_activation_state (MMModemCdma *self);

Gets the state of the activation in the 3GPP2 network.

#### Parameters

self | A MMModemCdma. |

#### Returns

a MMModemCdmaActivationState.

Since: 1.0

### mm_modem_cdma_activate ()

    void
    mm_modem_cdma_activate (MMModemCdma *self,
                            const gchar *carrier,
                            GCancellable *cancellable,
                            GAsyncReadyCallback callback,
                            gpointer user_data);

Asynchronously requests to provision the modem for use with a given carrier using the modem's OTA activation functionality, if any.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_cdma_activate_finish()` to get the result of the operation.

See `mm_modem_cdma_activate_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemCdma. |
carrier | Name of the carrier. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_cdma_activate_finish ()

    gboolean
    mm_modem_cdma_activate_finish (MMModemCdma *self,
                                   GAsyncResult *res,
                                   GError **error);

Finishes an operation started with `mm_modem_cdma_activate()`.

#### Parameters

self | A MMModemCdma. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_cdma_activate()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the activation was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_cdma_activate_sync ()

    gboolean
    mm_modem_cdma_activate_sync (MMModemCdma *self,
                                 const gchar *carrier,
                                 GCancellable *cancellable,
                                 GError **error);

Synchronously requests to provision the modem for use with a given carrier using the modem's OTA activation functionality, if any.

The calling thread is blocked until a reply is received. See `mm_modem_cdma_activate()` for the asynchronous version of this method.

#### Parameters

self | A MMModemCdma. |
carrier | Name of the carrier. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the activation was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_cdma_activate_manual ()

    void
    mm_modem_cdma_activate_manual (MMModemCdma *self,
                                   MMCdmaManualActivationProperties *properties,
                                   GCancellable *cancellable,
                                   GAsyncReadyCallback callback,
                                   gpointer user_data);

Asynchronously requests to provision the modem with the given properties.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_cdma_activate_manual_finish()` to get the result of the operation.

See `mm_modem_cdma_activate_manual_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemCdma. |
properties | A MMCdmaManualActivationProperties. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_cdma_activate_manual_finish ()

    gboolean
    mm_modem_cdma_activate_manual_finish (MMModemCdma *self,
                                          GAsyncResult *res,
                                          GError **error);

Finishes an operation started with `mm_modem_cdma_activate_manual()`.

#### Parameters

self | A MMModemCdma. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_cdma_activate_manual()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the activation was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_cdma_activate_manual_sync ()

    gboolean
    mm_modem_cdma_activate_manual_sync (MMModemCdma *self,
                                        MMCdmaManualActivationProperties *properties,
                                        GCancellable *cancellable,
                                        GError **error);

Synchronously requests to provision the modem with the given properties.

The calling thread is blocked until a reply is received. See `mm_modem_cdma_activate_manual()` for the asynchronous version of this method.

#### Parameters

self | A MMModemCdma. |
properties | A MMCdmaManualActivationProperties. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the activation was successful, `FALSE` if `error` is set.

Since: 1.0

## Types and Values

### struct MMModemCdma

    struct MMModemCdma;

The MMModemCdma structure contains private data and should only be accessed using the provided API.

### MM_MODEM_CDMA_NID_UNKNOWN

    #define MM_MODEM_CDMA_NID_UNKNOWN 99999

Identifier for an unknown NID.

### MM_MODEM_CDMA_SID_UNKNOWN

    #define MM_MODEM_CDMA_SID_UNKNOWN 99999

Identifier for an unknown SID.