## vlan vlan — VLAN Settings |

## Properties

Table 82.

Key Name | Value Type | Default Value | Value Description
--- | --- | --- | ---
    egress-priority-map
    array of string
| For outgoing packets, a list of mappings from Linux SKB priorities to 802.1p priorities. The mapping is given in the format "from:to" where both "from" and "to" are unsigned integers, ie "7:3".
    flags
    NMVlanFlags (uint32)
| One or more flags which control the behavior and features of the VLAN interface. Flags include NM_VLAN_FLAG_REORDER_HEADERS (0x1) (reordering of output packet headers), NM_VLAN_FLAG_GVRP (0x2) (use of the GVRP protocol), and NM_VLAN_FLAG_LOOSE_BINDING (0x4) (loose binding of the interface to its master device's operating state). NM_VLAN_FLAG_MVRP (0x8) (use of the MVRP protocol). The default value of this property is NM_VLAN_FLAG_REORDER_HEADERS, but it used to be 0. To preserve backward compatibility, the default-value in the D-Bus API continues to be 0 and a missing property on D-Bus is still considered as 0.
    id
    uint32
    0
| The VLAN identifier that the interface created by this connection should be assigned. The valid range is from 0 to 4094, without the reserved id 4095.
    ingress-priority-map
    array of string
| For incoming packets, a list of mappings from 802.1p priorities to Linux SKB priorities. The mapping is given in the format "from:to" where both "from" and "to" are unsigned integers, ie "7:3".
    interface-name
    string
| Deprecated in favor of connection.interface-name, but can be used for backward-compatibility with older daemons, to set the vlan's interface name.
    parent
    string
| If given, specifies the parent interface name or parent connection UUID from which this VLAN interface should be created. If this property is not specified, the connection must contain an "802-3-ethernet" setting with a "mac-address" property.