## org.freedesktop.NetworkManager.Device.Vxlan org.freedesktop.NetworkManager.Device.Vxlan — VXLAN Device |

## Properties

    Parent      readable   o
    HwAddress   readable   s
    Id          readable   u
    Group       readable   s
    Local       readable   s
    Tos         readable   y
    Ttl         readable   y
    Learning    readable   b
    Ageing      readable   u
    Limit       readable   u
    DstPort     readable   q
    SrcPortMin  readable   q
    SrcPortMax  readable   q
    Proxy       readable   b
    Rsc         readable   b
    L2miss      readable   b
    L3miss      readable   b

## Description

## Property Details

### The "Parent" property

    Parent  readable   o

The object path of the parent device (if the VXLAN is not purely internal to this host).

### The "HwAddress" property

    HwAddress  readable   s

Hardware address of the device. n DEPRECATED. Use the "HwAddress" property in "org.freedesktop.NetworkManager.Device" instead which exists since version NetworkManager 1.24.0.

### The "Id" property

    Id  readable   u

The VXLAN Network Identifier (VNI).

### The "Group" property

    Group  readable   s

The IP (v4 or v6) multicast group used to communicate with other physical hosts on this VXLAN.

### The "Local" property

    Local  readable   s

The local IPv4 or IPv6 address to use when sending VXLAN packets to other physical hosts.

### The "Tos" property

    Tos  readable   y

The value to use in the IP ToS field for VXLAN packets sent to other physical hosts.

### The "Ttl" property

    Ttl  readable   y

The value to use in the IP TTL field for VXLAN packets sent to other physical hosts.

### The "Learning" property

    Learning  readable   b

True if the VXLAN dynamically learns remote IP addresses.

### The "Ageing" property

    Ageing  readable   u

The interval in seconds at which the kernel purges stale cached addresses.

### The "Limit" property

    Limit  readable   u

The maximum number of entries that can be added to the VXLAN's forwarding table.

### The "DstPort" property

    DstPort  readable   q

Destination port for outgoing VXLAN packets.

### The "SrcPortMin" property

    SrcPortMin  readable   q

The lowest source port number to use for outgoing VXLAN packets.

### The "SrcPortMax" property

    SrcPortMax  readable   q

The highest source port number to use for outgoing VXLAN packets.

### The "Proxy" property

    Proxy  readable   b

True if the VXLAN is implementing DOVE ARP proxying for remote clients.

### The "Rsc" property

    Rsc  readable   b

True if the VXLAN is implementing DOVE route short-circuiting of known remote IP addresses.

### The "L2miss" property

    L2miss  readable   b

True if the VXLAN will emit netlink notifications of L2 switch misses.

### The "L3miss" property

    L3miss  readable   b

True if the VXLAN will emit netlink notifications of L3 switch misses.