## NMSetting8021x NMSetting8021x — Describes 802.1x-authenticated connection properties |

## Functions

NMSetting * | nm_setting_802_1x_new ()
NMSetting8021xCKScheme | nm_setting_802_1x_check_cert_scheme ()
guint32 | nm_setting_802_1x_get_num_eap_methods ()
const char * | nm_setting_802_1x_get_eap_method ()
gboolean | nm_setting_802_1x_add_eap_method ()
void | nm_setting_802_1x_remove_eap_method ()
gboolean | nm_setting_802_1x_remove_eap_method_by_value ()
void | nm_setting_802_1x_clear_eap_methods ()
const char * | nm_setting_802_1x_get_identity ()
const char * | nm_setting_802_1x_get_anonymous_identity ()
const char * | nm_setting_802_1x_get_pac_file ()
gboolean | nm_setting_802_1x_get_system_ca_certs ()
const char * | nm_setting_802_1x_get_ca_path ()
const char * | nm_setting_802_1x_get_phase2_ca_path ()
NMSetting8021xCKScheme | nm_setting_802_1x_get_ca_cert_scheme ()
GBytes * | nm_setting_802_1x_get_ca_cert_blob ()
const char * | nm_setting_802_1x_get_ca_cert_path ()
const char * | nm_setting_802_1x_get_ca_cert_uri ()
gboolean | nm_setting_802_1x_set_ca_cert ()
const char * | nm_setting_802_1x_get_ca_cert_password ()
NMSettingSecretFlags | nm_setting_802_1x_get_ca_cert_password_flags ()
const char * | nm_setting_802_1x_get_subject_match ()
guint32 | nm_setting_802_1x_get_num_altsubject_matches ()
const char * | nm_setting_802_1x_get_altsubject_match ()
gboolean | nm_setting_802_1x_add_altsubject_match ()
void | nm_setting_802_1x_remove_altsubject_match ()
gboolean | nm_setting_802_1x_remove_altsubject_match_by_value ()
void | nm_setting_802_1x_clear_altsubject_matches ()
const char * | nm_setting_802_1x_get_domain_suffix_match ()
const char * | nm_setting_802_1x_get_domain_match ()
NMSetting8021xCKScheme | nm_setting_802_1x_get_client_cert_scheme ()
GBytes * | nm_setting_802_1x_get_client_cert_blob ()
const char * | nm_setting_802_1x_get_client_cert_path ()
const char * | nm_setting_802_1x_get_client_cert_uri ()
gboolean | nm_setting_802_1x_set_client_cert ()
const char * | nm_setting_802_1x_get_client_cert_password ()
NMSettingSecretFlags | nm_setting_802_1x_get_client_cert_password_flags ()
const char * | nm_setting_802_1x_get_phase1_peapver ()
const char * | nm_setting_802_1x_get_phase1_peaplabel ()
const char * | nm_setting_802_1x_get_phase1_fast_provisioning ()
const char * | nm_setting_802_1x_get_phase2_auth ()
const char * | nm_setting_802_1x_get_phase2_autheap ()
NMSetting8021xCKScheme | nm_setting_802_1x_get_phase2_ca_cert_scheme ()
GBytes * | nm_setting_802_1x_get_phase2_ca_cert_blob ()
const char * | nm_setting_802_1x_get_phase2_ca_cert_path ()
const char * | nm_setting_802_1x_get_phase2_ca_cert_uri ()
gboolean | nm_setting_802_1x_set_phase2_ca_cert ()
const char * | nm_setting_802_1x_get_phase2_ca_cert_password ()
NMSettingSecretFlags | nm_setting_802_1x_get_phase2_ca_cert_password_flags ()
const char * | nm_setting_802_1x_get_phase2_subject_match ()
guint32 | nm_setting_802_1x_get_num_phase2_altsubject_matches ()
const char * | nm_setting_802_1x_get_phase2_altsubject_match ()
gboolean | nm_setting_802_1x_add_phase2_altsubject_match ()
void | nm_setting_802_1x_remove_phase2_altsubject_match ()
gboolean | nm_setting_802_1x_remove_phase2_altsubject_match_by_value ()
void | nm_setting_802_1x_clear_phase2_altsubject_matches ()
const char * | nm_setting_802_1x_get_phase2_domain_suffix_match ()
const char * | nm_setting_802_1x_get_phase2_domain_match ()
NMSetting8021xCKScheme | nm_setting_802_1x_get_phase2_client_cert_scheme ()
GBytes * | nm_setting_802_1x_get_phase2_client_cert_blob ()
const char * | nm_setting_802_1x_get_phase2_client_cert_path ()
const char * | nm_setting_802_1x_get_phase2_client_cert_uri ()
gboolean | nm_setting_802_1x_set_phase2_client_cert ()
const char * | nm_setting_802_1x_get_phase2_client_cert_password ()
NMSettingSecretFlags | nm_setting_802_1x_get_phase2_client_cert_password_flags ()
const char * | nm_setting_802_1x_get_password ()
NMSettingSecretFlags | nm_setting_802_1x_get_password_flags ()
GBytes * | nm_setting_802_1x_get_password_raw ()
NMSettingSecretFlags | nm_setting_802_1x_get_password_raw_flags ()
const char * | nm_setting_802_1x_get_pin ()
NMSettingSecretFlags | nm_setting_802_1x_get_pin_flags ()
NMSetting8021xCKScheme | nm_setting_802_1x_get_private_key_scheme ()
GBytes * | nm_setting_802_1x_get_private_key_blob ()
const char * | nm_setting_802_1x_get_private_key_path ()
const char * | nm_setting_802_1x_get_private_key_uri ()
gboolean | nm_setting_802_1x_set_private_key ()
const char * | nm_setting_802_1x_get_private_key_password ()
NMSettingSecretFlags | nm_setting_802_1x_get_private_key_password_flags ()
NMSetting8021xCKFormat | nm_setting_802_1x_get_private_key_format ()
NMSetting8021xCKScheme | nm_setting_802_1x_get_phase2_private_key_scheme ()
GBytes * | nm_setting_802_1x_get_phase2_private_key_blob ()
const char * | nm_setting_802_1x_get_phase2_private_key_path ()
const char * | nm_setting_802_1x_get_phase2_private_key_uri ()
gboolean | nm_setting_802_1x_set_phase2_private_key ()
const char * | nm_setting_802_1x_get_phase2_private_key_password ()
NMSettingSecretFlags | nm_setting_802_1x_get_phase2_private_key_password_flags ()
NMSetting8021xCKFormat | nm_setting_802_1x_get_phase2_private_key_format ()
NMSetting8021xAuthFlags | nm_setting_802_1x_get_phase1_auth_flags ()
int | nm_setting_802_1x_get_auth_timeout ()
gboolean | nm_setting_802_1x_get_optional ()

## Types and Values

#define | NM_SETTING_802_1X_CERT_SCHEME_PREFIX_PATH
#define | NM_SETTING_802_1X_CERT_SCHEME_PREFIX_PKCS11
enum | NMSetting8021xCKFormat
enum | NMSetting8021xCKScheme
enum | NMSetting8021xAuthFlags
#define | NM_SETTING_802_1X_SETTING_NAME
#define | NM_SETTING_802_1X_EAP
#define | NM_SETTING_802_1X_IDENTITY
#define | NM_SETTING_802_1X_ANONYMOUS_IDENTITY
#define | NM_SETTING_802_1X_PAC_FILE
#define | NM_SETTING_802_1X_CA_CERT
#define | NM_SETTING_802_1X_CA_CERT_PASSWORD
#define | NM_SETTING_802_1X_CA_CERT_PASSWORD_FLAGS
#define | NM_SETTING_802_1X_CA_PATH
#define | NM_SETTING_802_1X_SUBJECT_MATCH
#define | NM_SETTING_802_1X_ALTSUBJECT_MATCHES
#define | NM_SETTING_802_1X_DOMAIN_SUFFIX_MATCH
#define | NM_SETTING_802_1X_DOMAIN_MATCH
#define | NM_SETTING_802_1X_CLIENT_CERT
#define | NM_SETTING_802_1X_CLIENT_CERT_PASSWORD
#define | NM_SETTING_802_1X_CLIENT_CERT_PASSWORD_FLAGS
#define | NM_SETTING_802_1X_PHASE1_PEAPVER
#define | NM_SETTING_802_1X_PHASE1_PEAPLABEL
#define | NM_SETTING_802_1X_PHASE1_FAST_PROVISIONING
#define | NM_SETTING_802_1X_PHASE1_AUTH_FLAGS
#define | NM_SETTING_802_1X_PHASE2_AUTH
#define | NM_SETTING_802_1X_PHASE2_AUTHEAP
#define | NM_SETTING_802_1X_PHASE2_CA_CERT
#define | NM_SETTING_802_1X_PHASE2_CA_CERT_PASSWORD
#define | NM_SETTING_802_1X_PHASE2_CA_CERT_PASSWORD_FLAGS
#define | NM_SETTING_802_1X_PHASE2_CA_PATH
#define | NM_SETTING_802_1X_PHASE2_SUBJECT_MATCH
#define | NM_SETTING_802_1X_PHASE2_ALTSUBJECT_MATCHES
#define | NM_SETTING_802_1X_PHASE2_DOMAIN_SUFFIX_MATCH
#define | NM_SETTING_802_1X_PHASE2_DOMAIN_MATCH
#define | NM_SETTING_802_1X_PHASE2_CLIENT_CERT
#define | NM_SETTING_802_1X_PHASE2_CLIENT_CERT_PASSWORD
#define | NM_SETTING_802_1X_PHASE2_CLIENT_CERT_PASSWORD_FLAGS
#define | NM_SETTING_802_1X_PASSWORD
#define | NM_SETTING_802_1X_PASSWORD_FLAGS
#define | NM_SETTING_802_1X_PASSWORD_RAW
#define | NM_SETTING_802_1X_PASSWORD_RAW_FLAGS
#define | NM_SETTING_802_1X_PRIVATE_KEY
#define | NM_SETTING_802_1X_PRIVATE_KEY_PASSWORD
#define | NM_SETTING_802_1X_PRIVATE_KEY_PASSWORD_FLAGS
#define | NM_SETTING_802_1X_PHASE2_PRIVATE_KEY
#define | NM_SETTING_802_1X_PHASE2_PRIVATE_KEY_PASSWORD
#define | NM_SETTING_802_1X_PHASE2_PRIVATE_KEY_PASSWORD_FLAGS
#define | NM_SETTING_802_1X_PIN
#define | NM_SETTING_802_1X_PIN_FLAGS
#define | NM_SETTING_802_1X_SYSTEM_CA_CERTS
#define | NM_SETTING_802_1X_AUTH_TIMEOUT
#define | NM_SETTING_802_1X_OPTIONAL

## Object Hierarchy

        GEnum
        ├── NMSetting8021xCKFormat
        ╰── NMSetting8021xCKScheme
        GFlags
        ╰── NMSetting8021xAuthFlags

## Description

The NMSetting8021x object is a NMSetting subclass that describes properties necessary for connection to 802.1x-authenticated networks, such as WPA and WPA2 Enterprise Wi-Fi networks and wired 802.1x networks. 802.1x connections typically use certificates and/or EAP authentication methods to securely verify, identify, and authenticate the client to the network itself, instead of simply relying on a widely shared static key.

It's a good idea to read up on wpa_supplicant configuration before using this setting extensively, since most of the options here correspond closely with the relevant wpa_supplicant configuration options.

Furthermore, to get a good idea of 802.1x, EAP, TLS, TTLS, etc and their applications to Wi-Fi and wired networks, you'll want to get copies of the following books.

802.11 Wireless Networks: The Definitive Guide, Second Edition Author: Matthew Gast ISBN: 978-0596100520

Cisco Wireless LAN Security Authors: Krishna Sankar, Sri Sundaralingam, Darrin Miller, and Andrew Balinsky ISBN: 978-1587051548

## Functions

### nm_setting_802_1x_new ()

    NMSetting *
    nm_setting_802_1x_new (void);

Creates a new NMSetting8021x object with default values.

#### Returns

the new empty NMSetting8021x object

### nm_setting_802_1x_check_cert_scheme ()

    NMSetting8021xCKScheme
    nm_setting_802_1x_check_cert_scheme (gconstpointer pdata,
                                         gsize length,
                                         GError **error);

Determines and verifies the blob type. When setting certificate properties of NMSetting8021x the blob must be not UNKNOWN (or NULL).

#### Parameters

pdata | the data pointer. | [allow-none]
length | the length of the data |
error | validation reason. | [allow-none][out]

#### Returns

the scheme of the blob or `NM_SETTING_802_1X_CK_SCHEME_UNKNOWN`. For NULL it also returns NM_SETTING_802_1X_CK_SCHEME_UNKNOWN.

Since: 1.2

### nm_setting_802_1x_get_num_eap_methods ()

    guint32
    nm_setting_802_1x_get_num_eap_methods (NMSetting8021x *setting);

Returns the number of eap methods allowed for use when connecting to the network. Generally only one EAP method is used. Use the functions `nm_setting_802_1x_get_eap_method()`, `nm_setting_802_1x_add_eap_method()`, and `nm_setting_802_1x_remove_eap_method()` for adding, removing, and retrieving allowed EAP methods.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the number of allowed EAP methods

### nm_setting_802_1x_get_eap_method ()

    const char *
    nm_setting_802_1x_get_eap_method (NMSetting8021x *setting,
                                      guint32 i);

Returns the name of the allowed EAP method at index `i` .

#### Parameters

setting | the NMSetting8021x |
i | the index of the EAP method name to return |

#### Returns

the name of the allowed EAP method at index `i`

### nm_setting_802_1x_add_eap_method ()

    gboolean
    nm_setting_802_1x_add_eap_method (NMSetting8021x *setting,
                                      const char *eap);

Adds an allowed EAP method. The setting is not valid until at least one EAP method has been added. See “eap” property for a list of allowed EAP methods.

#### Parameters

setting | the NMSetting8021x |
eap | the name of the EAP method to allow for this connection |

#### Returns

`TRUE` if the EAP method was successfully added, `FALSE` if it was not a valid method or if it was already allowed.

### nm_setting_802_1x_remove_eap_method ()

    void
    nm_setting_802_1x_remove_eap_method (NMSetting8021x *setting,
                                         guint32 i);

Removes the allowed EAP method at the specified index.

#### Parameters

setting | the NMSetting8021x |
i | the index of the EAP method to remove |

### nm_setting_802_1x_remove_eap_method_by_value ()

    gboolean
    nm_setting_802_1x_remove_eap_method_by_value
                                   (NMSetting8021x *setting,
                                    const char *eap);

Removes the allowed EAP method `method` .

#### Parameters

setting | the NMSetting8021x |
eap | the name of the EAP method to remove |

#### Returns

`TRUE` if the EAP method was founs and removed, `FALSE` if it was not.

### nm_setting_802_1x_clear_eap_methods ()

    void
    nm_setting_802_1x_clear_eap_methods (NMSetting8021x *setting);

Clears all allowed EAP methods.

#### Parameters

setting | the NMSetting8021x |

### nm_setting_802_1x_get_identity ()

    const char *
    nm_setting_802_1x_get_identity (NMSetting8021x *setting);

Returns the identifier used by some EAP methods (like TLS) to authenticate the user. Often this is a username or login name.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the user identifier

### nm_setting_802_1x_get_anonymous_identity ()

    const char *
    nm_setting_802_1x_get_anonymous_identity
                                   (NMSetting8021x *setting);

Returns the anonymous identifier used by some EAP methods (like TTLS) to authenticate the user in the outer unencrypted "phase 1" authentication. The inner "phase 2" authentication will use the “identity” in a secure form, if applicable for that EAP method.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the anonymous identifier

### nm_setting_802_1x_get_pac_file ()

    const char *
    nm_setting_802_1x_get_pac_file (NMSetting8021x *setting);

Returns the file containing PAC credentials used by EAP-FAST method.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the PAC file

### nm_setting_802_1x_get_system_ca_certs ()

    gboolean
    nm_setting_802_1x_get_system_ca_certs (NMSetting8021x *setting);

Sets the “system-ca-certs” property. The “ca-path” and “phase2-ca-path” properties are ignored if the “system-ca-certs” property is `TRUE`, in which case a system-wide CA certificate directory specified at compile time (using the --system-ca-path configure option) is used in place of these properties.

#### Parameters

setting | the NMSetting8021x |

#### Returns

`TRUE` if a system CA certificate path should be used, `FALSE` if not

### nm_setting_802_1x_get_ca_path ()

    const char *
    nm_setting_802_1x_get_ca_path (NMSetting8021x *setting);

Returns the path of the CA certificate directory if previously set. Systems will often have a directory that contains multiple individual CA certificates which the supplicant can then add to the verification chain. This may be used in addition to the “ca-cert” property to add more CA certificates for verifying the network to client.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the CA certificate directory path

### nm_setting_802_1x_get_phase2_ca_path ()

    const char *
    nm_setting_802_1x_get_phase2_ca_path (NMSetting8021x *setting);

Returns the path of the "phase 2" CA certificate directory if previously set. Systems will often have a directory that contains multiple individual CA certificates which the supplicant can then add to the verification chain. This may be used in addition to the “phase2-ca-cert” property to add more CA certificates for verifying the network to client.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the "phase 2" CA certificate directory path

### nm_setting_802_1x_get_ca_cert_scheme ()

    NMSetting8021xCKScheme
    nm_setting_802_1x_get_ca_cert_scheme (NMSetting8021x *setting);

Returns the scheme used to store the CA certificate. If the returned scheme is `NM_SETTING_802_1X_CK_SCHEME_BLOB`, use `nm_setting_802_1x_get_ca_cert_blob()`; if `NM_SETTING_802_1X_CK_SCHEME_PATH`, use `nm_setting_802_1x_get_ca_cert_path()`; if `NM_SETTING_802_1X_CK_SCHEME_PKCS11`, use `nm_setting_802_1x_get_ca_cert_uri()`.

#### Parameters

setting | the NMSetting8021x |

#### Returns

scheme used to store the CA certificate (blob or path)

### nm_setting_802_1x_get_ca_cert_blob ()

    GBytes *
    nm_setting_802_1x_get_ca_cert_blob (NMSetting8021x *setting);

Returns the CA certificate blob if the CA certificate is stored using the `NM_SETTING_802_1X_CK_SCHEME_BLOB` scheme. Not all EAP methods use a CA certificate (LEAP for example), and those that can take advantage of the CA certificate allow it to be unset. Note that lack of a CA certificate reduces security by allowing man-in-the-middle attacks, because the identity of the network cannot be confirmed by the client.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the CA certificate data.

[transfer none]

### nm_setting_802_1x_get_ca_cert_path ()

    const char *
    nm_setting_802_1x_get_ca_cert_path (NMSetting8021x *setting);

Returns the CA certificate path if the CA certificate is stored using the `NM_SETTING_802_1X_CK_SCHEME_PATH` scheme. Not all EAP methods use a CA certificate (LEAP for example), and those that can take advantage of the CA certificate allow it to be unset. Note that lack of a CA certificate reduces security by allowing man-in-the-middle attacks, because the identity of the network cannot be confirmed by the client.

#### Parameters

setting | the NMSetting8021x |

#### Returns

path to the CA certificate file

### nm_setting_802_1x_get_ca_cert_uri ()

    const char *
    nm_setting_802_1x_get_ca_cert_uri (NMSetting8021x *setting);

Returns the CA certificate URI analogously to `nm_setting_802_1x_get_ca_cert_blob()` and `nm_setting_802_1x_get_ca_cert_path()`.

Currently, it's limited to PKCS11 URIs ('pkcs11' scheme as defined by RFC 7512), but may be extended to other schemes in future (such as 'file' URIs for local files and 'data' URIs for inline certificate data).

#### Parameters

setting | the NMSetting8021x |

#### Returns

the URI string

Since: 1.6

### nm_setting_802_1x_set_ca_cert ()

    gboolean
    nm_setting_802_1x_set_ca_cert (NMSetting8021x *setting,
                                   const char *value,
                                   NMSetting8021xCKScheme scheme,
                                   NMSetting8021xCKFormat *out_format,
                                   GError **error);

Reads a certificate from disk and sets the “ca-cert” property with the raw certificate data if using the `NM_SETTING_802_1X_CK_SCHEME_BLOB` scheme, or with the path to the certificate file if using the `NM_SETTING_802_1X_CK_SCHEME_PATH` scheme.

#### Parameters

setting | the NMSetting8021x |
value | when `scheme` is set to either `NM_SETTING_802_1X_CK_SCHEME_PATH` or `NM_SETTING_802_1X_CK_SCHEME_BLOB`, pass the path of the CA certificate file (PEM or DER format). The path must be UTF-8 encoded; use `g_filename_to_utf8()` to convert if needed. Passing `NULL` with any `scheme` clears the CA certificate. |
scheme | desired storage scheme for the certificate |
out_format | on successful return, the type of the certificate added |
error | on unsuccessful return, an error |

#### Returns

`TRUE` if the operation succeeded, `FALSE` if it was unsuccessful

### nm_setting_802_1x_get_ca_cert_password ()

    const char *
    nm_setting_802_1x_get_ca_cert_password
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the password used to access the CA certificate stored in “ca-cert” property. Only makes sense if the certificate is stored on a PKCS#11 token that requires a login.

Since: 1.8

### nm_setting_802_1x_get_ca_cert_password_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_ca_cert_password_flags
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “ca-cert-password”

Since: 1.8

### nm_setting_802_1x_get_subject_match ()

    const char *
    nm_setting_802_1x_get_subject_match (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the “subject-match” property. This is the substring to be matched against the subject of the authentication server certificate, or `NULL` no subject verification is to be performed.

### nm_setting_802_1x_get_num_altsubject_matches ()

    guint32
    nm_setting_802_1x_get_num_altsubject_matches
                                   (NMSetting8021x *setting);

Returns the number of entries in the “altsubject-matches” property of this setting.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the number of altsubject-matches entries.

### nm_setting_802_1x_get_altsubject_match ()

    const char *
    nm_setting_802_1x_get_altsubject_match
                                   (NMSetting8021x *setting,
                                    guint32 i);

Returns the altSubjectName match at index `i` .

#### Parameters

setting | the NMSettingConnection |
i | the zero-based index of the array of altSubjectName matches |

#### Returns

the altSubjectName match at index `i`

### nm_setting_802_1x_add_altsubject_match ()

    gboolean
    nm_setting_802_1x_add_altsubject_match
                                   (NMSetting8021x *setting,
                                    const char *altsubject_match);

Adds an allowed alternate subject name match. Until at least one match is added, the altSubjectName of the remote authentication server is not verified.

#### Parameters

setting | the NMSetting8021x |
altsubject_match | the altSubjectName to allow for this connection |

#### Returns

`TRUE` if the alternative subject name match was successfully added, `FALSE` if it was already allowed.

### nm_setting_802_1x_remove_altsubject_match ()

    void
    nm_setting_802_1x_remove_altsubject_match
                                   (NMSetting8021x *setting,
                                    guint32 i);

Removes the allowed altSubjectName at the specified index.

#### Parameters

setting | the NMSetting8021x |
i | the index of the altSubjectName match to remove |

### nm_setting_802_1x_remove_altsubject_match_by_value ()

    gboolean
    nm_setting_802_1x_remove_altsubject_match_by_value
                                   (NMSetting8021x *setting,
                                    const char *altsubject_match);

Removes the allowed altSubjectName `altsubject_match` .

#### Parameters

setting | the NMSetting8021x |
altsubject_match | the altSubjectName to remove |

#### Returns

`TRUE` if the alternative subject name match was found and removed, `FALSE` if it was not.

### nm_setting_802_1x_clear_altsubject_matches ()

    void
    nm_setting_802_1x_clear_altsubject_matches
                                   (NMSetting8021x *setting);

Clears all altSubjectName matches.

#### Parameters

setting | the NMSetting8021x |

### nm_setting_802_1x_get_domain_suffix_match ()

    const char *
    nm_setting_802_1x_get_domain_suffix_match
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the “domain-suffix-match” property.

Since: 1.2

### nm_setting_802_1x_get_domain_match ()

    const char *
    nm_setting_802_1x_get_domain_match (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the “domain-match” property.

Since: 1.24

### nm_setting_802_1x_get_client_cert_scheme ()

    NMSetting8021xCKScheme
    nm_setting_802_1x_get_client_cert_scheme
                                   (NMSetting8021x *setting);

Returns the scheme used to store the client certificate. If the returned scheme is `NM_SETTING_802_1X_CK_SCHEME_BLOB`, use `nm_setting_802_1x_get_client_cert_blob()`; if `NM_SETTING_802_1X_CK_SCHEME_PATH`, use `nm_setting_802_1x_get_client_cert_path()`; if `NM_SETTING_802_1X_CK_SCHEME_PKCS11`, use `nm_setting_802_1x_get_client_cert_uri()`.

#### Parameters

setting | the NMSetting8021x |

#### Returns

scheme used to store the client certificate (blob or path)

### nm_setting_802_1x_get_client_cert_blob ()

    GBytes *
    nm_setting_802_1x_get_client_cert_blob
                                   (NMSetting8021x *setting);

Client certificates are used to identify the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the client certificate data.

[transfer none]

### nm_setting_802_1x_get_client_cert_path ()

    const char *
    nm_setting_802_1x_get_client_cert_path
                                   (NMSetting8021x *setting);

Client certificates are used to identify the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

#### Parameters

setting | the NMSetting8021x |

#### Returns

path to the client certificate file

### nm_setting_802_1x_get_client_cert_uri ()

    const char *
    nm_setting_802_1x_get_client_cert_uri (NMSetting8021x *setting);

Returns the client certificate URI analogously to `nm_setting_802_1x_get_client_cert_blob()` and `nm_setting_802_1x_get_client_cert_path()`.

Currently, it's limited to PKCS11 URIs ('pkcs11' scheme as defined by RFC 7512), but may be extended to other schemes in future (such as 'file' URIs for local files and 'data' URIs for inline certificate data).

#### Parameters

setting | the NMSetting8021x |

#### Returns

the URI string

Since: 1.6

### nm_setting_802_1x_set_client_cert ()

    gboolean
    nm_setting_802_1x_set_client_cert (NMSetting8021x *setting,
                                       const char *value,
                                       NMSetting8021xCKScheme scheme,
                                       NMSetting8021xCKFormat *out_format,
                                       GError **error);

Reads a certificate from disk and sets the “client-cert” property with the raw certificate data if using the `NM_SETTING_802_1X_CK_SCHEME_BLOB` scheme, or with the path to the certificate file if using the `NM_SETTING_802_1X_CK_SCHEME_PATH` scheme.

Client certificates are used to identify the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

#### Parameters

setting | the NMSetting8021x |
value | when `scheme` is set to either `NM_SETTING_802_1X_CK_SCHEME_PATH` or `NM_SETTING_802_1X_CK_SCHEME_BLOB`, pass the path of the client certificate file (PEM, DER, or PKCS#12 format). The path must be UTF-8 encoded; use `g_filename_to_utf8()` to convert if needed. Passing `NULL` with any `scheme` clears the client certificate. |
scheme | desired storage scheme for the certificate |
out_format | on successful return, the type of the certificate added |
error | on unsuccessful return, an error |

#### Returns

`TRUE` if the operation succeeded, `FALSE` if it was unsuccessful

### nm_setting_802_1x_get_client_cert_password ()

    const char *
    nm_setting_802_1x_get_client_cert_password
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the password used to access the client certificate stored in “client-cert” property. Only makes sense if the certificate is stored on a PKCS#11 token that requires a login.

Since: 1.8

### nm_setting_802_1x_get_client_cert_password_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_client_cert_password_flags
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “client-cert-password”

Since: 1.8

### nm_setting_802_1x_get_phase1_peapver ()

    const char *
    nm_setting_802_1x_get_phase1_peapver (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the "phase 1" PEAP version to be used when authenticating with EAP-PEAP as contained in the “phase1-peapver” property. Valid values are `NULL` (unset), "0" (PEAP version 0), and "1" (PEAP version 1).

### nm_setting_802_1x_get_phase1_peaplabel ()

    const char *
    nm_setting_802_1x_get_phase1_peaplabel
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

whether the "phase 1" PEAP label is new-style or old-style, to be used when authenticating with EAP-PEAP, as contained in the “phase1-peaplabel” property. Valid values are `NULL` (unset), "0" (use old-style label), and "1" (use new-style label). See the wpa_supplicant documentation for more details.

### nm_setting_802_1x_get_phase1_fast_provisioning ()

    const char *
    nm_setting_802_1x_get_phase1_fast_provisioning
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

whether "phase 1" PEAP fast provisioning should be used, as specified by the “phase1-fast-provisioning” property. See the wpa_supplicant documentation for more details.

### nm_setting_802_1x_get_phase2_auth ()

    const char *
    nm_setting_802_1x_get_phase2_auth (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the "phase 2" non-EAP (ex MD5) allowed authentication method as specified by the “phase2-auth” property.

### nm_setting_802_1x_get_phase2_autheap ()

    const char *
    nm_setting_802_1x_get_phase2_autheap (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the "phase 2" EAP-based (ex TLS) allowed authentication method as specified by the “phase2-autheap” property.

### nm_setting_802_1x_get_phase2_ca_cert_scheme ()

    NMSetting8021xCKScheme
    nm_setting_802_1x_get_phase2_ca_cert_scheme
                                   (NMSetting8021x *setting);

Returns the scheme used to store the "phase 2" CA certificate. If the returned scheme is `NM_SETTING_802_1X_CK_SCHEME_BLOB`, use `nm_setting_802_1x_get_ca_cert_blob()`; if `NM_SETTING_802_1X_CK_SCHEME_PATH`, use `nm_setting_802_1x_get_ca_cert_path()`; if `NM_SETTING_802_1X_CK_SCHEME_PKCS11`, use `nm_setting_802_1x_get_ca_cert_uri()`.

#### Parameters

setting | the NMSetting8021x |

#### Returns

scheme used to store the "phase 2" CA certificate (blob or path)

### nm_setting_802_1x_get_phase2_ca_cert_blob ()

    GBytes *
    nm_setting_802_1x_get_phase2_ca_cert_blob
                                   (NMSetting8021x *setting);

Returns the "phase 2" CA certificate blob if the CA certificate is stored using the `NM_SETTING_802_1X_CK_SCHEME_BLOB` scheme. Not all EAP methods use a CA certificate (LEAP for example), and those that can take advantage of the CA certificate allow it to be unset. Note that lack of a CA certificate reduces security by allowing man-in-the-middle attacks, because the identity of the network cannot be confirmed by the client.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the "phase 2" CA certificate data.

[transfer none]

### nm_setting_802_1x_get_phase2_ca_cert_path ()

    const char *
    nm_setting_802_1x_get_phase2_ca_cert_path
                                   (NMSetting8021x *setting);

Returns the "phase 2" CA certificate path if the CA certificate is stored using the `NM_SETTING_802_1X_CK_SCHEME_PATH` scheme. Not all EAP methods use a CA certificate (LEAP for example), and those that can take advantage of the CA certificate allow it to be unset. Note that lack of a CA certificate reduces security by allowing man-in-the-middle attacks, because the identity of the network cannot be confirmed by the client.

#### Parameters

setting | the NMSetting8021x |

#### Returns

path to the "phase 2" CA certificate file

### nm_setting_802_1x_get_phase2_ca_cert_uri ()

    const char *
    nm_setting_802_1x_get_phase2_ca_cert_uri
                                   (NMSetting8021x *setting);

Returns the "phase 2" CA certificate URI analogously to `nm_setting_802_1x_get_phase2_ca_cert_blob()` and `nm_setting_802_1x_get_phase2_ca_cert_path()`.

Currently, it's limited to PKCS11 URIs ('pkcs11' scheme as defined by RFC 7512), but may be extended to other schemes in future (such as 'file' URIs for local files and 'data' URIs for inline certificate data).

#### Parameters

setting | the NMSetting8021x |

#### Returns

the URI string

Since: 1.6

### nm_setting_802_1x_set_phase2_ca_cert ()

    gboolean
    nm_setting_802_1x_set_phase2_ca_cert (NMSetting8021x *setting,
                                          const char *value,
                                          NMSetting8021xCKScheme scheme,
                                          NMSetting8021xCKFormat *out_format,
                                          GError **error);

Reads a certificate from disk and sets the “phase2-ca-cert” property with the raw certificate data if using the `NM_SETTING_802_1X_CK_SCHEME_BLOB` scheme, or with the path to the certificate file if using the `NM_SETTING_802_1X_CK_SCHEME_PATH` scheme.

#### Parameters

setting | the NMSetting8021x |
value | when `scheme` is set to either `NM_SETTING_802_1X_CK_SCHEME_PATH` or `NM_SETTING_802_1X_CK_SCHEME_BLOB`, pass the path of the "phase2" CA certificate file (PEM or DER format). The path must be UTF-8 encoded; use `g_filename_to_utf8()` to convert if needed. Passing `NULL` with any `scheme` clears the "phase2" CA certificate. |
scheme | desired storage scheme for the certificate |
out_format | on successful return, the type of the certificate added |
error | on unsuccessful return, an error |

#### Returns

`TRUE` if the operation succeeded, `FALSE` if it was unsuccessful

### nm_setting_802_1x_get_phase2_ca_cert_password ()

    const char *
    nm_setting_802_1x_get_phase2_ca_cert_password
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the password used to access the "phase2" CA certificate stored in “phase2-ca-cert” property. Only makes sense if the certificate is stored on a PKCS#11 token that requires a login.

Since: 1.8

### nm_setting_802_1x_get_phase2_ca_cert_password_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_phase2_ca_cert_password_flags
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “phase2-private-key-password”

Since: 1.8

### nm_setting_802_1x_get_phase2_subject_match ()

    const char *
    nm_setting_802_1x_get_phase2_subject_match
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the “phase2-subject-match” property. This is the substring to be matched against the subject of the "phase 2" authentication server certificate, or `NULL` no subject verification is to be performed.

### nm_setting_802_1x_get_num_phase2_altsubject_matches ()

    guint32
    nm_setting_802_1x_get_num_phase2_altsubject_matches
                                   (NMSetting8021x *setting);

Returns the number of entries in the “phase2-altsubject-matches” property of this setting.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the number of phase2-altsubject-matches entries.

### nm_setting_802_1x_get_phase2_altsubject_match ()

    const char *
    nm_setting_802_1x_get_phase2_altsubject_match
                                   (NMSetting8021x *setting,
                                    guint32 i);

Returns the "phase 2" altSubjectName match at index `i` .

#### Parameters

setting | the NMSettingConnection |
i | the zero-based index of the array of "phase 2" altSubjectName matches |

#### Returns

the "phase 2" altSubjectName match at index `i`

### nm_setting_802_1x_add_phase2_altsubject_match ()

    gboolean
    nm_setting_802_1x_add_phase2_altsubject_match
                                   (NMSetting8021x *setting,
                                    const char *phase2_altsubject_match);

Adds an allowed alternate subject name match for "phase 2". Until at least one match is added, the altSubjectName of the "phase 2" remote authentication server is not verified.

#### Parameters

setting | the NMSetting8021x |
phase2_altsubject_match | the "phase 2" altSubjectName to allow for this connection |

#### Returns

`TRUE` if the "phase 2" alternative subject name match was successfully added, `FALSE` if it was already allowed.

### nm_setting_802_1x_remove_phase2_altsubject_match ()

    void
    nm_setting_802_1x_remove_phase2_altsubject_match
                                   (NMSetting8021x *setting,
                                    guint32 i);

Removes the allowed "phase 2" altSubjectName at the specified index.

#### Parameters

setting | the NMSetting8021x |
i | the index of the "phase 2" altSubjectName match to remove |

### nm_setting_802_1x_remove_phase2_altsubject_match_by_value ()

    gboolean
    nm_setting_802_1x_remove_phase2_altsubject_match_by_value
                                   (NMSetting8021x *setting,
                                    const char *phase2_altsubject_match);

Removes the allowed "phase 2" altSubjectName `phase2_altsubject_match` .

#### Parameters

setting | the NMSetting8021x |
phase2_altsubject_match | the "phase 2" altSubjectName to remove |

#### Returns

`TRUE` if the alternative subject name match for "phase 2" was found and removed, `FALSE` if it was not.

### nm_setting_802_1x_clear_phase2_altsubject_matches ()

    void
    nm_setting_802_1x_clear_phase2_altsubject_matches
                                   (NMSetting8021x *setting);

Clears all "phase 2" altSubjectName matches.

#### Parameters

setting | the NMSetting8021x |

### nm_setting_802_1x_get_phase2_domain_suffix_match ()

    const char *
    nm_setting_802_1x_get_phase2_domain_suffix_match
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the “phase2-domain-suffix-match” property.

Since: 1.2

### nm_setting_802_1x_get_phase2_domain_match ()

    const char *
    nm_setting_802_1x_get_phase2_domain_match
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the “phase2-domain-match” property.

Since: 1.24

### nm_setting_802_1x_get_phase2_client_cert_scheme ()

    NMSetting8021xCKScheme
    nm_setting_802_1x_get_phase2_client_cert_scheme
                                   (NMSetting8021x *setting);

Returns the scheme used to store the "phase 2" client certificate. If the returned scheme is `NM_SETTING_802_1X_CK_SCHEME_BLOB`, use `nm_setting_802_1x_get_client_cert_blob()`; if `NM_SETTING_802_1X_CK_SCHEME_PATH`, use `nm_setting_802_1x_get_client_cert_path()`; if `NM_SETTING_802_1X_CK_SCHEME_PKCS11`, use `nm_setting_802_1x_get_client_cert_uri()`.

#### Parameters

setting | the NMSetting8021x |

#### Returns

scheme used to store the "phase 2" client certificate (blob or path)

### nm_setting_802_1x_get_phase2_client_cert_blob ()

    GBytes *
    nm_setting_802_1x_get_phase2_client_cert_blob
                                   (NMSetting8021x *setting);

Client certificates are used to identify the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the "phase 2" client certificate data.

[transfer none]

### nm_setting_802_1x_get_phase2_client_cert_path ()

    const char *
    nm_setting_802_1x_get_phase2_client_cert_path
                                   (NMSetting8021x *setting);

Client certificates are used to identify the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

#### Parameters

setting | the NMSetting8021x |

#### Returns

path to the "phase 2" client certificate file

### nm_setting_802_1x_get_phase2_client_cert_uri ()

    const char *
    nm_setting_802_1x_get_phase2_client_cert_uri
                                   (NMSetting8021x *setting);

Returns the "phase 2" client certificate URI analogously to `nm_setting_802_1x_get_phase2_ca_cert_blob()` and `nm_setting_802_1x_get_phase2_ca_cert_path()`.

Currently, it's limited to PKCS11 URIs ('pkcs11' scheme as defined by RFC 7512), but may be extended to other schemes in future (such as 'file' URIs for local files and 'data' URIs for inline certificate data).

#### Parameters

setting | the NMSetting8021x |

#### Returns

the URI string

Since: 1.6

### nm_setting_802_1x_set_phase2_client_cert ()

    gboolean
    nm_setting_802_1x_set_phase2_client_cert
                                   (NMSetting8021x *setting,
                                    const char *value,
                                    NMSetting8021xCKScheme scheme,
                                    NMSetting8021xCKFormat *out_format,
                                    GError **error);

Reads a certificate from disk and sets the “phase2-client-cert” property with the raw certificate data if using the `NM_SETTING_802_1X_CK_SCHEME_BLOB` scheme, or with the path to the certificate file if using the `NM_SETTING_802_1X_CK_SCHEME_PATH` scheme.

Client certificates are used to identify the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

#### Parameters

setting | the NMSetting8021x |
value | when `scheme` is set to either `NM_SETTING_802_1X_CK_SCHEME_PATH` or `NM_SETTING_802_1X_CK_SCHEME_BLOB`, pass the path of the "phase2" client certificate file (PEM, DER, or PKCS#12 format). The path must be UTF-8 encoded; use `g_filename_to_utf8()` to convert if needed. Passing `NULL` with any `scheme` clears the "phase2" client certificate. |
scheme | desired storage scheme for the certificate |
out_format | on successful return, the type of the certificate added |
error | on unsuccessful return, an error |

#### Returns

`TRUE` if the operation succeeded, `FALSE` if it was unsuccessful

### nm_setting_802_1x_get_phase2_client_cert_password ()

    const char *
    nm_setting_802_1x_get_phase2_client_cert_password
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the password used to access the "phase2" client certificate stored in “phase2-client-cert” property. Only makes sense if the certificate is stored on a PKCS#11 token that requires a login.

Since: 1.8

### nm_setting_802_1x_get_phase2_client_cert_password_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_phase2_client_cert_password_flags
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “phase2-client-cert-password”

Since: 1.8

### nm_setting_802_1x_get_password ()

    const char *
    nm_setting_802_1x_get_password (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the password used by the authentication method, if any, as specified by the “password” property

### nm_setting_802_1x_get_password_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_password_flags (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “password”

### nm_setting_802_1x_get_password_raw ()

    GBytes *
    nm_setting_802_1x_get_password_raw (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the password used by the authentication method as a UTF-8-encoded array of bytes, as specified by the “password-raw” property.

[transfer none]

### nm_setting_802_1x_get_password_raw_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_password_raw_flags
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “password-raw”

### nm_setting_802_1x_get_pin ()

    const char *
    nm_setting_802_1x_get_pin (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the PIN used by the authentication method, if any, as specified by the “pin” property

### nm_setting_802_1x_get_pin_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_pin_flags (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “pin”

### nm_setting_802_1x_get_private_key_scheme ()

    NMSetting8021xCKScheme
    nm_setting_802_1x_get_private_key_scheme
                                   (NMSetting8021x *setting);

Returns the scheme used to store the private key. If the returned scheme is `NM_SETTING_802_1X_CK_SCHEME_BLOB`, use `nm_setting_802_1x_get_client_cert_blob()`; if `NM_SETTING_802_1X_CK_SCHEME_PATH`, use `nm_setting_802_1x_get_client_cert_path()`; if `NM_SETTING_802_1X_CK_SCHEME_PKCS11`, use `nm_setting_802_1x_get_client_cert_uri()`.

#### Parameters

setting | the NMSetting8021x |

#### Returns

scheme used to store the private key (blob or path)

### nm_setting_802_1x_get_private_key_blob ()

    GBytes *
    nm_setting_802_1x_get_private_key_blob
                                   (NMSetting8021x *setting);

Private keys are used to authenticate the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

WARNING: the private key property is not a "secret" property, and thus unencrypted private key data may be readable by unprivileged users. Private keys should always be encrypted with a private key password.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the private key data.

[transfer none]

### nm_setting_802_1x_get_private_key_path ()

    const char *
    nm_setting_802_1x_get_private_key_path
                                   (NMSetting8021x *setting);

Private keys are used to authenticate the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

#### Parameters

setting | the NMSetting8021x |

#### Returns

path to the private key file

### nm_setting_802_1x_get_private_key_uri ()

    const char *
    nm_setting_802_1x_get_private_key_uri (NMSetting8021x *setting);

Returns the private key URI analogously to `nm_setting_802_1x_get_private_key_blob()` and `nm_setting_802_1x_get_private_key_path()`.

Currently, it's limited to PKCS11 URIs ('pkcs11' scheme as defined by RFC 7512), but may be extended to other schemes in future (such as 'file' URIs for local files and 'data' URIs for inline certificate data).

#### Parameters

setting | the NMSetting8021x |

#### Returns

the URI string

Since: 1.6

### nm_setting_802_1x_set_private_key ()

    gboolean
    nm_setting_802_1x_set_private_key (NMSetting8021x *setting,
                                       const char *value,
                                       const char *password,
                                       NMSetting8021xCKScheme scheme,
                                       NMSetting8021xCKFormat *out_format,
                                       GError **error);

Private keys are used to authenticate the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

This function reads a private key from disk and sets the “private-key” property with the private key file data if using the `NM_SETTING_802_1X_CK_SCHEME_BLOB` scheme, or with the path to the private key file if using the `NM_SETTING_802_1X_CK_SCHEME_PATH` scheme.

If `password` is given, this function attempts to decrypt the private key to verify that `password` is correct, and if it is, updates the “private-key-password” property with the given `password` . If the decryption is unsuccessful, `FALSE` is returned, `error` is set, and no internal data is changed. If no `password` is given, the private key is assumed to be valid, no decryption is performed, and the password may be set at a later time.

WARNING: the private key property is not a "secret" property, and thus unencrypted private key data using the BLOB scheme may be readable by unprivileged users. Private keys should always be encrypted with a private key password to prevent unauthorized access to unencrypted private key data.

#### Parameters

setting | the NMSetting8021x |
value | when `scheme` is set to either `NM_SETTING_802_1X_CK_SCHEME_PATH` or `NM_SETTING_802_1X_CK_SCHEME_BLOB`, pass the path of the private key file (PEM, DER, or PKCS#12 format). The path must be UTF-8 encoded; use `g_filename_to_utf8()` to convert if needed. Passing `NULL` with any `scheme` clears the private key. |
password | password used to decrypt the private key, or `NULL` if the password is unknown. If the password is given but fails to decrypt the private key, an error is returned. |
scheme | desired storage scheme for the private key |
out_format | on successful return, the type of the private key added |
error | on unsuccessful return, an error |

#### Returns

`TRUE` if the operation succeeded, `FALSE` if it was unsuccessful

### nm_setting_802_1x_get_private_key_password ()

    const char *
    nm_setting_802_1x_get_private_key_password
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the private key password used to decrypt the private key if previously set with `nm_setting_802_1x_set_private_key()`, or the “private-key-password” property.

### nm_setting_802_1x_get_private_key_password_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_private_key_password_flags
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “private-key-password”

### nm_setting_802_1x_get_private_key_format ()

    NMSetting8021xCKFormat
    nm_setting_802_1x_get_private_key_format
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the data format of the private key data stored in the “private-key” property

### nm_setting_802_1x_get_phase2_private_key_scheme ()

    NMSetting8021xCKScheme
    nm_setting_802_1x_get_phase2_private_key_scheme
                                   (NMSetting8021x *setting);

Returns the scheme used to store the "phase 2" private key. If the returned scheme is `NM_SETTING_802_1X_CK_SCHEME_BLOB`, use `nm_setting_802_1x_get_client_cert_blob()`; if `NM_SETTING_802_1X_CK_SCHEME_PATH`, use `nm_setting_802_1x_get_client_cert_path()`; if `NM_SETTING_802_1X_CK_SCHEME_PKCS11`, use `nm_setting_802_1x_get_client_cert_uri()`.

#### Parameters

setting | the NMSetting8021x |

#### Returns

scheme used to store the "phase 2" private key (blob or path)

### nm_setting_802_1x_get_phase2_private_key_blob ()

    GBytes *
    nm_setting_802_1x_get_phase2_private_key_blob
                                   (NMSetting8021x *setting);

Private keys are used to authenticate the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

WARNING: the phase2 private key property is not a "secret" property, and thus unencrypted private key data may be readable by unprivileged users. Private keys should always be encrypted with a private key password.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the "phase 2" private key data.

[transfer none]

### nm_setting_802_1x_get_phase2_private_key_path ()

    const char *
    nm_setting_802_1x_get_phase2_private_key_path
                                   (NMSetting8021x *setting);

Private keys are used to authenticate the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

#### Parameters

setting | the NMSetting8021x |

#### Returns

path to the "phase 2" private key file

### nm_setting_802_1x_get_phase2_private_key_uri ()

    const char *
    nm_setting_802_1x_get_phase2_private_key_uri
                                   (NMSetting8021x *setting);

Returns the "phase 2" private key URI analogously to `nm_setting_802_1x_get_phase2_private_key_blob()` and `nm_setting_802_1x_get_phase2_private_key_path()`.

Currently, it's limited to PKCS11 URIs ('pkcs11' scheme as defined by RFC 7512), but may be extended to other schemes in future (such as 'file' URIs for local files and 'data' URIs for inline certificate data).

#### Parameters

setting | the NMSetting8021x |

#### Returns

the URI string

Since: 1.6

### nm_setting_802_1x_set_phase2_private_key ()

    gboolean
    nm_setting_802_1x_set_phase2_private_key
                                   (NMSetting8021x *setting,
                                    const char *value,
                                    const char *password,
                                    NMSetting8021xCKScheme scheme,
                                    NMSetting8021xCKFormat *out_format,
                                    GError **error);

Private keys are used to authenticate the connecting client to the network when EAP-TLS is used as either the "phase 1" or "phase 2" 802.1x authentication method.

This function reads a private key from disk and sets the “phase2-private-key” property with the private key file data if using the `NM_SETTING_802_1X_CK_SCHEME_BLOB` scheme, or with the path to the private key file if using the `NM_SETTING_802_1X_CK_SCHEME_PATH` scheme.

If `password` is given, this function attempts to decrypt the private key to verify that `password` is correct, and if it is, updates the “phase2-private-key-password” property with the given `password` . If the decryption is unsuccessful, `FALSE` is returned, `error` is set, and no internal data is changed. If no `password` is given, the private key is assumed to be valid, no decryption is performed, and the password may be set at a later time.

WARNING: the "phase2" private key property is not a "secret" property, and thus unencrypted private key data using the BLOB scheme may be readable by unprivileged users. Private keys should always be encrypted with a private key password to prevent unauthorized access to unencrypted private key data.

#### Parameters

setting | the NMSetting8021x |
value | when `scheme` is set to either `NM_SETTING_802_1X_CK_SCHEME_PATH` or `NM_SETTING_802_1X_CK_SCHEME_BLOB`, pass the path of the "phase2" private key file (PEM, DER, or PKCS#12 format). The path must be UTF-8 encoded; use `g_filename_to_utf8()` to convert if needed. Passing `NULL` with any `scheme` clears the private key. |
password | password used to decrypt the private key, or `NULL` if the password is unknown. If the password is given but fails to decrypt the private key, an error is returned. |
scheme | desired storage scheme for the private key |
out_format | on successful return, the type of the private key added |
error | on unsuccessful return, an error |

#### Returns

`TRUE` if the operation succeeded, `FALSE` if it was unsuccessful

### nm_setting_802_1x_get_phase2_private_key_password ()

    const char *
    nm_setting_802_1x_get_phase2_private_key_password
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the private key password used to decrypt the private key if previously set with `nm_setting_802_1x_set_phase2_private_key()` or the “phase2-private-key-password” property.

### nm_setting_802_1x_get_phase2_private_key_password_flags ()

    NMSettingSecretFlags
    nm_setting_802_1x_get_phase2_private_key_password_flags
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the NMSettingSecretFlags pertaining to the “phase2-private-key-password”

### nm_setting_802_1x_get_phase2_private_key_format ()

    NMSetting8021xCKFormat
    nm_setting_802_1x_get_phase2_private_key_format
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the data format of the "phase 2" private key data stored in the “phase2-private-key” property

### nm_setting_802_1x_get_phase1_auth_flags ()

    NMSetting8021xAuthFlags
    nm_setting_802_1x_get_phase1_auth_flags
                                   (NMSetting8021x *setting);

#### Parameters

setting | the NMSetting8021x |

#### Returns

the authentication flags for "phase 1".

Since: 1.8

### nm_setting_802_1x_get_auth_timeout ()

    int
    nm_setting_802_1x_get_auth_timeout (NMSetting8021x *setting);

Returns the value contained in the “auth-timeout” property.

#### Parameters

setting | the NMSetting8021x |

#### Returns

the configured authentication timeout in seconds. Zero means the global default value.

Since: 1.8

### nm_setting_802_1x_get_optional ()

    gboolean
    nm_setting_802_1x_get_optional (NMSetting8021x *setting);

Returns the value contained in the “optional” property.

#### Parameters

setting | the NMSetting8021x |

#### Returns

`TRUE` if the activation should proceed even when the 802.1X authentication fails; `FALSE` otherwise

Since: 1.22

## Types and Values

### NM_SETTING_802_1X_CERT_SCHEME_PREFIX_PATH

    #define NM_SETTING_802_1X_CERT_SCHEME_PREFIX_PATH   "file://"

### NM_SETTING_802_1X_CERT_SCHEME_PREFIX_PKCS11

    #define NM_SETTING_802_1X_CERT_SCHEME_PREFIX_PKCS11 "pkcs11:"

### enum NMSetting8021xCKFormat

NMSetting8021xCKFormat values indicate the general type of a certificate or private key

#### Members

NM_SETTING_802_1X_CK_FORMAT_UNKNOWN | unknown file format |
NM_SETTING_802_1X_CK_FORMAT_X509 | file contains an X.509 format certificate |
NM_SETTING_802_1X_CK_FORMAT_RAW_KEY | file contains an old-style OpenSSL PEM or DER private key |
NM_SETTING_802_1X_CK_FORMAT_PKCS12 | file contains a PKCS#12 certificate and private key |

### enum NMSetting8021xCKScheme

NMSetting8021xCKScheme values indicate how a certificate or private key is stored in the setting properties, either as a blob of the item's data, or as a path to a certificate or private key file on the filesystem

#### Members

NM_SETTING_802_1X_CK_SCHEME_UNKNOWN | unknown certificate or private key scheme |
NM_SETTING_802_1X_CK_SCHEME_BLOB | certificate or key is stored as the raw item data |
NM_SETTING_802_1X_CK_SCHEME_PATH | certificate or key is stored as a path to a file containing the certificate or key data |
NM_SETTING_802_1X_CK_SCHEME_PKCS11 | certificate or key is stored as a URI of an object on a PKCS11 token |

### enum NMSetting8021xAuthFlags

NMSetting8021xAuthFlags values indicate which authentication settings should be used.

Before 1.22, this was wrongly marked as a enum and not as a flags type.

#### Members

NM_SETTING_802_1X_AUTH_FLAGS_NONE | No flags |
NM_SETTING_802_1X_AUTH_FLAGS_TLS_1_0_DISABLE | Disable TLSv1.0 |
NM_SETTING_802_1X_AUTH_FLAGS_TLS_1_1_DISABLE | Disable TLSv1.1 |
NM_SETTING_802_1X_AUTH_FLAGS_TLS_1_2_DISABLE | Disable TLSv1.2 |
NM_SETTING_802_1X_AUTH_FLAGS_ALL | All supported flags |

Since: 1.8

### NM_SETTING_802_1X_SETTING_NAME

    #define NM_SETTING_802_1X_SETTING_NAME "802-1x"

### NM_SETTING_802_1X_EAP

    #define NM_SETTING_802_1X_EAP                               "eap"

### NM_SETTING_802_1X_IDENTITY

    #define NM_SETTING_802_1X_IDENTITY                          "identity"

### NM_SETTING_802_1X_ANONYMOUS_IDENTITY

    #define NM_SETTING_802_1X_ANONYMOUS_IDENTITY                "anonymous-identity"

### NM_SETTING_802_1X_PAC_FILE

    #define NM_SETTING_802_1X_PAC_FILE                          "pac-file"

### NM_SETTING_802_1X_CA_CERT

    #define NM_SETTING_802_1X_CA_CERT                           "ca-cert"

### NM_SETTING_802_1X_CA_CERT_PASSWORD

    #define NM_SETTING_802_1X_CA_CERT_PASSWORD                  "ca-cert-password"

### NM_SETTING_802_1X_CA_CERT_PASSWORD_FLAGS

    #define NM_SETTING_802_1X_CA_CERT_PASSWORD_FLAGS            "ca-cert-password-flags"

### NM_SETTING_802_1X_CA_PATH

    #define NM_SETTING_802_1X_CA_PATH                           "ca-path"

### NM_SETTING_802_1X_SUBJECT_MATCH

    #define NM_SETTING_802_1X_SUBJECT_MATCH                     "subject-match"

### NM_SETTING_802_1X_ALTSUBJECT_MATCHES

    #define NM_SETTING_802_1X_ALTSUBJECT_MATCHES                "altsubject-matches"

### NM_SETTING_802_1X_DOMAIN_SUFFIX_MATCH

    #define NM_SETTING_802_1X_DOMAIN_SUFFIX_MATCH               "domain-suffix-match"

### NM_SETTING_802_1X_DOMAIN_MATCH

    #define NM_SETTING_802_1X_DOMAIN_MATCH                      "domain-match"

### NM_SETTING_802_1X_CLIENT_CERT

    #define NM_SETTING_802_1X_CLIENT_CERT                       "client-cert"

### NM_SETTING_802_1X_CLIENT_CERT_PASSWORD

    #define NM_SETTING_802_1X_CLIENT_CERT_PASSWORD              "client-cert-password"

### NM_SETTING_802_1X_CLIENT_CERT_PASSWORD_FLAGS

    #define NM_SETTING_802_1X_CLIENT_CERT_PASSWORD_FLAGS        "client-cert-password-flags"

### NM_SETTING_802_1X_PHASE1_PEAPVER

    #define NM_SETTING_802_1X_PHASE1_PEAPVER                    "phase1-peapver"

### NM_SETTING_802_1X_PHASE1_PEAPLABEL

    #define NM_SETTING_802_1X_PHASE1_PEAPLABEL                  "phase1-peaplabel"

### NM_SETTING_802_1X_PHASE1_FAST_PROVISIONING

    #define NM_SETTING_802_1X_PHASE1_FAST_PROVISIONING          "phase1-fast-provisioning"

### NM_SETTING_802_1X_PHASE1_AUTH_FLAGS

    #define NM_SETTING_802_1X_PHASE1_AUTH_FLAGS                 "phase1-auth-flags"

### NM_SETTING_802_1X_PHASE2_AUTH

    #define NM_SETTING_802_1X_PHASE2_AUTH                       "phase2-auth"

### NM_SETTING_802_1X_PHASE2_AUTHEAP

    #define NM_SETTING_802_1X_PHASE2_AUTHEAP                    "phase2-autheap"

### NM_SETTING_802_1X_PHASE2_CA_CERT

    #define NM_SETTING_802_1X_PHASE2_CA_CERT                    "phase2-ca-cert"

### NM_SETTING_802_1X_PHASE2_CA_CERT_PASSWORD

    #define NM_SETTING_802_1X_PHASE2_CA_CERT_PASSWORD           "phase2-ca-cert-password"

### NM_SETTING_802_1X_PHASE2_CA_CERT_PASSWORD_FLAGS

    #define NM_SETTING_802_1X_PHASE2_CA_CERT_PASSWORD_FLAGS     "phase2-ca-cert-password-flags"

### NM_SETTING_802_1X_PHASE2_CA_PATH

    #define NM_SETTING_802_1X_PHASE2_CA_PATH                    "phase2-ca-path"

### NM_SETTING_802_1X_PHASE2_SUBJECT_MATCH

    #define NM_SETTING_802_1X_PHASE2_SUBJECT_MATCH              "phase2-subject-match"

### NM_SETTING_802_1X_PHASE2_ALTSUBJECT_MATCHES

    #define NM_SETTING_802_1X_PHASE2_ALTSUBJECT_MATCHES         "phase2-altsubject-matches"

### NM_SETTING_802_1X_PHASE2_DOMAIN_SUFFIX_MATCH

    #define NM_SETTING_802_1X_PHASE2_DOMAIN_SUFFIX_MATCH        "phase2-domain-suffix-match"

### NM_SETTING_802_1X_PHASE2_DOMAIN_MATCH

    #define NM_SETTING_802_1X_PHASE2_DOMAIN_MATCH               "phase2-domain-match"

### NM_SETTING_802_1X_PHASE2_CLIENT_CERT

    #define NM_SETTING_802_1X_PHASE2_CLIENT_CERT                "phase2-client-cert"

### NM_SETTING_802_1X_PHASE2_CLIENT_CERT_PASSWORD

    #define NM_SETTING_802_1X_PHASE2_CLIENT_CERT_PASSWORD       "phase2-client-cert-password"

### NM_SETTING_802_1X_PHASE2_CLIENT_CERT_PASSWORD_FLAGS

    #define NM_SETTING_802_1X_PHASE2_CLIENT_CERT_PASSWORD_FLAGS "phase2-client-cert-password-flags"

### NM_SETTING_802_1X_PASSWORD

    #define NM_SETTING_802_1X_PASSWORD                          "password"

### NM_SETTING_802_1X_PASSWORD_FLAGS

    #define NM_SETTING_802_1X_PASSWORD_FLAGS                    "password-flags"

### NM_SETTING_802_1X_PASSWORD_RAW

    #define NM_SETTING_802_1X_PASSWORD_RAW                      "password-raw"

### NM_SETTING_802_1X_PASSWORD_RAW_FLAGS

    #define NM_SETTING_802_1X_PASSWORD_RAW_FLAGS                "password-raw-flags"

### NM_SETTING_802_1X_PRIVATE_KEY

    #define NM_SETTING_802_1X_PRIVATE_KEY                       "private-key"

### NM_SETTING_802_1X_PRIVATE_KEY_PASSWORD

    #define NM_SETTING_802_1X_PRIVATE_KEY_PASSWORD              "private-key-password"

### NM_SETTING_802_1X_PRIVATE_KEY_PASSWORD_FLAGS

    #define NM_SETTING_802_1X_PRIVATE_KEY_PASSWORD_FLAGS        "private-key-password-flags"

### NM_SETTING_802_1X_PHASE2_PRIVATE_KEY

    #define NM_SETTING_802_1X_PHASE2_PRIVATE_KEY                "phase2-private-key"

### NM_SETTING_802_1X_PHASE2_PRIVATE_KEY_PASSWORD

    #define NM_SETTING_802_1X_PHASE2_PRIVATE_KEY_PASSWORD       "phase2-private-key-password"

### NM_SETTING_802_1X_PHASE2_PRIVATE_KEY_PASSWORD_FLAGS

    #define NM_SETTING_802_1X_PHASE2_PRIVATE_KEY_PASSWORD_FLAGS "phase2-private-key-password-flags"

### NM_SETTING_802_1X_PIN

    #define NM_SETTING_802_1X_PIN                               "pin"

### NM_SETTING_802_1X_PIN_FLAGS

    #define NM_SETTING_802_1X_PIN_FLAGS                         "pin-flags"

### NM_SETTING_802_1X_SYSTEM_CA_CERTS

    #define NM_SETTING_802_1X_SYSTEM_CA_CERTS                   "system-ca-certs"

### NM_SETTING_802_1X_AUTH_TIMEOUT

    #define NM_SETTING_802_1X_AUTH_TIMEOUT                      "auth-timeout"

### NM_SETTING_802_1X_OPTIONAL

    #define NM_SETTING_802_1X_OPTIONAL                          "optional"