## connection connection — General Connection Profile Settings |

## Properties

Table 45.

Key Name | Value Type | Default Value | Value Description
--- | --- | --- | ---
    auth-retries
    int32
    -1
| The number of retries for the authentication. Zero means to try indefinitely; -1 means to use a global default. If the global default is not set, the authentication retries for 3 times before failing the connection. Currently, this only applies to 802-1x authentication.
    autoconnect
    boolean
    TRUE
| Whether or not the connection should be automatically connected by NetworkManager when the resources for the connection are available. TRUE to automatically activate the connection, FALSE to require manual intervention to activate the connection. Note that autoconnect is not implemented for VPN profiles. See "secondaries" as an alternative to automatically connect VPN profiles.
    autoconnect-priority
    int32
    0
| The autoconnect priority. If the connection is set to autoconnect, connections with higher priority will be preferred. Defaults to 0. The higher number means higher priority.
    autoconnect-retries
    int32
    -1
| The number of times a connection should be tried when autoactivating before giving up. Zero means forever, -1 means the global default (4 times if not overridden). Setting this to 1 means to try activation only once before blocking autoconnect. Note that after a timeout, NetworkManager will try to autoconnect again.
    autoconnect-slaves
    NMSettingConnectionAutoconnectSlaves (int32)
| Whether or not slaves of this connection should be automatically brought up when NetworkManager activates this connection. This only has a real effect for master connections. The properties "autoconnect", "autoconnect-priority" and "autoconnect-retries" are unrelated to this setting. The permitted values are: 0: leave slave connections untouched, 1: activate all the slave connections with this connection, -1: default. If -1 (default) is set, global connection.autoconnect-slaves is read to determine the real value. If it is default as well, this fallbacks to 0.
    gateway-ping-timeout
    uint32
    0
| If greater than zero, delay success of IP addressing until either the timeout is reached, or an IP gateway replies to a ping.
    id
    string
| A human readable unique identifier for the connection, like "Work Wi-Fi" or "T-Mobile 3G".
    interface-name
    string
| The name of the network interface this connection is bound to. If not set, then the connection can be attached to any interface of the appropriate type (subject to restrictions imposed by other settings). For software devices this specifies the name of the created device. For connection types where interface names cannot easily be made persistent (e.g. mobile broadband or USB Ethernet), this property should not be used. Setting this property restricts the interfaces a connection can be used with, and if interface names change or are reordered the connection may be applied to the wrong interface.
    lldp
    int32
    -1
| Whether LLDP is enabled for the connection.
    llmnr
    int32
    -1
| Whether Link-Local Multicast Name Resolution (LLMNR) is enabled for the connection. LLMNR is a protocol based on the Domain Name System (DNS) packet format that allows both IPv4 and IPv6 hosts to perform name resolution for hosts on the same local link. The permitted values are: "yes" (2) register hostname and resolving for the connection, "no" (0) disable LLMNR for the interface, "resolve" (1) do not register hostname but allow resolving of LLMNR host names If unspecified, "default" ultimately depends on the DNS plugin (which for systemd-resolved currently means "yes"). This feature requires a plugin which supports LLMNR. Otherwise, the setting has no effect. One such plugin is dns-systemd-resolved.
    master
    string
| Interface name of the master device or UUID of the master connection.
    mdns
    int32
    -1
| Whether mDNS is enabled for the connection. The permitted values are: "yes" (2) register hostname and resolving for the connection, "no" (0) disable mDNS for the interface, "resolve" (1) do not register hostname but allow resolving of mDNS host names and "default" (-1) to allow lookup of a global default in NetworkManager.conf. If unspecified, "default" ultimately depends on the DNS plugin (which for systemd-resolved currently means "no"). This feature requires a plugin which supports mDNS. Otherwise, the setting has no effect. One such plugin is dns-systemd-resolved.
    metered
    NMMetered (int32)
| Whether the connection is metered. When updating this property on a currently activated connection, the change takes effect immediately.
    mud-url
    string
| If configured, set to a Manufacturer Usage Description (MUD) URL that points to manufacturer-recommended network policies for IoT devices. It is transmitted as a DHCPv4 or DHCPv6 option. The value must be a valid URL starting with "https://". The special value "none" is allowed to indicate that no MUD URL is used. If the per-profile value is unspecified (the default), a global connection default gets consulted. If still unspecified, the ultimate default is "none".
    multi-connect
    int32
    0
| Specifies whether the profile can be active multiple times at a particular moment. The value is of type NMConnectionMultiConnect.
    permissions
    array of string
| An array of strings defining what access a given user has to this connection. If this is NULL or empty, all users are allowed to access this connection; otherwise users are allowed if and only if they are in this list. When this is not empty, the connection can be active only when one of the specified users is logged into an active session. Each entry is of the form "[type]:[id]:[reserved]"; for example, "user:dcbw:blah". At this time only the "user" [type] is allowed. Any other values are ignored and reserved for future use. [id] is the username that this permission refers to, which may not contain the ":" character. Any [reserved] information present must be ignored and is reserved for future use. All of [type], [id], and [reserved] must be valid UTF-8.
    read-only
    boolean
    FALSE
| FALSE if the connection can be modified using the provided settings service's D-Bus interface with the right privileges, or TRUE if the connection is read-only and cannot be modified.
    secondaries
    array of string
| List of connection UUIDs that should be activated when the base connection itself is activated. Currently, only VPN connections are supported.
    slave-type
    string
| Setting name of the device type of this slave's master connection (eg, "bond"), or NULL if this connection is not a slave.
    stable-id
    string
| This represents the identity of the connection used for various purposes. It allows to configure multiple profiles to share the identity. Also, the stable-id can contain placeholders that are substituted dynamically and deterministically depending on the context. The stable-id is used for generating IPv6 stable private addresses with ipv6.addr-gen-mode=stable-privacy. It is also used to seed the generated cloned MAC address for ethernet.cloned-mac-address=stable and wifi.cloned-mac-address=stable. It is also used as DHCP client identifier with ipv4.dhcp-client-id=stable and to derive the DHCP DUID with ipv6.dhcp-duid=stable-[llt,ll,uuid]. Note that depending on the context where it is used, other parameters are also seeded into the generation algorithm. For example, a per-host key is commonly also included, so that different systems end up generating different IDs. Or with ipv6.addr-gen-mode=stable-privacy, also the device's name is included, so that different interfaces yield different addresses. The per-host key is the identity of your machine and stored in /var/lib/NetworkManager/secret-key. The '$' character is treated special to perform dynamic substitutions at runtime. Currently, supported are "${CONNECTION}", "${DEVICE}", "${MAC}", "${BOOT}", "${RANDOM}". These effectively create unique IDs per-connection, per-device, per-boot, or every time. Note that "${DEVICE}" corresponds to the interface name of the device and "${MAC}" is the permanent MAC address of the device. Any unrecognized patterns following '$' are treated verbatim, however are reserved for future use. You are thus advised to avoid '$' or escape it as "$$". For example, set it to "${CONNECTION}-${BOOT}-${DEVICE}" to create a unique id for this connection that changes with every reboot and differs depending on the interface where the profile activates. If the value is unset, a global connection default is consulted. If the value is still unset, the default is similar to "${CONNECTION}" and uses a unique, fixed ID for the connection.
    timestamp
    uint64
    0
| The time, in seconds since the Unix Epoch, that the connection was last _successfully_ fully activated. NetworkManager updates the connection timestamp periodically when the connection is active to ensure that an active connection has the latest timestamp. The property is only meant for reading (changes to this property will not be preserved).
    type
    string
| Base type of the connection. For hardware-dependent connections, should contain the setting name of the hardware-type specific setting (ie, "802-3-ethernet" or "802-11-wireless" or "bluetooth", etc), and for non-hardware dependent connections like VPN or otherwise, should contain the setting name of that setting type (ie, "vpn" or "bridge", etc).
    uuid
    string
| A universally unique identifier for the connection, for example generated with libuuid. It should be assigned when the connection is created, and never changed as long as the connection still applies to the same network. For example, it should not be changed when the "id" property or NMSettingIP4Config changes, but might need to be re-created when the Wi-Fi SSID, mobile broadband network provider, or "type" property changes. The UUID must be in the format "2815492f-7e56-435e-b2e9-246bd7cdc664" (ie, contains only hexadecimal characters and "-").
    wait-device-timeout
    int32
    -1
| Timeout in milliseconds to wait for device at startup. During boot, devices may take a while to be detected by the driver. This property will cause to delay NetworkManager-wait-online.service and nm-online to give the device a chance to appear. This works by waiting for the given timeout until a compatible device for the profile is available and managed. The value 0 means no wait time. The default value is -1, which currently has the same meaning as no wait time.
    zone
    string
| The trust level of a the connection. Free form case-insensitive string (for example "Home", "Work", "Public"). NULL or unspecified zone means the connection will be placed in the default zone as defined by the firewall. When updating this property on a currently activated connection, the change takes effect immediately.