<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE refentry PUBLIC "-//OASIS//DTD DocBook XML V4.1.2//EN"
               "http://www.oasis-open.org/docbook/xml/4.1.2/docbookx.dtd" [
]>
<refentry id="gdbus-org.freedesktop.NetworkManager.AccessPoint">
  <refmeta>    <refentrytitle role="top_of_page" id="gdbus-interface-org-freedesktop-NetworkManager-AccessPoint.top_of_page">org.freedesktop.NetworkManager.AccessPoint</refentrytitle>
  <indexterm zone="gdbus-interface-org-freedesktop-NetworkManager-AccessPoint.top_of_page"><primary sortas=".AccessPoint">org.freedesktop.NetworkManager.AccessPoint</primary></indexterm>
  </refmeta>  <refnamediv>    <refname>org.freedesktop.NetworkManager.AccessPoint</refname>    <refpurpose>Wi-Fi Access Point</refpurpose>  </refnamediv>  <refsect1 role="properties">
    <title role="properties.title">Properties</title>
    <synopsis>
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Flags">Flags</link>       readable   u
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.WpaFlags">WpaFlags</link>    readable   u
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.RsnFlags">RsnFlags</link>    readable   u
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Ssid">Ssid</link>        readable   ay
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Frequency">Frequency</link>   readable   u
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.HwAddress">HwAddress</link>   readable   s
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Mode">Mode</link>        readable   u
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.MaxBitrate">MaxBitrate</link>  readable   u
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Strength">Strength</link>    readable   y
<link linkend="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.LastSeen">LastSeen</link>    readable   i
</synopsis>
  </refsect1>
<refsect1 role="desc" id="gdbus-interface-org-freedesktop-NetworkManager-AccessPoint">
  <title role="desc.title">Description</title>
  <para></para>
</refsect1>
<refsect1 role="details" id="gdbus-properties-org.freedesktop.NetworkManager.AccessPoint">
  <title role="details.title">Property Details</title>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Flags">
  <title>The "Flags" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Flags"><primary sortas=".AccessPoint:Flags">org.freedesktop.NetworkManager.AccessPoint:Flags</primary></indexterm>
<programlisting>
Flags  readable   u
</programlisting>
<para>        Flags describing the capabilities of the access point.
</para><para>        Returns: <link linkend="NM80211ApFlags">NM80211ApFlags</link>
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.WpaFlags">
  <title>The "WpaFlags" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.WpaFlags"><primary sortas=".AccessPoint:WpaFlags">org.freedesktop.NetworkManager.AccessPoint:WpaFlags</primary></indexterm>
<programlisting>
WpaFlags  readable   u
</programlisting>
<para>        Flags describing the access point's capabilities according to WPA (Wifi
        Protected Access).
</para><para>        Returns: <link linkend="NM80211ApSecurityFlags">NM80211ApSecurityFlags</link>
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.RsnFlags">
  <title>The "RsnFlags" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.RsnFlags"><primary sortas=".AccessPoint:RsnFlags">org.freedesktop.NetworkManager.AccessPoint:RsnFlags</primary></indexterm>
<programlisting>
RsnFlags  readable   u
</programlisting>
<para>        Flags describing the access point's capabilities according to the RSN
        (Robust Secure Network) protocol.
</para><para>        Returns: <link linkend="NM80211ApSecurityFlags">NM80211ApSecurityFlags</link>
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Ssid">
  <title>The "Ssid" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Ssid"><primary sortas=".AccessPoint:Ssid">org.freedesktop.NetworkManager.AccessPoint:Ssid</primary></indexterm>
<programlisting>
Ssid  readable   ay
</programlisting>
<para>        The Service Set Identifier identifying the access point.
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Frequency">
  <title>The "Frequency" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Frequency"><primary sortas=".AccessPoint:Frequency">org.freedesktop.NetworkManager.AccessPoint:Frequency</primary></indexterm>
<programlisting>
Frequency  readable   u
</programlisting>
<para>        The radio channel frequency in use by the access point, in MHz.
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.HwAddress">
  <title>The "HwAddress" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.HwAddress"><primary sortas=".AccessPoint:HwAddress">org.freedesktop.NetworkManager.AccessPoint:HwAddress</primary></indexterm>
<programlisting>
HwAddress  readable   s
</programlisting>
<para>        The hardware address (BSSID) of the access point.
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Mode">
  <title>The "Mode" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Mode"><primary sortas=".AccessPoint:Mode">org.freedesktop.NetworkManager.AccessPoint:Mode</primary></indexterm>
<programlisting>
Mode  readable   u
</programlisting>
<para>        Describes the operating mode of the access point.
</para><para>        Returns: <link linkend="NM80211Mode">NM80211Mode</link>
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.MaxBitrate">
  <title>The "MaxBitrate" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.MaxBitrate"><primary sortas=".AccessPoint:MaxBitrate">org.freedesktop.NetworkManager.AccessPoint:MaxBitrate</primary></indexterm>
<programlisting>
MaxBitrate  readable   u
</programlisting>
<para>        The maximum bitrate this access point is capable of, in kilobits/second
        (Kb/s).
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Strength">
  <title>The "Strength" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.Strength"><primary sortas=".AccessPoint:Strength">org.freedesktop.NetworkManager.AccessPoint:Strength</primary></indexterm>
<programlisting>
Strength  readable   y
</programlisting>
<para>        The current signal quality of the access point, in percent.
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.LastSeen">
  <title>The "LastSeen" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-AccessPoint.LastSeen"><primary sortas=".AccessPoint:LastSeen">org.freedesktop.NetworkManager.AccessPoint:LastSeen</primary></indexterm>
<programlisting>
LastSeen  readable   i
</programlisting>
<para>        The timestamp (in CLOCK_BOOTTIME seconds) for the last time the access
        point was found in scan results. A value of -1 means the access point has
        never been found in scan results.
</para>
</refsect2>
</refsect1>
</refentry>

