## vxlan vxlan — VXLAN Settings |

## Properties

Table 85.

Key Name | Value Type | Default Value | Value Description
--- | --- | --- | ---
    ageing
    uint32
    300
| Specifies the lifetime in seconds of FDB entries learnt by the kernel.
    destination-port
    uint32
    8472
| Specifies the UDP destination port to communicate to the remote VXLAN tunnel endpoint.
    id
    uint32
    0
| Specifies the VXLAN Network Identifier (or VXLAN Segment Identifier) to use.
    l2-miss
    boolean
    FALSE
| Specifies whether netlink LL ADDR miss notifications are generated.
    l3-miss
    boolean
    FALSE
| Specifies whether netlink IP ADDR miss notifications are generated.
    learning
    boolean
    TRUE
| Specifies whether unknown source link layer addresses and IP addresses are entered into the VXLAN device forwarding database.
    limit
    uint32
    0
| Specifies the maximum number of FDB entries. A value of zero means that the kernel will store unlimited entries.
    local
    string
| If given, specifies the source IP address to use in outgoing packets.
    parent
    string
| If given, specifies the parent interface name or parent connection UUID.
    proxy
    boolean
    FALSE
| Specifies whether ARP proxy is turned on.
    remote
    string
| Specifies the unicast destination IP address to use in outgoing packets when the destination link layer address is not known in the VXLAN device forwarding database, or the multicast IP address to join.
    rsc
    boolean
    FALSE
| Specifies whether route short circuit is turned on.
    source-port-max
    uint32
    0
| Specifies the maximum UDP source port to communicate to the remote VXLAN tunnel endpoint.
    source-port-min
    uint32
    0
| Specifies the minimum UDP source port to communicate to the remote VXLAN tunnel endpoint.
    tos
    uint32
    0
| Specifies the TOS value to use in outgoing packets.
    ttl
    uint32
    0
| Specifies the time-to-live value to use in outgoing packets.