## pppoe pppoe — PPP-over-Ethernet Settings |

## Properties

Table 73.

Key Name | Value Type | Default Value | Value Description
--- | --- | --- | ---
    parent
    string
| If given, specifies the parent interface name on which this PPPoE connection should be created. If this property is not specified, the connection is activated on the interface specified in "interface-name" of NMSettingConnection.
    password
    string
| Password used to authenticate with the PPPoE service.
    password-flags
    NMSettingSecretFlags (uint32)
| Flags indicating how to handle the "password" property.
    service
    string
| If specified, instruct PPPoE to only initiate sessions with access concentrators that provide the specified service. For most providers, this should be left blank. It is only required if there are multiple access concentrators or a specific service is known to be required.
    username
    string
| Username used to authenticate with the PPPoE service.