## cdma cdma — CDMA-based Mobile Broadband Settings |

## Properties

Table 53.

Key Name | Value Type | Default Value | Value Description
--- | --- | --- | ---
    mtu
    uint32
    0
| If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple frames.
    number
    string
| The number to dial to establish the connection to the CDMA-based mobile broadband network, if any. If not specified, the default number (#777) is used when required.
    password
    string
| The password used to authenticate with the network, if required. Many providers do not require a password, or accept any password. But if a password is required, it is specified here.
    password-flags
    NMSettingSecretFlags (uint32)
| Flags indicating how to handle the "password" property.
    username
    string
| The username used to authenticate with the network, if required. Many providers do not require a username, or accept any username. But if a username is required, it is specified here.