## adsl adsl — ADSL Settings |

## Properties

Table 48.

Key Name | Value Type | Default Value | Value Description
--- | --- | --- | ---
    encapsulation
    string
| Encapsulation of ADSL connection. Can be "vcmux" or "llc".
    password
    string
| Password used to authenticate with the ADSL service.
    password-flags
    NMSettingSecretFlags (uint32)
| Flags indicating how to handle the "password" property.
    protocol
    string
| ADSL connection protocol. Can be "pppoa", "pppoe" or "ipoatm".
    username
    string
| Username used to authenticate with the ADSL service.
    vci
    uint32
    0
| VCI of ADSL connection
    vpi
    uint32
    0
| VPI of ADSL connection