Hardware Locality (hwloc) 2.2.0

nvml.h
1 /*
2 * Copyright © 2012-2016 Inria. All rights reserved.
3 * See COPYING in top-level directory.
4 */
5
13 #ifndef HWLOC_NVML_H
14 #define HWLOC_NVML_H
15
16 #include "hwloc.h"
17 #include "hwloc/autogen/config.h"
18 #include "hwloc/helper.h"
19 #ifdef HWLOC_LINUX_SYS
20 #include "hwloc/linux.h"
21 #endif
22
23 #include <nvml.h>
24
25
26 #ifdef __cplusplus
27 extern "C" {
28 #endif
29
30
55 static __hwloc_inline int
56 hwloc_nvml_get_device_cpuset(hwloc_topology_t topology __hwloc_attribute_unused,
57 nvmlDevice_t device, hwloc_cpuset_t set)
58 {
59 #ifdef HWLOC_LINUX_SYS
60 /* If we're on Linux, use the sysfs mechanism to get the local cpus */
61 #define HWLOC_NVML_DEVICE_SYSFS_PATH_MAX 128
62 char path[HWLOC_NVML_DEVICE_SYSFS_PATH_MAX];
63 nvmlReturn_t nvres;
64 nvmlPciInfo_t pci;
65
66 if (!hwloc_topology_is_thissystem(topology)) {
67 errno = EINVAL;
68 return -1;
69 }
70
71 nvres = nvmlDeviceGetPciInfo(device, &pci);
72 if (NVML_SUCCESS != nvres) {
73 errno = EINVAL;
74 return -1;
75 }
76
77 sprintf(path, "/sys/bus/pci/devices/%04x:%02x:%02x.0/local_cpus", pci.domain, pci.bus, pci.device);
78 if (hwloc_linux_read_path_as_cpumask(path, set) < 0
79 || hwloc_bitmap_iszero(set))
80 hwloc_bitmap_copy(set, hwloc_topology_get_complete_cpuset(topology));
81 #else
82 /* Non-Linux systems simply get a full cpuset */
83 hwloc_bitmap_copy(set, hwloc_topology_get_complete_cpuset(topology));
84 #endif
85 return 0;
86 }
87
101 static __hwloc_inline hwloc_obj_t
102 hwloc_nvml_get_device_osdev_by_index(hwloc_topology_t topology, unsigned idx)
103 {
104 hwloc_obj_t osdev = NULL;
105 while ((osdev = hwloc_get_next_osdev(topology, osdev)) != NULL) {
106 if (HWLOC_OBJ_OSDEV_GPU == osdev->attr->osdev.type
107 && osdev->name
108 && !strncmp("nvml", osdev->name, 4)
109 && atoi(osdev->name + 4) == (int) idx)
110 return osdev;
111 }
112 return NULL;
113 }
114
128 static __hwloc_inline hwloc_obj_t
129 hwloc_nvml_get_device_osdev(hwloc_topology_t topology, nvmlDevice_t device)
130 {
131 hwloc_obj_t osdev;
132 nvmlReturn_t nvres;
133 nvmlPciInfo_t pci;
134 char uuid[64];
135
136 if (!hwloc_topology_is_thissystem(topology)) {
137 errno = EINVAL;
138 return NULL;
139 }
140
141 nvres = nvmlDeviceGetPciInfo(device, &pci);
142 if (NVML_SUCCESS != nvres)
143 return NULL;
144
145 nvres = nvmlDeviceGetUUID(device, uuid, sizeof(uuid));
146 if (NVML_SUCCESS != nvres)
147 uuid[0] = '\0';
148
149 osdev = NULL;
150 while ((osdev = hwloc_get_next_osdev(topology, osdev)) != NULL) {
151 hwloc_obj_t pcidev = osdev->parent;
152 const char *info;
153
154 if (strncmp(osdev->name, "nvml", 4))
155 continue;
156
157 if (pcidev
158 && pcidev->type == HWLOC_OBJ_PCI_DEVICE
159 && pcidev->attr->pcidev.domain == pci.domain
160 && pcidev->attr->pcidev.bus == pci.bus
161 && pcidev->attr->pcidev.dev == pci.device
162 && pcidev->attr->pcidev.func == 0)
163 return osdev;
164
165 info = hwloc_obj_get_info_by_name(osdev, "NVIDIAUUID");
166 if (info && !strcmp(info, uuid))
167 return osdev;
168 }
169
170 return NULL;
171 }
172
176 #ifdef __cplusplus
177 } /* extern "C" */
178 #endif
179
180
181 #endif /* HWLOC_NVML_H */
hwloc_bitmap_copy
int hwloc_bitmap_copy(hwloc_bitmap_t dst, hwloc_const_bitmap_t src)
Copy the contents of bitmap src into the already allocated bitmap dst.
HWLOC_OBJ_PCI_DEVICE
@ HWLOC_OBJ_PCI_DEVICE
PCI device (filtered out by default). They are not added to the topology unless I/O discovery is enab...
Definition: hwloc.h:266
hwloc_obj_get_info_by_name
static const char * hwloc_obj_get_info_by_name(hwloc_obj_t obj, const char *name)
Search the given key name in object infos and return the corresponding value.
hwloc_obj_attr_u::hwloc_osdev_attr_s::type
hwloc_obj_osdev_type_t type
Definition: hwloc.h:652
hwloc_obj_attr_u::hwloc_pcidev_attr_s::domain
unsigned short domain
Definition: hwloc.h:621
hwloc_topology_get_complete_cpuset
hwloc_const_cpuset_t hwloc_topology_get_complete_cpuset(hwloc_topology_t topology)
Get complete CPU set.
hwloc_obj_attr_u::osdev
struct hwloc_obj_attr_u::hwloc_osdev_attr_s osdev
hwloc_obj::type
hwloc_obj_type_t type
Type of object.
Definition: hwloc.h:386
hwloc_obj::attr
union hwloc_obj_attr_u * attr
Object type-specific Attributes, may be NULL if no attribute value was found.
Definition: hwloc.h:403
hwloc_obj_attr_u::hwloc_pcidev_attr_s::func
unsigned char func
Definition: hwloc.h:625
hwloc_topology_t
struct hwloc_topology * hwloc_topology_t
Topology context.
Definition: hwloc.h:678
hwloc_obj
Structure of a topology object.
Definition: hwloc.h:384
hwloc_nvml_get_device_cpuset
static int hwloc_nvml_get_device_cpuset(hwloc_topology_t topology, nvmlDevice_t device, hwloc_cpuset_t set)
Get the CPU set of logical processors that are physically close to NVML device device.
Definition: nvml.h:56
hwloc_obj::name
char * name
Object-specific name if any. Mostly used for identifying OS devices and Misc objects where a name str...
Definition: hwloc.h:396
HWLOC_OBJ_OSDEV_GPU
@ HWLOC_OBJ_OSDEV_GPU
Operating system GPU device. For instance ":0.0" for a GL display, "card0" for a Linux DRM device.
Definition: hwloc.h:330
hwloc_obj_attr_u::hwloc_pcidev_attr_s::bus
unsigned char bus
Definition: hwloc.h:625
hwloc_get_next_osdev
static hwloc_obj_t hwloc_get_next_osdev(hwloc_topology_t topology, hwloc_obj_t prev)
Get the next OS device in the system.
Definition: helper.h:1151
hwloc_topology_is_thissystem
int hwloc_topology_is_thissystem(hwloc_topology_t restrict topology)
Does the topology context come from this system?
hwloc_obj::parent
struct hwloc_obj * parent
Parent, NULL if root (Machine object)
Definition: hwloc.h:434
hwloc_obj_attr_u::pcidev
struct hwloc_obj_attr_u::hwloc_pcidev_attr_s pcidev
hwloc_cpuset_t
hwloc_bitmap_t hwloc_cpuset_t
A CPU set is a bitmap whose bits are set according to CPU physical OS indexes.
Definition: hwloc.h:140
hwloc_nvml_get_device_osdev
static hwloc_obj_t hwloc_nvml_get_device_osdev(hwloc_topology_t topology, nvmlDevice_t device)
Get the hwloc OS device object corresponding to NVML device device.
Definition: nvml.h:129
hwloc_obj_attr_u::hwloc_pcidev_attr_s::dev
unsigned char dev
Definition: hwloc.h:625
hwloc_linux_read_path_as_cpumask
int hwloc_linux_read_path_as_cpumask(const char *path, hwloc_bitmap_t set)
Convert a linux kernel cpumask file path into a hwloc bitmap set.
hwloc_bitmap_iszero
int hwloc_bitmap_iszero(hwloc_const_bitmap_t bitmap)
Test whether bitmap bitmap is empty.
hwloc_nvml_get_device_osdev_by_index
static hwloc_obj_t hwloc_nvml_get_device_osdev_by_index(hwloc_topology_t topology, unsigned idx)
Get the hwloc OS device object corresponding to the NVML device whose index is idx.
Definition: nvml.h:102