Hardware Locality (hwloc) 1.11.9

Functions
Interoperability with OpenFabrics

## Functions
static int | hwloc_ibv_get_device_cpuset (hwloc_topology_t topology, struct ibv_device *ibdev, hwloc_cpuset_t set)
static hwloc_obj_t | hwloc_ibv_get_device_osdev_by_name (hwloc_topology_t topology, const char *ibname)
static hwloc_obj_t | hwloc_ibv_get_device_osdev (hwloc_topology_t topology, struct ibv_device *ibdev)

## Detailed Description

This interface offers ways to retrieve topology information about OpenFabrics devices (InfiniBand, Omni-Path, usNIC, etc).

## Function Documentation

## ◆ hwloc_ibv_get_device_cpuset()

static int hwloc_ibv_get_device_cpuset | ( | hwloc_topology_t | topology,
|  | struct ibv_device * | ibdev,
|  | hwloc_cpuset_t | set
| ) |  |
| inline static

Get the CPU set of logical processors that are physically close to device `ibdev`.

Return the CPU set describing the locality of the OpenFabrics device `ibdev` (InfiniBand, etc).

Topology `topology` and device `ibdev` must match the local machine. I/O devices detection is not needed in the topology.

The function only returns the locality of the device. If more information about the device is needed, OS objects should be used instead, see hwloc_ibv_get_device_osdev() and hwloc_ibv_get_device_osdev_by_name().

This function is currently only implemented in a meaningful way for Linux; other systems will simply get a full cpuset.

## ◆ hwloc_ibv_get_device_osdev()

static hwloc_obj_t hwloc_ibv_get_device_osdev | ( | hwloc_topology_t | topology,
|  | struct ibv_device * | ibdev
| ) |  |
| inline static

Get the hwloc OS device object corresponding to the OpenFabrics device `ibdev`.

Return the OS device object describing the OpenFabrics device `ibdev` (InfiniBand, etc). Returns NULL if there is none.

Topology `topology` and device `ibdev` must match the local machine. I/O devices detection must be enabled in the topology. If not, the locality of the object may still be found using hwloc_ibv_get_device_cpuset().

Note
  The corresponding PCI device object can be obtained by looking at the OS device parent object.

## ◆ hwloc_ibv_get_device_osdev_by_name()

static hwloc_obj_t hwloc_ibv_get_device_osdev_by_name | ( | hwloc_topology_t | topology,
|  | const char * | ibname
| ) |  |
| inline static

Get the hwloc OS device object corresponding to the OpenFabrics device named `ibname`.

Return the OS device object describing the OpenFabrics device (InfiniBand, Omni-Path, usNIC, etc) whose name is `ibname` (mlx5_0, hfi1_0, usnic_0, qib0, etc). Returns NULL if there is none. The name `ibname` is usually obtained from ibv_get_device_name().

The topology `topology` does not necessarily have to match the current machine. For instance the topology may be an XML import of a remote host. I/O devices detection must be enabled in the topology.

Note
  The corresponding PCI device object can be obtained by looking at the OS device parent object.