Hardware Locality (hwloc) 2.2.0

opencl.h
1 /*
2 * Copyright © 2012-2019 Inria. All rights reserved.
3 * Copyright © 2013, 2018 Université Bordeaux. All right reserved.
4 * See COPYING in top-level directory.
5 */
6
14 #ifndef HWLOC_OPENCL_H
15 #define HWLOC_OPENCL_H
16
17 #include "hwloc.h"
18 #include "hwloc/autogen/config.h"
19 #include "hwloc/helper.h"
20 #ifdef HWLOC_LINUX_SYS
21 #include "hwloc/linux.h"
22 #endif
23
24 #ifdef __APPLE__
25 #include <OpenCL/cl.h>
26 #else
27 #include <CL/cl.h>
28 #endif
29
30 #include <stdio.h>
31
32
33 #ifdef __cplusplus
34 extern "C" {
35 #endif
36
37
38 /* OpenCL extensions aren't always shipped with default headers, and
39 * they don't always reflect what the installed implementations support.
40 * Try everything and let the implementation return errors when non supported.
41 */
42 /* Copyright (c) 2008-2018 The Khronos Group Inc. */
43
44 /* needs "cl_amd_device_attribute_query" device extension, but not strictly required for clGetDeviceInfo() */
45 #define HWLOC_CL_DEVICE_TOPOLOGY_AMD 0x4037
46 typedef union {
47 struct { cl_uint type; cl_uint data[5]; } raw;
48 struct { cl_uint type; cl_char unused[17]; cl_char bus; cl_char device; cl_char function; } pcie;
49 } hwloc_cl_device_topology_amd;
50 #define HWLOC_CL_DEVICE_TOPOLOGY_TYPE_PCIE_AMD 1
51
52 /* needs "cl_nv_device_attribute_query" device extension, but not strictly required for clGetDeviceInfo() */
53 #define HWLOC_CL_DEVICE_PCI_BUS_ID_NV 0x4008
54 #define HWLOC_CL_DEVICE_PCI_SLOT_ID_NV 0x4009
55 #define HWLOC_CL_DEVICE_PCI_DOMAIN_ID_NV 0x400A
56
57
73 static __hwloc_inline int
74 hwloc_opencl_get_device_pci_busid(cl_device_id device,
75 unsigned *domain, unsigned *bus, unsigned *dev, unsigned *func)
76 {
77 hwloc_cl_device_topology_amd amdtopo;
78 cl_uint nvbus, nvslot, nvdomain;
79 cl_int clret;
80
81 clret = clGetDeviceInfo(device, HWLOC_CL_DEVICE_TOPOLOGY_AMD, sizeof(amdtopo), &amdtopo, NULL);
82 if (CL_SUCCESS == clret
83 && HWLOC_CL_DEVICE_TOPOLOGY_TYPE_PCIE_AMD == amdtopo.raw.type) {
84 *domain = 0; /* can't do anything better */
85 *bus = (unsigned) amdtopo.pcie.bus;
86 *dev = (unsigned) amdtopo.pcie.device;
87 *func = (unsigned) amdtopo.pcie.function;
88 return 0;
89 }
90
91 clret = clGetDeviceInfo(device, HWLOC_CL_DEVICE_PCI_BUS_ID_NV, sizeof(nvbus), &nvbus, NULL);
92 if (CL_SUCCESS == clret) {
93 clret = clGetDeviceInfo(device, HWLOC_CL_DEVICE_PCI_SLOT_ID_NV, sizeof(nvslot), &nvslot, NULL);
94 if (CL_SUCCESS == clret) {
95 clret = clGetDeviceInfo(device, HWLOC_CL_DEVICE_PCI_DOMAIN_ID_NV, sizeof(nvdomain), &nvdomain, NULL);
96 if (CL_SUCCESS == clret) { /* available since CUDA 10.2 */
97 *domain = nvdomain;
98 } else {
99 *domain = 0;
100 }
101 *bus = nvbus & 0xff;
102 /* non-documented but used in many other projects */
103 *dev = nvslot >> 3;
104 *func = nvslot & 0x7;
105 return 0;
106 }
107 }
108
109 return -1;
110 }
111
129 static __hwloc_inline int
130 hwloc_opencl_get_device_cpuset(hwloc_topology_t topology __hwloc_attribute_unused,
131 cl_device_id device __hwloc_attribute_unused,
132 hwloc_cpuset_t set)
133 {
134 #if (defined HWLOC_LINUX_SYS)
135 /* If we're on Linux, try AMD/NVIDIA extensions + the sysfs mechanism to get the local cpus */
136 #define HWLOC_OPENCL_DEVICE_SYSFS_PATH_MAX 128
137 char path[HWLOC_OPENCL_DEVICE_SYSFS_PATH_MAX];
138 unsigned pcidomain, pcibus, pcidev, pcifunc;
139
140 if (!hwloc_topology_is_thissystem(topology)) {
141 errno = EINVAL;
142 return -1;
143 }
144
145 if (hwloc_opencl_get_device_pci_busid(device, &pcidomain, &pcibus, &pcidev, &pcifunc) < 0) {
146 hwloc_bitmap_copy(set, hwloc_topology_get_complete_cpuset(topology));
147 return 0;
148 }
149
150 sprintf(path, "/sys/bus/pci/devices/%04x:%02x:%02x.%01x/local_cpus", pcidomain, pcibus, pcidev, pcifunc);
151 if (hwloc_linux_read_path_as_cpumask(path, set) < 0
152 || hwloc_bitmap_iszero(set))
153 hwloc_bitmap_copy(set, hwloc_topology_get_complete_cpuset(topology));
154 #else
155 /* Non-Linux systems simply get a full cpuset */
156 hwloc_bitmap_copy(set, hwloc_topology_get_complete_cpuset(topology));
157 #endif
158 return 0;
159 }
160
176 static __hwloc_inline hwloc_obj_t
177 hwloc_opencl_get_device_osdev_by_index(hwloc_topology_t topology,
178 unsigned platform_index, unsigned device_index)
179 {
180 unsigned x = (unsigned) -1, y = (unsigned) -1;
181 hwloc_obj_t osdev = NULL;
182 while ((osdev = hwloc_get_next_osdev(topology, osdev)) != NULL) {
183 if (HWLOC_OBJ_OSDEV_COPROC == osdev->attr->osdev.type
184 && osdev->name
185 && sscanf(osdev->name, "opencl%ud%u", &x, &y) == 2
186 && platform_index == x && device_index == y)
187 return osdev;
188 }
189 return NULL;
190 }
191
212 static __hwloc_inline hwloc_obj_t
213 hwloc_opencl_get_device_osdev(hwloc_topology_t topology __hwloc_attribute_unused,
214 cl_device_id device __hwloc_attribute_unused)
215 {
216 hwloc_obj_t osdev;
217 unsigned pcidomain, pcibus, pcidevice, pcifunc;
218
219 if (hwloc_opencl_get_device_pci_busid(device, &pcidomain, &pcibus, &pcidevice, &pcifunc) < 0) {
220 errno = EINVAL;
221 return NULL;
222 }
223
224 osdev = NULL;
225 while ((osdev = hwloc_get_next_osdev(topology, osdev)) != NULL) {
226 hwloc_obj_t pcidev = osdev->parent;
227 if (strncmp(osdev->name, "opencl", 6))
228 continue;
229 if (pcidev
230 && pcidev->type == HWLOC_OBJ_PCI_DEVICE
231 && pcidev->attr->pcidev.domain == pcidomain
232 && pcidev->attr->pcidev.bus == pcibus
233 && pcidev->attr->pcidev.dev == pcidevice
234 && pcidev->attr->pcidev.func == pcifunc)
235 return osdev;
236 /* if PCI are filtered out, we need a info attr to match on */
237 }
238
239 return NULL;
240 }
241
245 #ifdef __cplusplus
246 } /* extern "C" */
247 #endif
248
249
250 #endif /* HWLOC_OPENCL_H */
hwloc_bitmap_copy
int hwloc_bitmap_copy(hwloc_bitmap_t dst, hwloc_const_bitmap_t src)
Copy the contents of bitmap src into the already allocated bitmap dst.
hwloc_cl_device_topology_amd
Definition: opencl.h:46
HWLOC_OBJ_PCI_DEVICE
@ HWLOC_OBJ_PCI_DEVICE
PCI device (filtered out by default). They are not added to the topology unless I/O discovery is enab...
Definition: hwloc.h:266
hwloc_cl_device_topology_amd::pcie
struct hwloc_cl_device_topology_amd::@4 pcie
hwloc_cl_device_topology_amd::function
cl_char function
Definition: opencl.h:48
hwloc_obj_attr_u::hwloc_osdev_attr_s::type
hwloc_obj_osdev_type_t type
Definition: hwloc.h:652
hwloc_obj_attr_u::hwloc_pcidev_attr_s::domain
unsigned short domain
Definition: hwloc.h:621
hwloc_topology_get_complete_cpuset
hwloc_const_cpuset_t hwloc_topology_get_complete_cpuset(hwloc_topology_t topology)
Get complete CPU set.
hwloc_obj_attr_u::osdev
struct hwloc_obj_attr_u::hwloc_osdev_attr_s osdev
hwloc_obj::type
hwloc_obj_type_t type
Type of object.
Definition: hwloc.h:386
hwloc_obj::attr
union hwloc_obj_attr_u * attr
Object type-specific Attributes, may be NULL if no attribute value was found.
Definition: hwloc.h:403
hwloc_obj_attr_u::hwloc_pcidev_attr_s::func
unsigned char func
Definition: hwloc.h:625
hwloc_topology_t
struct hwloc_topology * hwloc_topology_t
Topology context.
Definition: hwloc.h:678
hwloc_obj
Structure of a topology object.
Definition: hwloc.h:384
hwloc_opencl_get_device_cpuset
static int hwloc_opencl_get_device_cpuset(hwloc_topology_t topology, cl_device_id device, hwloc_cpuset_t set)
Get the CPU set of logical processors that are physically close to OpenCL device device.
Definition: opencl.h:130
hwloc_obj::name
char * name
Object-specific name if any. Mostly used for identifying OS devices and Misc objects where a name str...
Definition: hwloc.h:396
hwloc_obj_attr_u::hwloc_pcidev_attr_s::bus
unsigned char bus
Definition: hwloc.h:625
hwloc_get_next_osdev
static hwloc_obj_t hwloc_get_next_osdev(hwloc_topology_t topology, hwloc_obj_t prev)
Get the next OS device in the system.
Definition: helper.h:1151
hwloc_topology_is_thissystem
int hwloc_topology_is_thissystem(hwloc_topology_t restrict topology)
Does the topology context come from this system?
hwloc_cl_device_topology_amd::type
cl_uint type
Definition: opencl.h:47
hwloc_obj::parent
struct hwloc_obj * parent
Parent, NULL if root (Machine object)
Definition: hwloc.h:434
hwloc_opencl_get_device_osdev_by_index
static hwloc_obj_t hwloc_opencl_get_device_osdev_by_index(hwloc_topology_t topology, unsigned platform_index, unsigned device_index)
Get the hwloc OS device object corresponding to the OpenCL device for the given indexes.
Definition: opencl.h:177
hwloc_obj_attr_u::pcidev
struct hwloc_obj_attr_u::hwloc_pcidev_attr_s pcidev
hwloc_cpuset_t
hwloc_bitmap_t hwloc_cpuset_t
A CPU set is a bitmap whose bits are set according to CPU physical OS indexes.
Definition: hwloc.h:140
hwloc_opencl_get_device_pci_busid
static int hwloc_opencl_get_device_pci_busid(cl_device_id device, unsigned *domain, unsigned *bus, unsigned *dev, unsigned *func)
Return the domain, bus and device IDs of the OpenCL device device.
Definition: opencl.h:74
hwloc_cl_device_topology_amd::raw
struct hwloc_cl_device_topology_amd::@3 raw
hwloc_opencl_get_device_osdev
static hwloc_obj_t hwloc_opencl_get_device_osdev(hwloc_topology_t topology, cl_device_id device)
Get the hwloc OS device object corresponding to OpenCL device deviceX.
Definition: opencl.h:213
hwloc_cl_device_topology_amd::device
cl_char device
Definition: opencl.h:48
hwloc_obj_attr_u::hwloc_pcidev_attr_s::dev
unsigned char dev
Definition: hwloc.h:625
hwloc_cl_device_topology_amd::bus
cl_char bus
Definition: opencl.h:48
hwloc_linux_read_path_as_cpumask
int hwloc_linux_read_path_as_cpumask(const char *path, hwloc_bitmap_t set)
Convert a linux kernel cpumask file path into a hwloc bitmap set.
hwloc_bitmap_iszero
int hwloc_bitmap_iszero(hwloc_const_bitmap_t bitmap)
Test whether bitmap bitmap is empty.
HWLOC_OBJ_OSDEV_COPROC
@ HWLOC_OBJ_OSDEV_COPROC
Operating system co-processor device. For instance "mic0" for a Xeon Phi (MIC) on Linux,...
Definition: hwloc.h:340