.. highlight:: c

.. _KRB5-RESPONDER-OTP-FLAGS-SEPARATE-PIN-data:

KRB5_RESPONDER_OTP_FLAGS_SEPARATE_PIN
=====================================

..
.. data:: KRB5_RESPONDER_OTP_FLAGS_SEPARATE_PIN
..

This flag indicates that the PIN MUST be returned as a separate item.

This flag only takes effect if KRB5_RESPONDER_OTP_FLAGS_COLLECT_PIN is set. If this flag is not set, the responder may either concatenate PIN + token value and store it as "value" in the answer or it may return them separately. If they are returned separately, they will be concatenated internally.

============================================ ======================
``KRB5_RESPONDER_OTP_FLAGS_SEPARATE_PIN``       ``0x0008``
============================================ ======================
