libnl 3.5.0

Neighbour Tables
Routing Library (libnl-route)

## Allocation/Freeing
struct rtnl_neightbl * | rtnl_neightbl_alloc (void)
void | rtnl_neightbl_put (struct rtnl_neightbl *neightbl)

## Neighbour Table Cache Management
int | rtnl_neightbl_alloc_cache (struct nl_sock *sk, struct nl_cache **result)
| Build a neighbour table cache including all neighbour tables currently configured in the kernel. More...
struct rtnl_neightbl * | rtnl_neightbl_get (struct nl_cache *cache, const char *name, int ifindex)
| Lookup neighbour table by name and optional interface index. More...

## Neighbour Table Modifications
int | rtnl_neightbl_build_change_request (struct rtnl_neightbl *old, struct rtnl_neightbl *tmpl, struct nl_msg **result)
| Builds a netlink change request message to change neighbour table attributes. More...
int | rtnl_neightbl_change (struct nl_sock *sk, struct rtnl_neightbl *old, struct rtnl_neightbl *tmpl)
| Change neighbour table attributes. More...

## Attribute Modification
void | rtnl_neightbl_set_family (struct rtnl_neightbl *ntbl, int family)
void | rtnl_neightbl_set_gc_interval (struct rtnl_neightbl *ntbl, uint64_t ms)
void | rtnl_neightbl_set_gc_tresh1 (struct rtnl_neightbl *ntbl, int thresh)
void | rtnl_neightbl_set_gc_tresh2 (struct rtnl_neightbl *ntbl, int thresh)
void | rtnl_neightbl_set_gc_tresh3 (struct rtnl_neightbl *ntbl, int thresh)
void | rtnl_neightbl_set_name (struct rtnl_neightbl *ntbl, const char *name)
void | rtnl_neightbl_set_dev (struct rtnl_neightbl *ntbl, int ifindex)
void | rtnl_neightbl_set_queue_len (struct rtnl_neightbl *ntbl, int len)
| Set the queue length for pending requests of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_proxy_queue_len (struct rtnl_neightbl *ntbl, int len)
| Set the queue length for delay proxy arp requests of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_app_probes (struct rtnl_neightbl *ntbl, int probes)
| Set the number of application probes of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_ucast_probes (struct rtnl_neightbl *ntbl, int probes)
| Set the number of unicast probes of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_mcast_probes (struct rtnl_neightbl *ntbl, int probes)
| Set the number of multicast probes of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_base_reachable_time (struct rtnl_neightbl *ntbl, uint64_t ms)
| Set the base reachable time of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_retrans_time (struct rtnl_neightbl *ntbl, uint64_t ms)
| Set the retransmit time of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_gc_stale_time (struct rtnl_neightbl *ntbl, uint64_t ms)
| Set the gc stale time of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_delay_probe_time (struct rtnl_neightbl *ntbl, uint64_t ms)
| Set the first probe delay time of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_anycast_delay (struct rtnl_neightbl *ntbl, uint64_t ms)
| Set the anycast delay of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_proxy_delay (struct rtnl_neightbl *ntbl, uint64_t ms)
| Set the proxy delay of a neighbour table to the specified value. More...
void | rtnl_neightbl_set_locktime (struct rtnl_neightbl *ntbl, uint64_t ms)
| Set the locktime of a neighbour table to the specified value. More...

## Detailed Description

## Function Documentation

## ◆ rtnl_neightbl_alloc_cache()

int rtnl_neightbl_alloc_cache | ( | struct nl_sock * | sk,
|  | struct nl_cache ** | result
| ) |  |

Build a neighbour table cache including all neighbour tables currently configured in the kernel.

Parameters

  sk | Netlink socket.
  result | Pointer to store resulting cache.

Allocates a new neighbour table cache, initializes it properly and updates it to include all neighbour tables currently configured in the kernel.

Returns
  0 on success or a negative error code.

Definition at line 400 of file neightbl.c.

References nl_cache_alloc_and_fill().

Here is the call graph for this function:

## ◆ rtnl_neightbl_get()

struct rtnl_neightbl* rtnl_neightbl_get | ( | struct nl_cache * | cache,
|  | const char * | name,
|  | int | ifindex
| ) |  |

Lookup neighbour table by name and optional interface index.

Parameters

  cache | neighbour table cache
  name | name of table
  ifindex | optional interface index

Looks up the neighbour table matching the specified name and optionally the specified ifindex to retrieve device specific parameter sets.

Returns
  ptr to neighbour table inside the cache or NULL if no match was found.

Definition at line 418 of file neightbl.c.

## ◆ rtnl_neightbl_build_change_request()

int rtnl_neightbl_build_change_request | ( | struct rtnl_neightbl * | old,
|  | struct rtnl_neightbl * | tmpl,
|  | struct nl_msg ** | result
| ) |  |

Builds a netlink change request message to change neighbour table attributes.

Parameters

  old | neighbour table to change
  tmpl | template with requested changes
  result | Pointer to store resulting message.

Builds a new netlink message requesting a change of neighbour table attributes. The netlink message header isn't fully equipped with all relevant fields and must be sent out via nl_send_auto_complete() or supplemented as needed. old must point to a neighbour table currently configured in the kernel and tmpl must contain the attributes to be changed set via `rtnl_neightbl_set_*` functions.

Returns
  0 on success or a negative error code.

Definition at line 461 of file neightbl.c.

References nla_put_nested(), NLA_PUT_STRING, NLA_PUT_U32, NLA_PUT_U64, nlmsg_alloc(), nlmsg_alloc_simple(), nlmsg_append(), and nlmsg_free().

Referenced by rtnl_neightbl_change().

Here is the call graph for this function:
Here is the caller graph for this function:

## ◆ rtnl_neightbl_change()

int rtnl_neightbl_change | ( | struct nl_sock * | sk,
|  | struct rtnl_neightbl * | old,
|  | struct rtnl_neightbl * | tmpl
| ) |  |

Change neighbour table attributes.

Parameters

  sk | Netlink socket.
  old | neighbour table to be changed
  tmpl | template with requested changes

Builds a new netlink message by calling rtnl_neightbl_build_change_request(), sends the request to the kernel and waits for the next ACK to be received, i.e. blocks until the request has been processed.

Returns
  0 on success or a negative error code

Definition at line 578 of file neightbl.c.

References nl_send_auto_complete(), nlmsg_free(), and rtnl_neightbl_build_change_request().

Here is the call graph for this function:

## ◆ rtnl_neightbl_set_queue_len()

void rtnl_neightbl_set_queue_len | ( | struct rtnl_neightbl * | ntbl,
|  | int | len
| ) |  |

Set the queue length for pending requests of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  len | new queue len

Definition at line 650 of file neightbl.c.

## ◆ rtnl_neightbl_set_proxy_queue_len()

void rtnl_neightbl_set_proxy_queue_len | ( | struct rtnl_neightbl * | ntbl,
|  | int | len
| ) |  |

Set the queue length for delay proxy arp requests of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  len | new queue len

Definition at line 662 of file neightbl.c.

## ◆ rtnl_neightbl_set_app_probes()

void rtnl_neightbl_set_app_probes | ( | struct rtnl_neightbl * | ntbl,
|  | int | probes
| ) |  |

Set the number of application probes of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  probes | new probes value

Definition at line 674 of file neightbl.c.

## ◆ rtnl_neightbl_set_ucast_probes()

void rtnl_neightbl_set_ucast_probes | ( | struct rtnl_neightbl * | ntbl,
|  | int | probes
| ) |  |

Set the number of unicast probes of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  probes | new probes value

Definition at line 686 of file neightbl.c.

## ◆ rtnl_neightbl_set_mcast_probes()

void rtnl_neightbl_set_mcast_probes | ( | struct rtnl_neightbl * | ntbl,
|  | int | probes
| ) |  |

Set the number of multicast probes of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  probes | new probes value

Definition at line 698 of file neightbl.c.

## ◆ rtnl_neightbl_set_base_reachable_time()

void rtnl_neightbl_set_base_reachable_time | ( | struct rtnl_neightbl * | ntbl,
|  | uint64_t | ms
| ) |  |

Set the base reachable time of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  ms | new base reachable time in milliseconds

Definition at line 710 of file neightbl.c.

## ◆ rtnl_neightbl_set_retrans_time()

void rtnl_neightbl_set_retrans_time | ( | struct rtnl_neightbl * | ntbl,
|  | uint64_t | ms
| ) |  |

Set the retransmit time of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  ms | new retransmit time

Definition at line 723 of file neightbl.c.

## ◆ rtnl_neightbl_set_gc_stale_time()

void rtnl_neightbl_set_gc_stale_time | ( | struct rtnl_neightbl * | ntbl,
|  | uint64_t | ms
| ) |  |

Set the gc stale time of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  ms | new gc stale time in milliseconds

Definition at line 735 of file neightbl.c.

## ◆ rtnl_neightbl_set_delay_probe_time()

void rtnl_neightbl_set_delay_probe_time | ( | struct rtnl_neightbl * | ntbl,
|  | uint64_t | ms
| ) |  |

Set the first probe delay time of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  ms | new first probe delay time in milliseconds

Definition at line 747 of file neightbl.c.

## ◆ rtnl_neightbl_set_anycast_delay()

void rtnl_neightbl_set_anycast_delay | ( | struct rtnl_neightbl * | ntbl,
|  | uint64_t | ms
| ) |  |

Set the anycast delay of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  ms | new anycast delay in milliseconds

Definition at line 759 of file neightbl.c.

## ◆ rtnl_neightbl_set_proxy_delay()

void rtnl_neightbl_set_proxy_delay | ( | struct rtnl_neightbl * | ntbl,
|  | uint64_t | ms
| ) |  |

Set the proxy delay of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  ms | new proxy delay in milliseconds

Definition at line 771 of file neightbl.c.

## ◆ rtnl_neightbl_set_locktime()

void rtnl_neightbl_set_locktime | ( | struct rtnl_neightbl * | ntbl,
|  | uint64_t | ms
| ) |  |

Set the locktime of a neighbour table to the specified value.

Parameters

  ntbl | neighbour table to change
  ms | new locktime in milliseconds

Definition at line 783 of file neightbl.c.