# nvme-lba-status-log(1) Manual Page

## NAME

nvme-lba-status-log - Send LBA Status Log Page request returns result and log

## SYNOPSIS

    nvme lba-status-log <device> [--rae | -r] [--output-format=<fmt> | -o <fmt>]

## DESCRIPTION

Retrieves the NVMe LBA Status Log Page from an NVMe device and provides the returned structure.

The <device> parameter is mandatory and may be either the NVMe character device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

On success, the returned LBA Status Log Page structure may be returned in one of several ways depending on the option flags; the structure may parsed by the program and printed in a readable format or the raw buffer may be printed to stdout for another program to parse.

## OPTIONS

-r
--rae

  Retain an Asynchronous Event.

-o <format>
--output-format=<format>

  Set the reporting format to normal, json, or binary. Only one output format can be used at a time.

## EXAMPLES

- Print the LBA Status Log page in a normal readable format:

      # nvme lba-status-log /dev/nvme0

- Show the output in json format

      # nvme lba-status-log /dev/nvme0 -o json
      +

      NVME

Part of the nvme-user suite