# nvme-zns-finish-zone(1) Manual Page

## NAME

nvme-zns-finish-zone - Finishes one or all zones

## SYNOPSIS

    nvme zns finish-zone nvme zns id-ctrl <device> [--namespace-id=<NUM> | -n <NUM>]
                                                    [--start-lba=<LBA> | -s <LBA>]
                                                    [--select-all | -a]

## DESCRIPTION

For the NVMe device given, issues the Zone Management Send command with the "Finish Zone" action. This will transition the zone to the full state on success.

The <device> parameter is mandatory and may be either the NVMe character device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

## OPTIONS

-n <NUM>
--namespace-id=<NUM>

  Use the provided namespace id for the command. If not provided, the namespace id of the block device will be used. If the command is issued to a non-block device, the parameter is required.

-s <lba>
--start-lba=<lba>

  The starting LBA of the zone to finish.

-a
--select-all

  Select all zones for this action.

## EXAMPLES

- Finish all zones on namespace 1:

      # nvme zns finish-zone /dev/nvme0 -a -n 1

## NVME

Part of nvme-cli