nvme-zns-close-zone(1)
======================

NAME
----
nvme-zns-close-zone - Closes one or all zones

SYNOPSIS
--------
[verse]
'nvme zns close-zone nvme zns id-ctrl' <device> [--namespace-id=<NUM> | -n <NUM>]
						[--start-lba=<LBA> | -s <LBA>]
						[--select-all | -a]

DESCRIPTION
-----------
For the NVMe device given, issues the Zone Management Send command with the
"Close Zone" action. This will transition the zone to the closed state.

The <device> parameter is mandatory and may be either the NVMe character
device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

OPTIONS
-------
-n <NUM>::
--namespace-id=<NUM>::
	Use the provided namespace id for the command. If not provided, the
	namespace id of the block device will be used. If the command is issued
	to a non-block device, the parameter is required.

-s <lba>::
--start-lba=<lba>::
	The starting LBA of the zone to close. 

-a::
--select-all::
	Select all zones for this action

EXAMPLES
--------
* Close all zones on namespace 1:
+
------------
# nvme zns close-zone /dev/nvme0 -a -n 1
------------

NVME
----
Part of nvme-cli
