# nvme-micron-selective-download(1)

## NAME

nvme-micron-selective-download - Performs selective firmware download that allows user to select which firmware binary to update for 9200 devices. This requires power cycle once the update completes.

## SYNOPSIS

    nvme micron selective-download <device> [--fw=<FILE>, -f <FILE>] [--select=<flag>, -s <flag>]

## DESCRIPTION

This command uses micron vendor specific nvme commands to download given firmware image to the specified 9200 device to update selected or all portions of firmware image.

The <device> parameter is mandatory and may be either the NVMe character device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

This will only work on Micron devices devices of model number 9200. Support for new devices may be added subsequently. Results for any other device are undefined.

## OPTIONS

-f <FILE>
--fw=<FILE>

  name of the firmware image file

-s <flag>
--select=<flag>

  flag that has following values

OOB

  This updates the OOB and main firmware\n"

EEP

  This updates the eeprom and main firmware\n"

ALL

  This updates the eeprom, OOB, and main firmware";

## EXAMPLES

- Update OOB and main firmware

      # nvme micron selective-download /dev/nvme0 --fw=firmware_bin --select=OOB
      # nvme micron selective-download /dev/nvme0 -f firmware_bin -s OOB

- Update OOB and main firmware

      # nvme micron selective-download /dev/nvme0 --fw=firmware_bin --select=EEP
      # nvme micron selective-download /dev/nvme0 -f firmware_bin --s EEP

- Update eeprom, OOB and main firmware

      # nvme micron selective-download /dev/nvme0 --fw=firmware_bin --select=ALL
      # nvme micron selective-download /dev/nvme0 -f firmware_bin --s ALL

## NVME

Part of the nvme-user suite