nvme-intel-temp-stats(1)
========================

NAME
----
nvme-intel-temp-stats - Send NVMe SMART log page request, returns result and log

SYNOPSIS
--------
[verse]
'nvme intel temp-stats' <device> [--raw-binary | -b]

DESCRIPTION
-----------
Retrieves the NVMe Intel Additional SMART log page from the device and
provides the returned structure.

The <device> parameter is mandatory and may be either the NVMe character
device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

On success, the returned smart log structure may be returned in one of
several ways depending on the option flags; the structure may parsed by
the program and printed in a readable format or the raw buffer may be
printed to stdout for another program to parse.

OPTIONS
-------
-b::
--raw-binary::
	Print the raw temperature stats log buffer to stdout.

EXAMPLES
--------
* Print the temperature stats log page in a human readable format:
+
------------
# nvme intel temp-stats /dev/nvme0
------------
+

* Print the raw SMART log to a file:
+
------------
# nvme intel temp-stats /dev/nvme0 --raw-binary > temp_stats_log.raw
------------
+
It is probably a bad idea to not redirect stdout when using this mode.

NVME
----
Part of the nvme-user suite
