nvme-micron-selective-download(1)
=================================

NAME
----
nvme-micron-selective-download - Performs selective firmware download that allows user
to select which firmware binary to update for 9200 devices. This requires power cycle
once the update completes.

SYNOPSIS
--------
[verse]
'nvme micron selective-download' <device> [--fw=<FILE>, -f <FILE>] [--select=<flag>, -s <flag>]

DESCRIPTION
-----------
This command uses micron vendor specific nvme commands to download given firmware image to the
specified 9200 device to update selected or all portions of firmware image. 

The <device> parameter is mandatory and may be either the NVMe
character device (ex: /dev/nvme0), or a namespace block device (ex:
/dev/nvme0n1). 

This will only work on Micron devices devices of model number 9200. Support for new devices
may be added subsequently. Results for any other device are undefined.

OPTIONS
-------
-f <FILE>::
--fw=<FILE>::
        name of the firmware image file
-s <flag>::
--select=<flag>::
        flag that has following values
         OOB:: This updates the OOB and main firmware\n"
         EEP:: This updates the eeprom and main firmware\n"
         ALL:: This updates the eeprom, OOB, and main firmware";

EXAMPLES
--------
* Update OOB and main firmware
+
------------
# nvme micron selective-download /dev/nvme0 --fw=firmware_bin --select=OOB
# nvme micron selective-download /dev/nvme0 -f firmware_bin -s OOB   

------------
* Update OOB and main firmware
+
------------
# nvme micron selective-download /dev/nvme0 --fw=firmware_bin --select=EEP
# nvme micron selective-download /dev/nvme0 -f firmware_bin --s EEP
------------
* Update eeprom, OOB and main firmware
+
------------
# nvme micron selective-download /dev/nvme0 --fw=firmware_bin --select=ALL
# nvme micron selective-download /dev/nvme0 -f firmware_bin --s ALL
------------

NVME
----
Part of the nvme-user suite
