# nvme-device-self-test(1) Manual Page

## NAME

nvme-device-self-test - Perform the necessary tests to observe the performance and the parameters

## SYNOPSIS

    nvme device-self-test <device> [--namespace-id=<NUM> | -n <NUM>]
                            [--self-test-code=<NUM> | -s <NUM>]

## DESCRIPTION

Initiates the required test based on the user input.

The <device> parameter is mandatory and may be either the NVMe character device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

On success, the corresponding test is initiated.

## OPTIONS

-n <NUM>
--namespace-id=<NUM>

  Indicate the namespace in which the device self-test has to becarried out

-s <NUM>
--self-test-code=<NUM>

  This field specifies the action taken by the device self-test command : 1h: Start a short device self-test operation 2h: Start a extended device self-test operation eh: Start a vendor specific device self-test operation fh: abort the device self-test operation

## EXAMPLES

- Start a short device self-test in the namespace-id 1:

      # nvme device-self-test /dev/nvme0 -n 1 -s 1

- Abort the device self-test operation in the namespace-id 1:

      # nvme device-self-test /dev/nvme0 -n 1 -s 0xf

## NVME

Part of the nvme-user suite