nvme-lba-status-log(1)
======================

NAME
----
nvme-lba-status-log - Send LBA Status Log Page request returns result and log

SYNOPSIS
--------
[verse]
'nvme lba-status-log' <device> [--rae | -r] [--output-format=<fmt> | -o <fmt>]

DESCRIPTION
-----------
Retrieves the NVMe LBA Status Log Page from an NVMe device and provides
the returned structure.

The <device> parameter is mandatory and may be either the NVMe character
device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

On success, the returned LBA Status Log Page structure may be returned
in one of several ways depending on the option flags; the structure may
parsed by the program and printed in a readable format or the raw buffer
may be printed to stdout for another program to parse.

OPTIONS
-------
-r::
--rae::
	Retain an Asynchronous Event.

-o <format>::
--output-format=<format>::
    Set the reporting format to 'normal', 'json', or 'binary'.
    Only one output format can be used at a time.

EXAMPLES
--------
* Print the LBA Status Log page in a normal readable format:
+
------------
# nvme lba-status-log /dev/nvme0
------------
+

* Show the output in json format
+
------------
# nvme lba-status-log /dev/nvme0 -o json
+

NVME
----
Part of the nvme-user suite