# nvme-zns-changed-zone-list(1) Manual Page

## NAME

nvme-zns-changed-zone-list - Retrieve Changed Zone log for the given device

## SYNOPSIS

    nvme zns changed-zone-list <device> [-o <fmt> | --output-format=<fmt>]
                                          [--namespace-id=<NUM> | -n <NUM>]
                                          [--rae | -r]

## DESCRIPTION

For the NVMe device given, requests the namespace’s changed zoned list log and provides the result and returned structure.

The <device> parameter is mandatory and may be either the NVMe character device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

On success, the returned list may be decoded and displayed in one of several ways.

## OPTIONS

-o <format>
--output-format=<format>

  Set the reporting format to normal, json, or binary. Only one output format can be used at a time.

-r
--rae

  Retain an Asynchronous Event.

## EXAMPLES

- Get the changed zone list log for namespace 1

      # nvme zns changed-zone-list /dev/nvme0 -n 1

- Show the output in json format

      # nvme zns changed-zone-list /dev/nvme0 -o json -n 1

## NVME

Part of nvme-cli