# nvme-sanitize-log(1) Manual Page

## NAME

nvme-sanitize-log - Send NVMe sanitize-log Command, return result

## SYNOPSIS

    nvme sanitize-log <device> [--rae | -r] [--output-format=<fmt> | -o <fmt>]
                                 [--human-readable | -H]
                                 [--raw-binary | -b]

## DESCRIPTION

Retrieves the NVMe Sanitize log page from an NVMe device and provides the status of sanitize command.

The <device> parameter is mandatory NVMe character device (ex: /dev/nvme0).

Expected status and description :-

Status Code | Description
--- | ---
0x0000 | NVM subsystem has never been sanitized.
0x0001 | The most recent sanitize operation completed successfully.
0x0002 | A sanitize operation is currently in progress.
0x0003 | The most recent sanitize operation failed.
0x0100 | Global Data Erased bit If set to 1 then non-volatile storage in the NVM subsystem has not been written to: a) since being manufactured and the NVM subsystem has never been sanitized; or b) since the most recent successful sanitize operation. If cleared to 0, then non-volatile storage in the NVM subsystem has been written to: a) since being manufactured and the NVM subsystem has never been sanitized; or b) since the most recent successful sanitize operation of the NVM subsystem.

Sanitize Progress - percentage complete

On success it returns 0, error code otherwise.

## OPTIONS

-r
--rae

  Retain an Asynchronous Event.

-o <format>
--output-format=<format>

  Set the reporting format to normal, json, or binary. Only one output format can be used at a time.

-H
--human-readable

  This option will parse and format many of the bit fields into human-readable formats.

-b
--raw-binary

  Print the raw buffer to stdout. Structure is not parsed by program. This overrides the vendor specific and human readable options.

## EXAMPLES

- Has the program issue Sanitize-log Command :

      # nvme sanitize-log /dev/nvme0

## NVME

Part of the nvme-user suite.