nvme-set-feature(1)
===================

NAME
----
nvme-set-feature - Sets an NVMe feature, returns applicable results

SYNOPSIS
--------
[verse]
'nvme set-feature' <device> [--namespace-id=<nsid> | -n <nsid>]
			  [--feature-id=<fid> | -f <fid>] [--value=<value> | -v <value>]
			  [--data-len=<data-len> | -l <data-len>]
			  [--data=<data-file> | -d <data-file>]
			  [--save| -s]

DESCRIPTION
-----------
Submits an NVMe Set Feature admin command and returns the applicable
results. This may be the feature's value, or may also include a feature
structure if the feature requires it (ex: LBA Range Type).

The <device> parameter is mandatory and may be either the NVMe character
device (ex: /dev/nvme0), or a namespace block device (ex: /dev/nvme0n1).

On success, the value sent to the device is displayed

OPTIONS
-------
-n <nsid>::
--namespace-id=<nsid>::
	Sets the feature for the given nsid. This is optional and
	most features do not use this value.

-f <fid>::
--feature-id=<fid>::
	The feature id to send with the command. Value provided should
	be in hex.

-l <data-len>::
--data-len=<data-len>::
	The data length for the buffer submitted for this feature. Most
	known features do not use this value. The exceptions are LBA
	Range Type and host identifier.

-d <data-file>::
--data=<data-file>::
	The data file for the buffer submitted for this feature. Most
	known features do not use this value. The exceptions is LBA
	Range Type and host identifier. This defaults to STDIN so files
	and echo can be piped.

-v <value>::
--value=<value>::
	The value for command dword 11, the value you want to set the
	feature to.

-s::
--save::
	Save the attribute so that it persists through all power states and resets.	

EXAMPLES
--------
* Sets the Power State (PS) to 1  in feature id 2:
+
------------
# nvme set-feature /dev/nvme0 -f 2 /dev/nvme0n1 -v 0x1
------------
+

* Sets the host id to the ascii string.
+
------------
# echo "abcdefgh" | nvme set-feature /dev/nvme0 -f 0x81 -l 8
------------

NVME
----
Part of the nvme-user suite
