---
date: 2018-10-19
footer: libibverbs
header: "Libibverbs Programmer's Manual"
layout: page
license: 'Licensed under the OpenIB.org BSD license (FreeBSD Variant) - See COPYING.md'
section: 3
title: IBV_ADVISE_MR
---

# NAME

ibv_advise_mr - Gives advice or directions to the kernel about an
		address range belongs to a memory region (MR).

# SYNOPSIS

```c
#include <infiniband/verbs.h>

int ibv_advise_mr(struct ibv_pd *pd,
		  enum ibv_advise_mr_advice advice,
		  uint32_t flags,
		  struct ibv_sge *sg_list,
		  uint32_t num_sge)
```

# DESCRIPTION

**ibv_advise_mr()** Give advice or directions to the kernel about an
address range belonging to a memory region (MR).
Applications that are aware of future access patterns can use this verb
in order to leverage this knowledge to improve system or
application performance.

**Conventional advice values**

*IBV_ADVISE_MR_ADVICE_PREFETCH*
:	Pre-fetch a range of an on-demand paging MR.
	Make pages present with read-only permission before the actual IO is conducted.
	This would provide a way to reduce latency by overlapping paging-in
	and either compute time or IO to other ranges.

*IBV_ADVISE_MR_ADVICE_PREFETCH_WRITE*
:	Like IBV_ADVISE_MR_ADVICE_PREFETCH but with read-access
	and write-access permission to the fetched memory.

*IBV_ADVISE_MR_ADVICE_PREFETCH_NO_FAULT*
:	Pre-fetch a range of an on-demand paging MR without faulting.
	This allows presented pages in the CPU to become presented to the device.

# ARGUMENTS
*pd*
:	The protection domain (PD) associated with the MR.

*advice*
:	The requested advise value (as listed above).

*flags*
:	Describes the properties of the advise operation
	**Conventional advice values**
	*IBV_ADVISE_MR_FLAG_FLUSH*
	:	Request to be a synchronized operation. Return to the caller
		after the operation is completed.

*sg_list*
:	Pointer to the s/g array
	When using IBV_ADVISE_OP_PREFETCH advise value, all the lkeys of all
	the scatter gather elements (SGEs) must be associated with ODP MRs
	(MRs that were registered with IBV_ACCESS_ON_DEMAND).

*num_sge*
:	Number of elements in the s/g array

# RETURN VALUE

**ibv_advise_mr()** returns 0 when the call was successful, or the value
		    of errno on failure (which indicates the failure reason).

*EOPNOTSUPP*
:	libibverbs or provider driver doesn't support the ibv_advise_mr() verb
	(ENOSYS may sometimes be returned by old versions of libibverbs).

*ENOTSUP*
:	The advise operation isn't supported.

*EFAULT*
:	In one of the following:
	o When the range requested is out of the MR bounds, or when parts of
	  it are not part of the process address space.
	o One of the lkeys provided in the scatter gather list is invalid or
	  with wrong write access.

*EINVAL*
:	In one of the following:
	o The PD is invalid.
	o The flags are invalid.

# NOTES

An application may pre-fetch any address range within an ODP MR when using the
**IBV_ADVISE_MR_ADVICE_PREFETCH** or **IBV_ADVISE_MR_ADVICE_PREFETCH_WRITE** advice.
Semantically, this operation is best-effort. That means the kernel does not
guarantee that underlying pages are updated in the HCA or the pre-fetched pages
would remain resident.

When using **IBV_ADVISE_MR_ADVICE_PREFETCH** or **IBV_ADVISE_MR_ADVICE_PREFETCH_WRITE**
advice, the operation will be done in the following stages:
	o Page in the user pages to memory (pages aren't pinned).
	o Get the dma mapping of these user pages.
	o Post the underlying page translations to the HCA.

If **IBV_ADVISE_MR_FLAG_FLUSH** is specified then the underlying pages are
guaranteed to be updated in the HCA before returning SUCCESS.
Otherwise the driver can choose to postpone the posting of the new translations
to the HCA.
When performing a local RDMA access operation it is recommended to use
IBV_ADVISE_MR_FLAG_FLUSH flag with one of the pre-fetch advices to
increase probability that the pages translations are valid in the HCA
and avoid future page faults.

# SEE ALSO

**ibv_reg_mr**(3),
**ibv_rereg_mr**(3),
**ibv_dereg_mr**(3)

# AUTHOR

Aviad Yehezkel <aviadye@mellanox.com>

