# This is the hex for a SAS protocol specific diagnostic
# page. It will attempt to stop phy identifier 1 of the
# given device producing a test pattern.
# N.B. This should make phy id 1 usable for SAS protocols again.
#
# Usage example: 'sg_senddiag --pf --raw=- /dev/sg2 < {this_file}'
#
3f,6,0,1c,1,0,2,9,
0,0,0,0,0,0,0,0,
0,0,0,0,0,0,0,0,
0,0,0,0,0,0,0,0
