# This is the hex for a SAS protocol specific diagnostic
# page. It will attempt to put phy identifier 1 of the
# given device into PRBS15 (jitter pattern) generation mode.
# Physical transmission speed is 22.5 Gbps
# N.B. This will turn the receiver off on phy id 1.
#
# Usage example: 'sg_senddiag --pf --raw=- /dev/sg2 < {this_file}'
#
3f,6,0,1c,1,1,4,c,
0,0,0,0,0,0,0,0,
0,0,0,0,0,0,0,0,
0,0,0,0,0,0,0,0
