= syslinux.cfg(5) =
:doctype: manpage
:revdate: 2012-10-28
:author: H. Peter Anvin
:author-email: hpa@zytor.com
:editor1: Gene Cumm
:editor1-email: gene.cumm@gmail.com
:editor1-revlast: 2012-10-28
:nbsp8: &#160;&#160;&#160;&#160;&#160;&#160;&#160;&#160;
:nbsp32: {nbsp8}{nbsp8}{nbsp8}{nbsp8}
:data-uri:

== NAME ==
syslinux.cfg - *Syslinux* configuration file


== DESCRIPTION ==
Configuration for the boot behavior and user experience of *Syslinux*
boot loaders, the format of display files and the boot prompt behavior.

Blank lines are ignored.

Note that the configuration file is not completely decoded.  Syntax
different from the one described above may still work correctly in this
version of *Syslinux*, but may break in a future one.


== LOCATION/NAME ==
*SYSLINUX* (before 4.00) used the configuration filename of
syslinux.cfg.  *EXTLINUX* (merged into *SYSLINUX* as of 4.00) used the
filename extlinux.conf.  Both default to searching for the config file
in the installed directory (containing ldlinux.sys/extlinux.sys).  As of
4.00, *SYSLINUX* will search for extlinux.conf then syslinux.cfg in each
directory before falling back to the next directory.

As of 3.35, *SYSLINUX* also searches /boot/syslinux, /syslinux and /.

*ISOLINUX* (before 4.02) used the configuration filename of
isolinux.cfg, searching  /boot/isolinux (starting 2.00), then /isolinux
and /.  As of 4.02, *ISOLINUX* will search for isolinux.cfg then
syslinux.cfg in /boot/isolinux before searching for the same files in
/isolinux, /boot/syslinux, /syslinux, and /.


== GLOBAL DIRECTIVES - MAIN ==
*#* comment::
A line comment.  As of version 3.10, the space between the *#* and the
comment is no longer required.

*MENU* any string::
(3.00+) A directive for the simple menu system, treated as a comment
outside the menu.  See menu.txt.

*INCLUDE* 'filename'::
Inserts the contents of another file at this point in the configuration
file. Files can currently be nested up to 16 levels deep, but it is not
guaranteed that more than 8 levels will be supported in the future.

*DEFAULT* 'kernel' 'options...'::
Sets the default command line (which often references a LABEL).  If
*Syslinux* boots automatically, it will act just as if the entries after
*DEFAULT* had been typed in at the 'boot:' prompt.  Multiple uses will
result in an override.
+
If no configuration file is present, or no *DEFAULT* or *UI* entry is
present in the config file, an error message is displayed and the
'boot:' prompt is shown (3.85+).

*UI* 'module' 'options...'::
Selects a specific user interface 'module' (typically menu.c32 or
vesamenu.c32).  The command-line interface treats this as a directive
that overrides the *DEFAULT* directive to load this module instead at
startup, for an empty command line and at timeout and *PROMPT* directive
to not prompt (but these directives may have effects on other
configuration parsers).  Multiple uses will result in an override.

*LABEL* 'mylabel'::
Begin a new *LABEL* clause.  If 'mylabel' is entered as the kernel to
boot, *Syslinux* should instead boot "image" (specified by a directive
from *KERNEL-LIKE DIRECTIVES*) with any specified *DUAL-PURPOSE
DIRECTIVES* being used instead of the global instance.
+
'mylabel' must be unique.  Currently the first instance is used but may
result in an error or undesired behavior.  'mylabel' ends at the first
character that is not a non-white-space printable character and should
be restricted to non-white-space typeable characters.  Prior to version
3.32, this would transformed to a DOS compatible format of 8.3 with a
restricted character set.  A *LABEL* clause must contain exactly 1 of
the *KERNEL-LIKE DIRECTIVES* and may contain 1 each of the *LABEL-ONLY
DIRECTIVES* or *DUAL-PURPOSE DIRECTIVES*.
+
Within a *LABEL*, using multiple *KERNEL-LIKE DIRECTIVES* or reuse of
*LABEL-ONLY DIRECTIVES* or *DUAL-PURPOSE DIRECTIVES* will result in an
override.  Otherwise, multiple instances of the same directive will
result in the last being effective.


== DUAL-PURPOSE DIRECTIVES ==
Use of any of the *DUAL-PURPOSE DIRECTIVES* as *GLOBAL DIRECTIVES* is
discouraged if there will be any non-Linux images loaded as *ALL* images
will get these, including those manually entered at the 'boot:' prompt.

*APPEND* 'options...'::
Add one or more options to the kernel command line.  These are added
both for automatic and manual boots.  The options are added at the very
beginning of the kernel command line, usually permitting explicitly
entered kernel options to override them.  This is the equivalent of the
LILO "append" option.
+
Use of the parameter 'initrd=' supports multiple filenames separated by
commas (ie 'initrd=initrd_file1,initrd_file2') within a single instance.
This is mostly useful for initramfs, which can be composed of multiple
separate cpio or cpio.gz archives.
+
Note: all initrd files except the last one are zero-padded to a 4K page
boundary.  This should not affect initramfs.
+
Note: Only the last effective 'initrd=' parameter is used for loading
initrd files.

*APPEND* -::
Append nothing.  *APPEND* with a single hyphen as argument in a *LABEL*
section can be used to override a global *APPEND*.

//[FIXME: Shorten subdefinitions]
*SYSAPPEND* 'bitmask'::
*IPAPPEND* 'bitmask'::
(*SYSAPPEND*: 5.10+; *IPAPPEND*: *PXELINUX* only)
The *SYSAPPEND* option was introduced in *Syslinux* 5.10; it is an
enhancement of a previous option *IPAPPEND* which was only available on
*PXELINUX*.  'bitmask' is interpreted as decimal format unless prefixed
with "0x" for hexadecimal or "0" (zero) for octal.  The 'bitmask' is an
OR (sum) of the following integer options:

ifndef::doctype-manpage[[horizontal]]
*1*::: An option of the following format should be generated, based on
the input from the DHCP/BOOTP or PXE boot server and added to the kernel
command line(see note below; empty for non-PXELINUX variants):
+
----
ip=<client-ip>:<boot-server-ip>:<gw-ip>:<netmask>
----
+
NOTE:  The use of option 1 is no substitute for running a DHCP client in
the booted system and should instead only be used to seed the client for
a request.  Without regular renewals, the lease acquired by the PXE BIOS
will expire, making the IP address available for reuse by the DHCP
server.
+
*2*::: An option of the following format should be generated, in
dash-separated hexadecimal with leading hardware type (same as for the
configuration file; see pxelinux.txt.) and added to the kernel command
line, allowing an initrd program to determine from which interface the
system booted(empty for non-PXELINUX variants):
+
----
BOOTIF=<hardware-address-of-boot-interface>
----
+
*4*::: An option of the following format should be generated, in lower
case hexadecimal in the format normally used for UUIDs (same as for the
configuration file; see pxelinux.txt.) and added to the kernel command
line:
+
----
SYSUUID=<system uuid>
----
+
*8*::: (5.10+) indicate the CPU family and certain particularly
significant CPU feature bits:
+
----
CPU=<family><features>
----
+
The <family> is a single digit from 3 (i386) to 6 (i686 or higher.)  The
following CPU features are currently reported; additional flags may be
added in the future:
+
....
P	Physical Address Extension (PAE)
V	Intel Virtualization Technology (VT/VMX)
T	Intel Trusted Exection Technology (TXT/SMX)
X	Execution Disable (XD/NX)
L	Long Mode (x86-64)
S	AMD SMX virtualization
....
+
*DMI*::: (5.10+) The following strings are derived from DMI/SMBIOS
information if available:
+
	Bit	String		Significance
	-------------------------------------------------------------
	0x00010	SYSVENDOR=	System vendor name
	0x00020	SYSPRODUCT=	System product name
	0x00040	SYSVERSION=	System version
	0x00080	SYSSERIAL=	System serial number
	0x00100	SYSSKU=		System SKU
	0x00200	SYSFAMILY=	System family
	0x00400	MBVENDOR=	Motherboard vendor name
	0x00800	MBPRODUCT=	Motherboard product name
	0x01000	MBVERSION=	Motherboard version
	0x02000	MBSERIAL=	Motherboard serial number
	0x04000 MBASSET=	Motherboard asset tag
	0x08000	BIOSVENDOR=	BIOS vendor name
	0x10000	BIOSVERSION=	BIOS version
	0x20000	SYSFF=		System form factor
+
If these strings contain white-space characters, they are replaced with
underscores (_).
+
The system form factor value is a number defined in the SMBIOS
specification, available at http://www.dmtf.org/.  As of version 2.7.1
of the specification, the following values are defined:
+
	  1	Other
	  2	Unknown
	  3	Desktop
	  4	Low profile desktop
	  5	Pizza box
	  6	Mini tower
	  7	Tower
	  8	Portble
	  9	Laptop
	 10	Notebook
	 11	Handheld
	 12	Docking station
	 13	All-in-one
	 14	Subnotebook
	 15	Space-saving
	 16	Lunch box
	 17	Main server chassis
	 18	Expansion chassis
	 19	Subchassis
	 20	Bus expansion chassis
	 21	Peripheral chassis
	 22	RAID chassis
	 23	Rack mount chasss
	 24	Sealed-case PC
	 25	Multi-system chassis
	 26	Compact PCI
	 27	Advanced TCI
	 28	Blade
	 29	Blade enclosure
+
*0x40000*::: (6.03+) Append a file system UUID string.  For EXT2/3/4, this is the typical file system UUID.  For FAT12/16/32, this is the 32-bit file system serial number (ie DA1A-0B2E).
+
----
FSUUID=<FS-UUID>
----


== KERNEL-LIKE DIRECTIVES ==
// Alpha sort after KERNEL and LINUX
*KERNEL* 'image'::
Load a kernel-like file 'image' with automatic filetype detection based
on file extension, listed under the non-auto-detecting directives,
defaulting to *LINUX*.

//[FIXME: Should "'image' as " be removed entirely or added to all? 
*LINUX* is used as an example]
*LINUX* 'image'::
Load 'image' as a Linux-like kernel. MEMDISK is an example of a
non-Linux kernel loaded in a Linux-like fashion.

*BOOT* 'image'::
(*ISOLINUX* only: .bin; *SYSLINUX* only: .bs) Load a boot sector.  .bin
is a "CD boot sector" and .bs is a regular disk boot sector.

*BSS* 'image'::
(*SYSLINUX* only: .bss) Load a BSS image, a .bs image with the DOS
superblock patched in.

*COMBOOT* 'image'::
(.com, .cbt; Removed as of 5.00) Load a *Syslinux* COMBOOT image.  .com
images may also be runnable from DOS while .cbt images are not.  See
also *comboot.txt*

*COM32* 'image'::
(.c32) Load a *Syslinux* COM32 (32-bit *COMBOOT*) image.  See also
*comboot.txt*

*CONFIG* 'image'::
Load a new configuration file.  The configuration file is read, the
working directory is changed (if specified via an *APPEND*), then the
configuration file is parsed.

*FDIMAGE* 'image'::
(Removed as of 4.05, added 1.65; *ISOLINUX* only: .img) Load a disk
image.

*LOCALBOOT* 'type'::
(*PXELINUX* 1.53+; *ISOLINUX* ??3.10+; *SYSLINUX* 3.70+)Attempt a
different local boot method.  The special value -1 causes the boot
loader to report failure to the BIOS, which, on recent BIOSes, should
mean that the next boot device in the boot sequence should be activated.
 Values other than those documented may produce undesired results.
+
On *PXELINUX*, 'type' 0 means perform a normal boot.  'type' 4 will
perform a local boot with the Universal Network Driver Interface (UNDI)
driver still resident in memory.  Finally, 'type' 5 will perform a local
boot with the entire PXE stack, including the UNDI driver, still
resident in memory. All other values are undefined.  If you don't know
what the UNDI or PXE stacks are, don't worry -- you don't want them,
just specify 0.
+
On *ISOLINUX*/*SYSLINUX*, the 'type' specifies the local drive number to
boot from; 0x00 is the primary floppy drive and 0x80 is the primary hard
drive.

*PXE* 'image'::
(*PXELINUX* only: .0) Load a PXE NBP (Network Boot Program) image.  The
PXE protocol does not provide any means for specifiying or using a
command line or initrd.


== LABEL-ONLY DIRECTIVES ==
*INITRD* 'initrd_file'::
(3.71+) An initrd can be specified in a separate statement (INITRD)
instead of as part of the *APPEND* statement; this functionally appends
"initrd=initrd_file" to the kernel command line.  Like 'initrd=', this
also supports multiple comma separated file names (see *APPEND*).


== GLOBAL DIRECTIVES - SECONDARY ==
These are global directives that are of lesser importance, often
affecting the user experience and not the boot process.

*ALLOWOPTIONS* 'flag_val'::
If 'flag_val' is 0, the user is not allowed to specify any arguments on
the kernel command line.  The only options recognized are those
specified in an *APPEND*) statement.  The default is 1.

*IMPLICIT* 'flag_val'::
If 'flag_val' is 0, do not load a kernel image unless it has been
explicitly named in a *LABEL* statement.  The default is 1.

*TIMEOUT* 'timeout'::
Indicates how long to wait at the 'boot:' prompt until booting
automatically, in units of 1/10 s.  The timeout is cancelled as soon as
the user types anything on the keyboard, the assumption being that the
user will complete the command line already begun.  The timer is reset
to 0 upon return from an unsuccessful attempt to boot or from a module. 
A timeout of zero (the default) will disable the timeout completely.

*TOTALTIMEOUT* 'timeout'::
Indicates how long to wait until booting automatically, in units of
1/10 s.  This timeout is *not* cancelled by user input, and can thus be
used to deal with serial port glitches or "the user walked away" type
situations.  A timeout of zero (the default) will disable the timeout
completely.
+
Both *TIMEOUT* and *TOTALTIMEOUT* can be used together, for example:
+
----
# Wait 5 seconds unless the user types something, but
# always boot after 15 minutes.
TIMEOUT 50
TOTALTIMEOUT 9000
----

// FIXME: be consistent
*ONTIMEOUT* 'kernel options...'::
Sets the command line invoked on a timeout (which often references a
LABEL).  If not specified, 'UI' (if used) or 'DEFAULT is used.

*ONERROR* 'kernel options...'::
If a kernel image is not found (either due to it not existing, or
because *IMPLICIT* is set), run the specified command.  The faulty
command line is appended to the specified options, so if the *ONERROR*
directive reads as:
+
----
ONERROR xyzzy plugh
----
+
and the command line as entered by the user is:
+
----
foo bar baz
----
+
*Syslinux* will execute the following as if entered by the user:
+
----
xyzzy plugh foo bar baz
----

*SERIAL* 'port [baudrate [flowcontrol]]'::
Enables a serial port to act as the console.  'port' is a number (0 =
/dev/ttyS0 = COM1, etc.) or an I/O port address (e.g. 0x3F8); if
'baudrate' is omitted, the baud rate defaults to 9600 bps.  The serial
parameters are hardcoded to be 8 bits, no parity, 1 stop bit.
+
'flowcontrol' is a combination of the following bits:
+
....
0x001 - Assert DTR
0x002 - Assert RTS
0x008 - Enable interrupts
0x010 - Wait for CTS assertion
0x020 - Wait for DSR assertion
0x040 - Wait for RI assertion
0x080 - Wait for DCD assertion
0x100 - Ignore input unless CTS asserted
0x200 - Ignore input unless DSR asserted
0x400 - Ignore input unless RI asserted
0x800 - Ignore input unless DCD asserted
....
+
All other bits are reserved.
+
Typical values are:
+
....
    0 - No flow control (default)
0x303 - Null modem cable detect
0x013 - RTS/CTS flow control
0x813 - RTS/CTS flow control, modem input
0x023 - DTR/DSR flow control
0x083 - DTR/DCD flow control
....
+
For the *SERIAL* directive to be guaranteed to work properly, it should
be the first directive in the configuration file.
+
NOTE: 'port' values from 0 to 3 means the first four serial ports
detected by the BIOS.  They may or may not correspond to the legacy port
values 0x3F8, 0x2F8, 0x3E8, 0x2E8.
+
Enabling interrupts (setting the 0x008 bit) may give better
responsiveness without setting the *NOHALT* option, but could
potentially cause problems with buggy BIOSes.
+
This option is "sticky" and is not automatically reset when loading a
new configuration file with the CONFIG command.

*NOHALT* 'flag_val'::
If 'flag_val' is 1, don't halt the processor while idle. Halting the
processor while idle significantly reduces the power consumption, but
can cause poor responsiveness to the serial console, especially when
using scripts to drive the serial console, as opposed to human
interaction.

*CONSOLE* 'flag_val'::
If 'flag_val' is 0, disable output to the normal video console. If
'flag_val' is 1, enable output to the video console (this is the
default.)
+
Some BIOSes try to forward this to the serial console and sometimes make
a total mess thereof, so this option lets you disable the video console
on these systems.

*FONT* 'filename'::
Load a font in .psf format before displaying any output (except the
copyright line, which is output as ldlinux.sys itself is loaded.) 
*Syslinux* only loads the font onto the video card; if the .psf file
contains a Unicode table it is ignored.  This only works on EGA and VGA
cards; hopefully it should do nothing on others.

*KBDMAP* 'keymap'::
Install a simple keyboard map.  The keyboard remapper used is *very*
simplistic (it simply remaps the keycodes received from the BIOS, which
means that only the key combinations relevant in the default layout --
usually U.S. English -- can be mapped) but should at least help people
with AZERTY keyboard layout and the locations of = and , (two special
characters used heavily on the Linux kernel command line.)
+
The included program keytab-lilo.pl from the LILO distribution can be
used to create such keymaps.  The file keytab-lilo.txt contains the
documentation for this program.

*DISPLAY* 'filename'::
Displays the indicated file on the screen at boot time (before the boot:
prompt, if displayed).  Please see the section below on *DISPLAY* files.
+
NOTE: If the file is missing, this option is simply ignored.

*SAY* 'message'::
Prints the message on the screen.

*PROMPT* 'flag_val'::
If 'flag_val' is 0, display the boot: prompt only if the Shift or Alt
key is pressed, or Caps Lock or Scroll lock is set (this is the
default).  If 'flag_val' is 1, always display the boot: prompt.

*NOESCAPE* 'flag_val'::
If 'flag_val' is set to 1, ignore the Shift/Alt/Caps Lock/Scroll Lock
escapes.  Use this (together with PROMPT 0) to force the default boot
alternative.

*NOCOMPLETE* 'flag_val'::
If 'flag_val' is set to 1, the Tab key does not display labels at the
boot: prompt.

//   ...etc...
*F1* 'filename'::
*F2* 'filename'::
*F3* 'filename'::
*F4* 'filename'::
*F5* 'filename'::
*F6* 'filename'::
*F7* 'filename'::
*F8* 'filename'::
*F9* 'filename'::
*F10* 'filename'::
*F11* 'filename'::
*F12* 'filename'::
Displays the indicated file on the screen when a function key is pressed
at the boot: prompt.  This can be used to implement pre-boot online help
(presumably for the kernel command line options.)  Please see the
section below on DISPLAY files.
+
When using the serial console, press <Ctrl-F><digit> to get to the help
screens, e.g. <Ctrl-F><2> to get to the F2 screen. For F10-F12, hit
<Ctrl-F><A>, <Ctrl-F>B, <Ctrl-F>C.  For compatibility with earlier
versions, F10 can also be entered as <Ctrl-F>0.

*PATH* 'path'::
(5.00+) Specify a space-separated (' '; 5.00-5.10 was a colon ':') list
of directories to search when attempting to load modules. This directive
is useful for specifying the directories containing the lib*.c32 library
files as other modules may be dependent on these files, but may not
reside in the same directory.  Multiple instances will append additional
paths.

*SENDCOOKIES* 'bitmask'::
(*PXELINUX* 5.10+) When downloading files over http, the SYSAPPEND
strings are prepended with _Syslinux_ and sent to the server as cookies.
The cookies are URL-encoded; whitespace is *not* replaced with
underscores.
+
This command limits the cookies send; 0 means no cookies.  The default
is -1, meaning send all cookies.
+
This option is "sticky" and is not automatically reset when loading a
new configuration file with the CONFIG command.


== DISPLAY FILE FORMAT ==
DISPLAY and function-key help files are text files in either DOS or UNIX
format (with or without <CR>).  In addition, the following special codes
are interpreted:

//[FIXME]: #1 doesn't break; #2 as-is; #3 broken but not on right; #4
identical to #3
// horizontal extends the line's label, reducing the definition
// tab or space to shift explanation ?  align beginning or end?

// ifndef::doctype-manpage[[horizontal]]
*<FF>*:: {nbsp32} 				= <Ctrl-L> = ASCII 12 +
Clear the screen, home the cursor.  Note that the screen is filled with
the current display color.

*<FF>*::
= <Ctrl-L> = ASCII 12; Clear the screen, home the cursor.  Note that the
screen is filled with the current display color.

*<FF>*::                                      <FF> = <Ctrl-L> = ASCII 12
+
Clear the screen, home the cursor.  Note that the screen is filled with
the current display color.

*<FF>*::
<FF> = <Ctrl-L> = ASCII 12 +
Clear the screen, home the cursor.  Note that the screen is filled with
the current display color.

*<SI>*'<bg><fg>'::                            <SI> = <Ctrl-O> = ASCII 15
+
Set the display colors to the specified background and foreground
colors, where <bg> and <fg> are the 2 hex digits representing 1 byte,
corresponding to the standard PC display attributes:
+
        0 = black               8 = dark grey
        1 = dark blue           9 = bright blue
        2 = dark green          a = bright green
        3 = dark cyan           b = bright cyan
        4 = dark red            c = bright red
        5 = dark purple         d = bright purple
        6 = brown               e = yellow
        7 = light grey          f = white
+
Picking a bright color (8-f) for the background results in the
corresponding dark color (0-7), with the foreground flashing.
+
Colors are not visible over the serial console.

*<CAN>*'filename<newline>'::                 <CAN> = <Ctrl-X> = ASCII 24
+
If a VGA display is present, enter graphics mode and display the graphic
included in the specified file.  The file format is an ad hoc format
called LSS16; the included Perl program "ppmtolss16" can be used to
produce these images.  This Perl program also includes the file format
specification.
+
The image is displayed in 640x480 16-color mode.  Once in graphics mode,
the display attributes (set by <SI> code sequences) work slightly
differently: the background color is ignored, and the foreground colors
are the 16 colors specified in the image file.  For that reason,
ppmtolss16 allows you to specify that certain colors should be assigned
to specific color indicies.
+
Color indicies 0 and 7, in particular, should be chosen with care: 0 is
the background color, and 7 is the color used for the text printed by
*Syslinux* itself.

*<EM>*::				<EM> = <Ctrl-Y> = ASCII 25 +
If we are currently in graphics mode, return to text mode.

*<DLE>*..*<ETB>*::			<Ctrl-P>..<Ctrl-W> = ASCII 16-23
+
These codes can be used to select which modes to print a certain part of
the message file in.  Each of these control characters select a specific
set of modes (text screen, graphics screen, serial port) for which the
output is actually displayed:
+
	Character			Text	Graph	Serial
	------------------------------------------------------
	<DLE> = <Ctrl-P> = ASCII 16	No	No	No
	<DC1> = <Ctrl-Q> = ASCII 17	Yes	No	No
	<DC2> = <Ctrl-R> = ASCII 18	No	Yes	No
	<DC3> = <Ctrl-S> = ASCII 19	Yes	Yes	No
	<DC4> = <Ctrl-T> = ASCII 20	No	No	Yes
	<NAK> = <Ctrl-U> = ASCII 21	Yes	No	Yes
	<SYN> = <Ctrl-V> = ASCII 22	No	Yes	Yes
	<ETB> = <Ctrl-W> = ASCII 23	Yes	Yes	Yes
+
For example, the following will actually print out which mode the
console is in:
+
	<DC1>Text mode<DC2>Graphics mode<DC4>Serial port<ETB>

*<SUB>*::                                   <SUB> = <Ctrl-Z> = ASCII 26
+
End of file (DOS convention).

*<BEL>*::				<BEL> = <Ctrl-G> = ASCII 7 +
Beep the speaker.


== BOOT LOADER IDS USED ==
The Linux boot protocol supports a "boot loader ID", a single byte where
the upper nybble specifies a boot loader family (3 = *Syslinux*) and the
lower nybble is version or, in the case of *Syslinux*, media:

	0x31 (49) = SYSLINUX
	0x32 (50) = PXELINUX
	0x33 (51) = ISOLINUX
	0x34 (52) = EXTLINUX

In recent versions of Linux, this ID is available as
/proc/sys/kernel/bootloader_type.


== NOVICE PROTECTION ==
*Syslinux* will attempt to detect booting on a machine with too little
memory, which means the Linux boot sequence cannot complete.  If so, a
message is displayed and the boot sequence aborted.  Holding down the
Ctrl key while booting disables this feature.

Any file that *Syslinux* uses can be marked hidden, system or readonly
if so is convenient; *Syslinux* ignores all file attributes.  The
*SYSLINUX* installer automatically sets the readonly/hidden/system
attributes on LDLINUX.SYS.

== EXAMPLE ==
Here are some sample config files:
----
# SERIAL 0 115200
DEFAULT linux
PROMPT 1
TIMEOUT 600

LABEL linux
  LINUX vmlinuz
  APPEND initrd=initrd1.gz,initrd2.gz

LABEL m
  COM32 menu.c32
----
In this example, serial port use is disabled but can be enabled by
uncommenting the first line and utilize serial port 0 at 115200 bps.  If
'linux' is typed on the command line, the kernel-like file 'vmlinuz' is
executed as a Linux kernel, initrd files initrd1.gz and initrd2.gz are
loaded as initial ramdisk files (like cpio.gz files for initramfs).  If
'm' is typed on the command line, the COM32 module 'menu.c32' is
executed to launch a menu system.



== KNOWN BUGS ==
include::com-bug.txt[]


== BUG REPORTS ==
include::com-rpt.txt[]


== AUTHOR ==
This AsciiDoc derived document is a modified version of the original
*SYSLINUX* documentation by {author} <{author-email}>.  The conversion
to an AsciiDoc was made by {editor1} <{editor1-email}>
