# wc3270-script Manual Page

## Contents

> Name
> Synopsis
> Description
> Status Format
> Differences
> Basic Programming Strategies
> Script-Specific Actions
> File Transfer
> See Also
> Version

## Name

Scripting Facilities for wc3270 and ws3270

## Synopsis

wc3270 -scriptport port [ ws3270-options ]
ws3270 [ ws3270-options ]
Script ( command [ ,arg... ] )

## Description

The x3270 scripting facilities allow the interactive 3270 emulator wc3270 to be operated under the control of another program, and forms the basis for the script-only emulator ws3270.

There are three basic scripting methods. The first is the peer script facility, the default mode for ws3270. This runs the emulator as a child of another process. Typically this would be a script using expect(1), perl(1), or the co-process facility of the Korn Shell ksh(1). In this mode, the emulator process looks for commands on its standard input, and places the responses on standard output.

The second method is the child script facility, invoked by the emulator's Script action. This runs a script as a child process of the emulator. The emulator creates a TCP listening socket on the IPv4 loopback address, 127.0.0.1, and places the TCP port in the environment variable X3270PORT (e.g., the text string "47196" if the TCP port is 47196).

The third method uses a TCP socket. The -scrpiptport command-line option causes the emulator to bind a socket to the specified port (on the IPv4 loopback address, 127.0.0.1). The emulator accepts TCP connections on that port. Multiple commands and responses can be sent over each connection. (Note that if the Script action is used with -scriptport, it will pass the scriptport port number to child scripts, rather than creating a new socket.)

It is possible to nest the methods. For example, a peer or TCP socket script can invoke the Script action. The calling script will be resumed when the nested script completes.

Commands are emulator actions; the syntax is the same as for the right-hand side of a wc3270 keymap. Unlike translation tables, action names are case-insensitive, can be uniquely abbreviated, and the parentheses may be omitted if there are no parameters. Any input line that begins with # or ! is treaded as a comment and will be ignored.

Any emulator action may be specified. Several specific actions have been defined for use by scripts, and the behavior of certain other actions (and of the emulators in general) is different when an action is initiated by a script.

Some actions generate output; some may delay completion until the certain external events occur, such as the host unlocking the keyboard. The completion of every command is marked by a two-line message. The first line is the current status of the emulator, documented below. If the command is successful, the second line is the string "ok"; otherwise it is the string "error".

## Status Format

The status message consists of 12 blank-separated fields:

1 Keyboard State
  If the keyboard is unlocked, the letter U. If the keyboard is locked waiting for a response from the host, or if not connected to a host, the letter L. If the keyboard is locked because of an operator error (field overflow, protected field, etc.), the letter E.
2 Screen Formatting
  If the screen is formatted, the letter F. If unformatted or in NVT mode, the letter U.
3 Field Protection
  If the field containing the cursor is protected, the letter P. If unprotected or unformatted, the letter U.
4 Connection State
  If connected to a host, the string C(hostname). Otherwise, the letter N.
5 Emulator Mode
  If connected in 3270 mode, the letter I. If connected in NVT line mode, the letter L. If connected in NVT character mode, the letter C. If connected in unnegotiated mode (no BIND active from the host), the letter P. If not connected, the letter N.
6 Model Number (2-5)
7 Number of Rows
  The current number of rows defined on the screen. The host can request that the emulator use a 24x80 screen, so this number may be smaller than the maximum number of rows possible with the current model.
8 Number of Columns
  The current number of columns defined on the screen, subject to the same difference for rows, above.
9 Cursor Row
  The current cursor row (zero-origin).
10 Cursor Column
  The current cursor column (zero-origin).
11 Window ID
  The X window identifier for the main x3270 window, in hexadecimal preceded by 0x. For ws3270 and wc3270, this is zero.
12 Command Execution Time
  The time that it took for the host to respond to the previous commnd, in seconds with milliseconds after the decimal. If the previous command did not require a host response, this is a dash.

## Differences

When an action is initiated by a script, the emulators behave in several different ways:

If an error occurs in processing an action, the usual pop-up window does not appear. Instead, the text is written to standard output.

If end-of-file is detected on standard input, the emulator exits. (A script can exit without killing the emulator by using the CloseScript action, below.) Note that this applies to peer scripts only; end-of-file on the pipe connected to a child script simply causes the pipes to be closed and the Script action to complete.

The Quit action always causes the emulator to exit. (When called from the keyboard, it will exit only if not connected to a host.)

Normally, the AID actions (Clear, Enter, PF, and PA) will not complete until the host unlocks the keyboard. If the parameter to a String action includes a code for one these actions, it will also wait for the keyboard to unlock before proceeding.

The AidWait toggle controls with behavior. When this toggle is set (the default), actions block as described above. When the toggle is clear, AID actions complete immediately. The Wait(Output) action can then be used to delay a script until the host changes something on the screen, and the Wait(Unlock) action can be used to delay a script until the host unlocks the keyboard, regardless of the state of the AidWait toggle.

Note that the Script action does not complete until the CloseScript action is called by the child process. This behavior is not affected by the state of the AidWait toggle.

## Basic Programming Strategies

3270 session scripting can be more difficult than other kinds of scripting, because it can be hard to tell when the host is finished processing a command. There is a well-defined 3270 Data Stream facility for doing this: The emulator locks the keyboard when it sends the host an AID, and the later host unlocks the keyboard. The emulator supports this facility directly by not allowing an AID action to complete until the keyboard is unlocked. Unfortunately, some hosts and some host applications unlock the keyboard as soon as they begin processing the command, instead of after it is finished. A human operator can see on the screen when the command is finished (e.g., when a READY prompt is displayed), but it can be difficult for a script to do this. For such early-unlock hosts, the only option in a script is to poll the screen until it can determine that the command is complete.

Another complication is that host I/O and script operation are asynchronous. That is, the host can update the screen at any time, even between actions that are reading the screen contents, so a script can get inconsistent results. Assistance for this problem is provided by the Snap action. The Snap(Save) action saves a snapshot of the screen in a special buffer. Then the script can use Snap variants of the Ascii and Ebcdic actions (Snap(Ascii) and Snap(Ebcdic)) to query the saved buffer -- which the host cannot modify -- to get the data it wants. Finally, Snap(Wait Output) blocks the script until the host modifies the screen, specifically since the last call to Snap(Save). Thus a script can poll the screen efficiently by writing a loop that begins with Snap(Save) and ends with Snap(Wait Output).

## Script-Specific Actions

The following actions have been defined or modified for use with scripts. (Note that unlike the display on the status line, row and col coordinates used in these actions use [0,0] as their origin at the upper left, not [1,1]).

AnsiText
  Outputs whatever data that has been output by the host in NVT mode since the last time that AnsiText was called. The data is preceded by the string "data: ", and has had all control characters expanded into C backslash sequences.

  This is a convenient way to capture NVT mode output in a synchronous manner without trying to decode the screen contents.

Ascii(row,col,rows,cols)
Ascii(row,col,length)
Ascii(length)
Ascii
  Outputs an ASCII text representation of the screen contents. Each line is preceded by the string "data: ", and there are no control characters.

  If four parameters are given, a rectangular region of the screen is output. (Note that the row and column are zero-origin.)

  If three parameters are given, length characters are output, starting at the specified zero-origin row and column.

  If only the length parameter is given, that many characters are output, starting at the cursor position.

  If no parameters are given, the entire screen is output.

  The EBCDIC-to-ASCII translation and output character set depend on the both the emulator character set (the -charset option) and the locale. UTF-8 and certain DBCS locales may result in multi-byte expansions of EBCDIC characters that translate to ASCII codes greater than 0x7f.

AsciiField
  Outputs an ASCII text representation of the field containing the cursor. The text is preceded by the string "data: ".
Connect(hostname)
  Connects to a host. The command does not return until the emulator is successfully connected in the proper mode, or the connection fails.
CloseScript(status)
  Causes the emulator to stop reading commands from the script. This is useful to allow a peer script to exit, with the emulator proceeding interactively. (Without this command, the emulator would exit when it detected end-of-file on standard input.) If the script was invoked by the Script action, the optional status is used as the return status of Script; if nonzero, Script will complete with an error, and if this script was invoked as part of login through the ibm_hosts file, the connection will be broken.
ContinueScript([param])
  Allows a script that is waiting in a PauseScript action, below, to continue. The optional param string is output by the PauseScript action.
Disconnect
  Disconnects from the host.
Ebcdic(row,col,rows,cols)
Ebcdic(row,col,length)
Ebcdic(length)
Ebcdic
  The same function as Ascii above, except that rather than generating ASCII text, each character is output as a 2-digit or 4-digit hexadecimal EBCDIC code.
EbcdicField
  The same function as AsciiField above, except that it generates hexadecimal EBCDIC codes.
Info(message)
  In x3270, pops up an informational message. In c3270 and wc3270, writes an informational message to the OIA (the line below the display). Not defined for s3270 or tcl3270.
Expect(text[,timeout])
  Pauses the script until the specified text appears in the data stream from the host, or the specified timeout (in seconds) expires. If no timeout is specified, the default is 30 seconds. Text can contain standard C-language escape (backslash) sequences. No wild-card characters or pattern anchor characters are understood. Expect is valid only in NVT mode.
Keymap([keymap])
  Adds or removes a temporary keymap. If the keymap parameter is given, the named keymap is added. If no parameter is given, the most recently added keymap is removed.
MoveCursor(row,col)
  Moves the cursor to the specified zero-origin coordinates.
PauseScript
  Stops a script until the ContinueScript action, above, is executed. This allows a script to wait for user input and continue. Outputs the single parameter to ContinueScript, if one is given.
PrintText([command,]filter)
  Pipes an ASCII representation of the current screen image through the named filter, e.g., lpr.
PrintText([html,][append,][replace,]file,filename)
  Saves the current screen contents in a file. With the html option, saves it as HTML, otherwise saves it as plain ASCII. The append option (the default) causes the data to be appended to the file if it already exists. The replace option causes the file to be overwritten instead.
PrintText(html,string)
  Returns the current screen contents as HTML.
Query(keyword)
  Returns state information. Keywords are:

  Keyword | Output
  BindPluName | BIND PLU returned by the host
  ConnectionState | TN3270/TN3270E mode and submode
  CodePage | Host code page
  Cursor | Cursor position (row col)
  Formatted | 3270 format state (formatted or unformatted)
  Host | Host name and port
  LocalEncoding | Local character encoding
  LuName | Host name LU name
  Model | 3270 model name (IBM-327x-n)
  ScreenCurSize | Current screen size (rows cols)
  ScreenMaxSize | Maximum screen size (rows cols)
  Ssl | SSL state (secure or not-secure) and host validation state (host-verified or host-unverified)

  Without a keyword, Query returns each of the defined attributes, one per line, labeled by its name.

ReadBuffer(Ascii)
  Dumps the contents of the screen buffer, one line at a time. Positions inside data fields are generally output as 2-digit hexadecimal codes in the current display character set. If the current locale specifies UTF-8 (or certain DBCS character sets), some positions may be output as multi-byte strings (4-, 6- or 8-digit codes). DBCS characters take two positions in the screen buffer; the first location is output as a multi-byte string in the current locale codeset, and the second location is output as a dash. Start-of-field characters (each of which takes up a display position) are output as SF(aa=nn[,...]), where aa is a field attribute type and nn is its value.

  Attribute | Values
  c0 basic 3270 | 20 protected
  | 10 numeric
  | 04 detectable
  | 08 intensified
  | 0c non-display
  | 01 modified
  41 highlighting | f1 blink
  | f2 reverse
  | f4 underscore
  | f8 intensify
  42 foreground | f0 neutral black
  | f1 blue
  | f2 red
  | f3 pink
  | f4 green
  | f5 turquoise
  | f6 yellow
  | f7 neutral white
  | f8 black
  | f9 deep blue
  | fa orange
  | fb purple
  | fc pale green
  | fd pale turquoise
  | fe grey
  | ff white
  43 character set | f0 default
  | f1 APL
  | f8 DBCS

  Extended attributes (which do not take up display positions) are output as SA(aa=nn), with aa and nn having the same definitions as above (though the basic 3270 attribute will never appear as an extended attribute).

  In addition, NULL characters in the screen buffer are reported as ASCII character 00 instead of 20, even though they should be displayed as blanks.

ReadBuffer(Ebcdic)
  Equivalent to ReadBuffer(Ascii), but with the data fields output as hexadecimal EBCDIC codes instead. Additionally, if a buffer position has the Graphic Escape attribute, it is displayed as GE(xx).
Script(path[,arg...])
  Runs a child script, passing it optional command-line arguments. path must specify an executable (binary) program: the emulator will create a new process and execute it. If you simply want the emulator to read commands from a file, use the Source action.
Snap
  Equivalent to Snap(Save) (see below).
Snap(Ascii,...)
  Performs the Ascii action on the saved screen image.
Snap(Cols)
  Returns the number of columns in the saved screen image.
Snap(Ebcdic,...)
  Performs the Ebcdic action on the saved screen image.
Snap(ReadBuffer)
  Performs the ReadBuffer action on the saved screen image.
Snap(Rows)
  Returns the number of rows in the saved screen image.
Snap(Save)
  Saves a copy of the screen image and status in a temporary buffer. This copy can be queried with other Snap actions to allow a script to examine a consistent screen image, even when the host may be changing the image (or even the screen dimensions) dynamically.
Snap(Status)
  Returns the status line from when the screen was last saved.
Snap(Wait[,timeout],Output)
  Pauses the script until the host sends further output, then updates the snap buffer with the new screen contents. Used when the host unlocks the keyboard (allowing the script to proceed after an Enter, PF or PA action), but has not finished updating the screen. This action is usually invoked in a loop that uses the Snap(Ascii) or Snap(Ebcdic) action to scan the screen for some pattern that indicates that the host has fully processed the last command.

  The optional timeout parameter specifies a number of seconds to wait before failing the Snap action. The default is to wait indefinitely.

Source(file)
  Read and execute commands from file. Any output from those commands will become the output from Source. If any of the commands fails, the Source command will not abort; it will continue reading commands until EOF.
Title(text)
  Changes the wc3270 window title to text.
Transfer(keyword=value,...)
  Invokes IND$FILE file transfer. See FILE TRANSFER below.
Wait([timeout,] 3270Mode)
  Used when communicating with a host that switches between NVT mode and 3270 mode. Pauses the script or macro until the host negotiates 3270 mode, then waits for a formatted screen as above.

  The optional timeout parameter specifies a number of seconds to wait before failing the Wait action. The default is to wait indefinitely.

  For backwards compatibility, Wait(3270) is equivalent to Wait(3270Mode)

Wait([timeout,] Disconnect)
  Pauses the script until the host disconnects. Often used to after sending a logoff command to a VM/CMS host, to ensure that the session is not unintentionally set to disconnected state.

  The optional timeout parameter specifies a number of seconds to wait before failing the Wait action. The default is to wait indefinitely.

Wait([timeout,] InputField)
  A useful utility for use at the beginning of scripts and after the Connect action. In 3270 mode, waits until the screen is formatted, and the host has positioned the cursor on a modifiable field. In NVT mode, waits until the host sends at least one byte of data.

  The optional timeout parameter specifies a number of seconds to wait before failing the Wait action. The default is to wait indefinitely.

  For backwards compatibility, Wait is equivalent to Wait(InputField).

Wait([timeout,] NVTMode)
  Used when communicating with a host that switches between 3270 mode and NVT mode. Pauses the script or macro until the host negotiates NVT mode, then waits for a byte from the host as above.

  The optional timeout parameter specifies a number of seconds to wait before failing the Wait action. The default is to wait indefinitely.

  For backwards compatibility, Wait(ansi) is equivalent to Wait(NVTMode).

Wait([timeout,] Output)
  Pauses the script until the host sends further output. Often needed when the host unlocks the keyboard (allowing the script to proceed after a Clear, Enter, PF or PA action), but has not finished updating the screen. Also used in non-blocking AID mode (see DIFFERENCES for details). This action is usually invoked in a loop that uses the Ascii or Ebcdic action to scan the screen for some pattern that indicates that the host has fully processed the last command.

  The optional timeout parameter specifies a number of seconds to wait before failing the Wait action. The default is to wait indefinitely.

Wait([timeout,] Unlock)
  Pauses the script until the host unlocks the keyboard. This is useful when operating in non-blocking AID mode (toggle AidWait clear), to wait for a host command to complete. See DIFFERENCES for details).

  The optional timeout parameter specifies a number of seconds to wait before failing the Wait action. The default is to wait indefinitely.

Wait(timeout, Seconds)
  Delays the script timeout seconds. Unlike the other forms of Wait, the timeout is not optional.

## File Transfer

The Transfer action implements IND$FILE file transfer. This action requires that the IND$FILE program be installed on the IBM host, and that the 3270 cursor be located in a field that will accept a TSO or VM/CMS command.

The Transfer action can be entered at the command prompt with no parameters, which will cause it to prompt interactively for the file names and options. It can also be invoked with parameters to define the entire transfer.

Because of the complexity and number of options for file transfer, the parameters to the Transfer action take the unique form of option=value, and can appear in any order. Note that if the value contains spaces (such as a VM/CMS file name), then the entire parameter must be quoted, e.g., "HostFile=xxx foo a". The options are:

Option | Required? | Default | Other Values
Direction | No | receive | send
HostFile | Yes |  |
LocalFile | Yes |  |
Host | No | tso | vm, cics
Mode | No | ascii | binary
Cr | No | remove | add, keep
Remap | No | yes | no
Exist | No | keep | replace, append
Recfm | No |  | fixed, variable, undefined
Lrecl | No |  |
Blksize | No |  |
Allocation | No |  | tracks, cylinders, avblock
PrimarySpace | Sometimes |  |
SecondarySpace | No |  |
Avblock | Sometimes |  |
BufferSize | No | 4096 |

The option details are as follows.

Direction
  send to send a file to the host, receive to receive a file from the host.
HostFile
  The name of the file on the host.
LocalFile
  The name of the file on the local workstation.
Host
  The type of host (which dictates the form of the IND$FILE command): tso (the default), vm or cics.
Mode
  Use ascii (the default) for a text file, which will be translated between EBCDIC and ASCII as necessary. Use binary for non-text files.
Cr
  Controls how Newline characters are handled when transferring Mode=ascii files. remove (the default) strips Newline characters in local files before transferring them to the host. add adds Newline characters to each host file record before transferring it to the local workstation. keep preserves Newline characters when transferring a local file to the host.
Remap
  Controls text translation for Mode=ascii files. The value yes (the default) causes wc3270 to remap the text to ensure maximum compatibility between the workstation's character set and encoding and the host's EBCDIC code page. The value no causes wc3270 to pass the text to or from the host as-is, leaving all translation to the IND$FILE program on the host.
Exist
  Controls what happens when the destination file already exists. keep (the default) preserves the file, causing the Transfer action to fail. replace overwrites the destination file with the source file. append appends the source file to the destination file.
Recfm
  Controls the record format of files created on the host. (TSO and VM hosts only.) fixed creates a file with fixed-length records. variable creates a file with variable-length records. undefined creates a file with undefined-length records (TSO hosts only). The Lrecl option controls the record length or maximum record length for Recfm=fixed and Recfm=variable files, respectively.
Lrecl
  Specifies the record length (or maximum record length) for files created on the host. (TSO and VM hosts only.)
Blksize
  Specifies the block size for files created on the host. (TSO and VM hosts only.)
Allocation
  Specifies the units for the PrimarySpace and SecondarySpace options: tracks, cylinders or avblock. (TSO hosts only.)
PrimarySpace
  Primary allocation for a file. The units are given by the Allocation option. Required when the Allocation is specified as something other than default. (TSO hosts only.)
SecondarySpace
  Secondary allocation for a file. The units are given by the Allocation option. (TSO hosts only.)
Avblock
  Average block size, required when Allocation specifies avblock. (TSO hosts only.)
BufferSize
  Buffer size for DFT-mode transfers. Can range from 256 to 32768. Larger values give better performance, but some hosts may not be able to support them.
WindowsCodePage
  Overrides the workstation code page used for ASCII file transfers. By default, the system ANSI code page is used.

There are also resources that control the default values for each of the file transfer parameters. These resources have the same names as the Transfer keywords, but with ft prepended. E.g., the default for the Mode keyword is the wc3270.ftMode resource.

## See Also

expect(1)
perl(1)
ksh(1)
x3270if(1)
wc3270(1)
ws3270(1)

## Version

Version 3.6ga5

This HTML document and the accompanying troff document were generated with a set of write-only m4 macros and the powerful vi editor.
Last modified 10 February 2018.