# Key Table: HandyTech Braille Wave

- Help Screen Version

Contents

- Default Bindings
  - Special Modes
  - Cursor Functions
  - Vertical Navigation
  - Horizontal Navigation
  - Clipboard Functions
  - Configuration Functions
  - Menu Operations
  - Special Functions
- Braille Input Mode
  - Special Modes
  - Keyboard Input

## Default Bindings

### Special Modes

- enter/leave help display: B8
- enter/leave command learn mode: B4+B5
- enter/leave preferences menu: B7+B1
- enter/leave status display:
  - B7+B6
  - Escape+Space+Return
- set display mode attributes/text: B6
- set screen image frozen/unfrozen: B8+B6
- describe character: B2+RoutingKey
- show current date and time: B2+B3+B5+B6
- switch to Default Bindings: B1+B8+Left
- switch to Braille Input Mode: B1+B8+Right

### Cursor Functions

- go to screen cursor: B1
- go back after cursor tracking: B3
- bring screen cursor to character: RoutingKey

### Vertical Navigation

- go up one line: B4
- go down one line: B5
- go to beginning of top line: B2
- go up to nearest line with different content: B8+B4
- go down to nearest line with different content: B8+B5
- go up to nearest line with different highlighting: B6+B4
- go down to nearest line with different highlighting: B6+B5
- go up to first line of paragraph: B1+B4
- go down to first line of next paragraph: B1+B5
- go up to previous command prompt: B2+B4
- go down to next command prompt: B2+B5
- go up several lines: B7+B4
- go down several lines: B7+B5
- go up to nearest line with less indent than character: Left+RoutingKey
- go down to nearest line with less indent than character: Right+RoutingKey

### Horizontal Navigation

- go backward one braille window: Left
- go forward one braille window: Right
- place left end of braille window at character: B1+RoutingKey

### Clipboard Functions

- start new clipboard at character: B4+RoutingKey
- append to clipboard from character: B3+RoutingKey
- linear copy to character: B6+RoutingKey
- rectangular copy to character: B5+RoutingKey
- copy characters to clipboard: RoutingKey+RoutingKey
- insert clipboard text after screen cursor: Left+Right
- search backward for clipboard text: B3+B4
- search forward for clipboard text: B3+B5

### Configuration Functions

- set text style 6-dot/8-dot: B7
- set skipping of lines with identical content on/off: B6+B1
- set skipping of blank braille windows on/off: B6+B2
- set sliding braille window on/off: B6+B3
- set track screen cursor on/off: B8+B1
- set screen cursor visibility on/off: B8+B2
- set attribute underlining on/off: B8+B3
- set alert tunes on/off: B8+B7

### Menu Operations

- restore preferences from disk: B7+B2
- save preferences to disk: B7+B3

### Special Functions

- remember current braille window position: B7+RoutingKey
- go to remembered braille window position: B8+RoutingKey

## Braille Input Mode

### Special Modes

- switch to Default Bindings: B1+B8+Left

### Keyboard Input

- braille keyboard dot7: B1
- braille keyboard dot3: B2
- braille keyboard dot2: B3
- braille keyboard dot1: B4
- braille keyboard control: Space
- braille keyboard dot4: B5
- braille keyboard meta: Return
- braille keyboard dot5: B6
- braille keyboard dot6: B7
- braille keyboard dot8: B8
- type braille dots [space]: Space
- backspace key: Space+B1
- enter key: Return