# Key Table: Baum (variokeys=yes)

- Help Screen Version

Contents

- Notes
- Default Bindings
  - Special Modes
  - Cursor Functions
  - Vertical Navigation
  - Horizontal Navigation
  - Clipboard Functions
  - Configuration Functions
  - Keyboard Input
  - Special Functions

## Notes

- RoutingKey refers to any of the keys immediately behind the braille cells.

## Default Bindings

### Special Modes

- enter/leave help display: Display1+Display2+Display5
- enter/leave preferences menu: Display1+Display4
- enter/leave status display: Display2+Display4
- set display mode attributes/text: Display1+Display2+Display3+Display6
- set screen image frozen/unfrozen: Display1+Display2+Display4
- describe character: Display3+RoutingKey

### Cursor Functions

- go to screen cursor: Display1+Display3
- bring screen cursor to character: RoutingKey

### Vertical Navigation

- go up one line: Display1
- go down one line: Display3
- go to beginning of top line: Display2+Display1
- go to beginning of bottom line: Display2+Display3
- go up to nearest line with less indent than character: Display2+Display1+RoutingKey
- go down to nearest line with less indent than character: Display2+Display3+RoutingKey
- go up to nearest line with different character: Display5+Display4+RoutingKey
- go down to nearest line with different character: Display5+Display6+RoutingKey

### Horizontal Navigation

- go backward one braille window: Display2
- go forward one braille window: Display5
- place left end of braille window at character: Display6+RoutingKey

### Clipboard Functions

- start new clipboard at character: Display1+RoutingKey
- append to clipboard from character: Display2+RoutingKey
- linear copy to character: Display4+RoutingKey
- rectangular copy to character: Display5+RoutingKey
- copy characters to clipboard: RoutingKey+RoutingKey
- append characters to clipboard: Display2+RoutingKey+RoutingKey

### Configuration Functions

- set track screen cursor on/off: Display2+Display3+Display4+Display5
- set attribute underlining on/off: Display1+Display3+Display6

### Keyboard Input

- cursor-up key: Display4
- cursor-down key: Display6
- switch to specific virtual terminal: Display4+Display5+Display6+RoutingKey

### Special Functions

- remember current braille window position: Display1+Display3+RoutingKey
- go to remembered braille window position: Display4+Display6+RoutingKey