# Class CIM_RemoteReplicationCollection
extends CIM_ConnectivityCollection

A RemoteReplicationCollection collects all paths (for example, ProtocolEndpoints) that provide access to a remote system for replication operations.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Collection
|
+--CIM_SystemSpecificCollection
|
+--CIM_ConnectivityCollection
|
+--CIM_RemoteReplicationCollection

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A RemoteReplicationCollection collects all paths (for example, ProtocolEndpoints) that provide access to a remote system for replication operations.
Experimental | boolean | true
UMLPackagePath | string | CIM::Device::StorageServices
Version | string | 2.34.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Active | boolean | true
Description | string | Indicates that this RemoteReplicationCollection is currently active and allows replication traffic to/from remote elements.
Write | boolean | true
DeleteOnUnassociated | boolean | false
Description | string | The instance of RemoteReplicationCollection will be deleted when it is no longer associated with an access point.
Write | boolean | true
ElementName | string |
Description | string | A user-friendly name for the RemoteReplicationCollection.
Override | string | ElementName
Write | boolean | true
HardwareCompressionEnabled | boolean | false
Description | string | The property indicates if hardware compression is enabled -- the transmitted/received data is compressed by hardware.
Write | boolean | true
SoftwareCompressionEnabled | boolean | false
Description | string | The property indicates if software compression is enabled -- the transmitted/received data is compressed by sofware.
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ConnectivityStatus | uint16 | CIM_ConnectivityCollection
Description | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SystemSpecificCollection

## Class Methods