# Class CIM_IndicationService
extends CIM_Service

An IndicationService is a Service of the CIM Object Manager that is responsible for delivering indications to Indication Handlers.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_IndicationService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | An IndicationService is a Service of the CIM Object Manager that is responsible for delivering indications to Indication Handlers.
UMLPackagePath | string | CIM::Event
Version | string | 2.20.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DeliveryRetryAttempts | uint16 | 3
Description | string | Defines the number of retries that the indication service will try to deliver an indication to a particular listener destination. This does not effect the original delivery attempt, thus if set to 0, it will only try to deliver the indication once. Note that implementations may preset this setting and not allow this value to be modified.
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_IndicationService.DeliveryRetryInterval
DeliveryRetryInterval | uint32 | 30
Description | string | Defines the minimal time interval in seconds for the indication service to use before delivering an indication to a particular listener destination that previously failed. The implementation may take longer due to QoS or other processing. Note that implementations may preset this setting and not allow this value to be modified.
ModelCorrespondence | string | CIM_IndicationService.DeliveryRetryAttempts
PUnit | string | second
FilterCreationEnabled | boolean | false
Description | string | The FilterCreationEnabled property controls whether or not clients can create indication filters. If this value is set to false, only the indication filters that exist can be subscribed to. If this value is true clients may attempt to create filters. Note that implementations may preset this setting and not allow this value to be modified.
SubscriptionRemovalAction | uint16 |
Description | string | Defines the removal action for subscriptions that have two failed indication deliveries without any successful indication deliveries in between and the time between the failed deliveries exceeded the timeout defined in the SubscriptionRemovalTimeInterval property. "Remove" defines the subscription is to be removed. "Disable" indicates that subscription removal process isnot being enforced. "Ignore" indicates that the removal action is temporarily not enforced. implementations may preset this setting and not allow this value to be modified.
ModelCorrespondence | string | CIM_IndicationService.SubscriptionRemovalTimeInterval
ValueMap | string | 2, 3, 4, ..
Values | string | Remove, Disable, Ignore, DMTF Reserved
SubscriptionRemovalTimeInterval | uint32 |
Description | string | Minimum time between two failed indication deliveries without any successful indication deliveries in between before the SubscriptionRemovalPolicy goes into effect.
ModelCorrespondence | string | CIM_IndicationService.SubscriptionRemovalAction
PUnit | string | second

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service