# Class CIM_RAIDDiagnosticTest
extends CIM_DiagnosticTest

This class specializes CIM_DiagnosticTest to define the tests specific to RAID controllers.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_DiagnosticService
|
+--CIM_DiagnosticTest
|
+--CIM_RAIDDiagnosticTest

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class specializes CIM_DiagnosticTest to define the tests specific to RAID controllers.
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.30.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
OtherRAIDTestType | string |
Description | string | A string that describes the test when the RAIDTestType property is set to 1 ("Other"). This property must be set to null when RAIDTestType is any value other than 1.
ModelCorrespondence | string | CIM_RAIDDiagnosticTest.RAIDTestType
RAIDTestType | uint16 |
Description | string | The descriptions for each RAID controller test type are below: * "Battery" (value=2) is specified for the test that verifies the presence and charge of the battery. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Internal Registers" (value=3) is specified for the test that verifies that read and write operations can be performed on the internal registers . CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Controller Status" (value=4) is specified for the test that verifies the overall status of the RAID controller. CIM_DiagnosticTest.TestTypes shall be set to Health Check (value=4). * "Controller Self-Test" (value=5) is specified for the test that performs an extended set of vendor-specific tests to verify that the RAID controller is operating properly. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Cache Memory" (value=6) is specified for the test that verifies that the cache memory is operating properly. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Hard Drive Status" (value=7) is specified for the test that returns information about the relative health of the disk drive based on internal analysis of failure statistics. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Hard Drive Self-Test" (value=8) is specified for the test that performs a set of vendor-specific tests to verify that the disk is operating properly. CIM_DiagnosticTest.TestTypes shall be set to Health Check (value=4). * "Hard Drive Random Read" (value=9) is specified for the test that performs a read operation from disk sectors in random order, but limited to a specific region of the disk. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * "Hard Drive Grown Defect" (value=10) is specified for the test that retrieves statistics collected by the disk driver regarding its sector remap mechanism such as the number of remapped sectors. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2).
ModelCorrespondence | string | CIM_RAIDDiagnosticTest.OtherRAIDTestType
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, .., 0x8000..
Values | string | Unknown, Other, Battery, Internal Registers, Controller Status, Controller Self-Test, Cache Memory, Hard Drive Status, Hard Drive Self-Test, Hard Drive Random Read, Hard Drive Grown Defect, Vendor Reserved, DMTF Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsInUse | boolean | CIM_DiagnosticTest
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCharacteristicDescription | string | CIM_DiagnosticTest
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Characteristics | uint16[] | CIM_DiagnosticTest
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherCharacteristicsDescriptions | string[] | CIM_DiagnosticTest
OtherTestTypesDescriptions | string[] | CIM_DiagnosticTest
ResourcesUsed | uint16[] | CIM_DiagnosticTest
StatusDescriptions | string[] | CIM_ManagedSystemElement
TestTypes | uint16[] | CIM_DiagnosticTest

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
ClearResults | uint32 | CIM_DiagnosticTest
DiscontinueTest | uint32 | CIM_DiagnosticTest
RequestStateChange | uint32 | CIM_EnabledLogicalElement
RunDiagnostic | uint32 | CIM_DiagnosticService
RunDiagnosticService | uint32 | CIM_DiagnosticService
RunTest | uint32 | CIM_DiagnosticTest
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service