# Class CIM_AccessControlService
extends CIM_SecurityService

CIM_AccessControlService represents an access control service that is desployed on a software module or a hardware device, and controls access to protected resources on a managed system based on specified access control policies. The CIM_AccessControlService extends the CIM_SecurityService. The CIM_AccessControlSerivece may be associated with CIM_AuthorizationService through the CIM_ServiceServiceDependency.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_SecurityService
|
+--CIM_AccessControlService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_AccessControlService represents an access control service that is desployed on a software module or a hardware device, and controls access to protected resources on a managed system based on specified access control policies. The CIM_AccessControlService extends the CIM_SecurityService. The CIM_AccessControlSerivece may be associated with CIM_AuthorizationService through the CIM_ServiceServiceDependency.
Experimental | boolean | true
UMLPackagePath | string | CIM::Policy
Version | string | 2.28.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ImplementationType | uint16 |
Description | string | ImplementationType specifies the type of access control service implementation on a managed system. A value of "OS module" indicates the service is implemented as an access control module embedded in the operating system. A value of "Application" indicates the service is implemented as an application software module installed on the managed system. A value of "Hardware" indicates the service is implemented as a device of the managed system.
Experimental | boolean | true
ValueMap | string | 1, 2, 3, .., 0x8000..
Values | string | OS module, Application, Hardware, DMTF Reserved, Vendor Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service