# Class CIM_MPLSTunnelStats
extends CIM_StatisticalData

This class represents the statistics for an MPLSTunnel. The statistics are associated to the tunnel using the relationship, CIM_ElementStatisticalData.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_MPLSTunnelStats

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class represents the statistics for an MPLSTunnel. The statistics are associated to the tunnel using the relationship, CIM_ElementStatisticalData.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::MPLS
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
TunnelInstanceUpTime | uint32 |
Counter | boolean | true
Description | string | This value identifies the total time for which the the OperationalStatus of the tunnel is up (i.e., "OK"=2).
MappingStrings | string | MIB.IETF|MPLS-TE-MIB.MPLSTunnelInstanceUpTime
PUnit | string | second * 10^-2
Units | string | Hundredths of a Second
TunnelLastPathChange | uint32 |
Counter | boolean | true
Description | string | Specifies the time since the last path change for this tunnel.
MappingStrings | string | MIB.IETF|MPLS-TE-MIB.MPLSTunnelLastPathChange
MaxValue | sint64 | 4294967295
PUnit | string | second * 10^-2
Units | string | Hundredths of a Second
TunnelPathChanges | uint32 |
Counter | boolean | true
Description | string | Specifies the number of times the paths have changed for this tunnel.
MappingStrings | string | MIB.IETF|MPLS-TE-MIB.MPLSTunnelPathChanges
TunnelPrimaryTimeUp | uint32 |
Counter | boolean | true
Description | string | Specifies the total time the primary tunnel has been active. A primary tunnel is found/designated in situations where multiple tunnels exist - i.e., when parallel or backup tunnels are defined.
MappingStrings | string | MIB.IETF|MPLS-TE-MIB.MPLSTunnelPrimaryTimeUp
MaxValue | sint64 | 4294967295
PUnit | string | second * 10^-2
Units | string | Hundredths of a Second
TunnelStateTransitions | uint32 |
Counter | boolean | true
Description | string | Specifies the number of times the operational status of this tunnel has changed.
MappingStrings | string | MIB.IETF|MPLS-TE-MIB.MPLSTunnelStateTransitions

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_StatisticalData
RateIntervalEndTime | datetime | CIM_StatisticalData
RateIntervalStartTime | datetime | CIM_StatisticalData
SampleInterval | datetime | CIM_StatisticalData
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData