# Class CIM_SystemSpecificCollection
extends CIM_Collection

SystemSpecificCollection represents the general concept of a collection that is scoped (or contained) by a System. It represents a Collection that has meaning only in the context of a System, a Collection whose elements are restricted by the definition of the System, or both of these types of Collections. This meaning is explicitly described by the (required) association, HostedCollection. An example of a SystemSpecificCollection is a Fibre Channel zone that collects network ports, port groupings, and aliases (as required by a customer) in the context of an AdminDomain. The Collection is not a part of the domain, but merely an arbitrary grouping of the devices and other Collections in the domain. In other words, the context of the Collection is restricted to the domain, and its members are also limited by the domain.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Collection
|
+--CIM_SystemSpecificCollection

## Direct Known Subclasses

CIM_AllocatedResources
CIM_BlockStatisticsManifestCollection
CIM_ConnectivityCollection
CIM_DeviceSet
CIM_FailoverStorageExtentsCollection
CIM_FileSystemStatisticsManifestCollection
CIM_LogicalPortGroup
CIM_MaskingGroup
CIM_NamedAddressCollection
CIM_OperationalPowerManifestCollection
CIM_PolicyRoleCollection
CIM_RangeOfIPAddresses
CIM_RedundancySet
CIM_RemoteResources
CIM_ReplicationGroup
CIM_SCSITargetPortGroup
CIM_StatisticsCollection
CIM_StorageResourceLoadGroup
CIM_StorageTier
CIM_TargetPortGroup
CIM_VirtualRoutingAndForwardingTable

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SystemSpecificCollection represents the general concept of a collection that is scoped (or contained) by a System. It represents a Collection that has meaning only in the context of a System, a Collection whose elements are restricted by the definition of the System, or both of these types of Collections. This meaning is explicitly described by the (required) association, HostedCollection. An example of a SystemSpecificCollection is a Fibre Channel zone that collects network ports, port groupings, and aliases (as required by a customer) in the context of an AdminDomain. The Collection is not a part of the domain, but merely an arbitrary grouping of the devices and other Collections in the domain. In other words, the context of the Collection is restricted to the domain, and its members are also limited by the domain.
UMLPackagePath | string | CIM::Core::Collection
Version | string | 2.19.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
InstanceID | string |
Description | string | Within the scope of the instantiating Namespace, InstanceID opaquely and uniquely identifies an instance of this class. To ensure uniqueness within the NameSpace, the value of InstanceID should be constructed using the following 'preferred' algorithm: <OrgID>:<LocalID> Where <OrgID> and <LocalID> are separated by a colon ':', and where <OrgID> must include a unique name. It can be a copyrighted, trademarked, or otherwise unique name that is owned by the business entity that is creating or defining the InstanceID. Or, it could be a registered ID that is assigned to the business entity by a recognized global authority.(This requirement is similar to the <Schema Name>_<Class Name> structure of Schema class names.) In addition, to ensure uniqueness <OrgID> must not contain a colon (':'). When using this algorithm, the first colon to appear in InstanceID must appear between <OrgID> and <LocalID>. <LocalID> is chosen by the business entity and should not be re-used to identify different underlying (real-world) elements. If the above 'preferred' algorithm is not used, the defining entity must ensure that the resulting InstanceID is not re-used as any of InstanceIDs produced by this or other providers for the NameSpace of this instance. For DMTF-defined instances, the 'preferred' algorithm must be used with the <OrgID> set to 'CIM'.
Key | boolean | true
Override | string | InstanceID

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement

## Class Methods