# Class CIM_CPUDiagnosticTest
extends CIM_DiagnosticTest

This class specializes CIM_DiagnosticTest to define the tests specific to CPUs.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_DiagnosticService
|
+--CIM_DiagnosticTest
|
+--CIM_CPUDiagnosticTest

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class specializes CIM_DiagnosticTest to define the tests specific to CPUs.
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.28.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CPUTestType | uint16 |
Description | string | The descriptions for each CPU test type are below: * "Register" (value=2) is specified for the testshat verify access to all registers. CIM_DiagnosticTest.TestTypes shall be set to (value=2). * Instruction (value=3) is specified for the tests that verify the functionality of the general CPU instruction. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * FPU Instruction (value=3) is specified for the tests that verify the functionality of the FPU instructions. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). Mixed Instruction Width (value=5) is specified for the tests that verify the ability of the CPU to run mix of 32-bit and 64-bit instructions. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * Paging and Protected Mode Entry (value=6) is specified for the tests that verify the functionality of the page tables that are used to map virtual addresses to physical locations in memory. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). Virtual Machine (value=7) is specified for the tests that verify the functionality of the VM instructions and the ability to intercept VM privileged instructions. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * Exceptions (value=8) is specified for the tests that verify the functionality of the CPU exception handlers. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * Machine Check (value=9) is specified for the tests that verify the functionality of the CPU Machine Check mechanism. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * Power Management (value=10) is specified for the tests that verify the functionality of the power management features of the CPU. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * Speed (value=11) is specified for the tests that verify that the CPU can run at various clock speeds. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * Voltage (value=12) is specified for the tests that verify the the ability of the CPU to operate at various voltages. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * Stress (value=13) is specified for the tests that verify the proper operation of the CPU when running under heavy load. CIM_DiagnosticTest.TestTypes shall be set to Stress (value=4). * Cache (value=14) is specified for the tests that verify the accessibility of all available caches. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2). * IPC (value=15) is specified for the tests that verify the functionality of the inter process communication mechanism between various components of the CPU. CIM_DiagnosticTest.TestTypes shall be set to Functional (value=2).
ModelCorrespondence | string | CIM_CPUDiagnosticTest.OtherCPUTestTypeDescription, CIM_DiagnosticTest.TestTypes
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, .., 0x8000..
Values | string | Unknown, Other, Register, Instruction, FPU Instruction, Mixed Instruction Width, Paging and Protected Mode Entry, Virtual Machine, Exceptions, Status, Power Management, Speed, Voltage, Stress, Cache, IPC, DMTF Reserved, Vendor Reserved
OtherCPUTestTypeDescription | string |
Description | string | A string that describes the test when the CPUTestType property is set to 1 ("Other"). This property must be set to null when CPUTestType is any value other than 1.
ModelCorrespondence | string | CIM_CPUDiagnosticTest.CPUTestType

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsInUse | boolean | CIM_DiagnosticTest
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCharacteristicDescription | string | CIM_DiagnosticTest
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Characteristics | uint16[] | CIM_DiagnosticTest
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherCharacteristicsDescriptions | string[] | CIM_DiagnosticTest
OtherTestTypesDescriptions | string[] | CIM_DiagnosticTest
ResourcesUsed | uint16[] | CIM_DiagnosticTest
StatusDescriptions | string[] | CIM_ManagedSystemElement
TestTypes | uint16[] | CIM_DiagnosticTest

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
ClearResults | uint32 | CIM_DiagnosticTest
DiscontinueTest | uint32 | CIM_DiagnosticTest
RequestStateChange | uint32 | CIM_EnabledLogicalElement
RunDiagnostic | uint32 | CIM_DiagnosticService
RunDiagnosticService | uint32 | CIM_DiagnosticService
RunTest | uint32 | CIM_DiagnosticTest
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service