# Class CIM_ImagingWorkStatisticalData
extends CIM_ImagingStatisticalData

This class defines work counters (for accounting and billing) ImagingStatisticalData associated with an imaging system (e.g., ComputerSystem), imaging service (e.g., PrintService), imaging device (e.g., Printer), imaging job (e.g., PrintJob), or any other imaging element. See: Section 4 Overview in PWG Counter MIB v2 (PWG 5106.3).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_ImagingStatisticalData
|
+--CIM_ImagingWorkStatisticalData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class defines work counters (for accounting and billing) ImagingStatisticalData associated with an imaging system (e.g., ComputerSystem), imaging service (e.g., PrintService), imaging device (e.g., Printer), imaging job (e.g., PrintJob), or any other imaging element. See: Section 4 Overview in PWG Counter MIB v2 (PWG 5106.3).
Experimental | boolean | true
UMLPackagePath | string | CIM::Core::Statistics
Version | string | 2.20.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BlankImpressions | uint32 |
Description | string | Blank hardcopy impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImpressionBlankImps
BlankSheets | uint32 |
Description | string | Blank media sheets consumed by this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icSheetBlankSheets
BlankTwoSidedImpressions | uint32 |
Description | string | Blank two-sided impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTwoSidedBlankImps
FullColorImages | uint32 |
Description | string | Full color images processed by this managed element (e.g., Scanner).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImageFullColorImages
FullColorImpressions | uint32 |
Description | string | Full color hardcopy impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImpressionFullColorImps
FullColorSheets | uint32 |
Description | string | Full color media sheets consumed by this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icSheetFullColorSheets
FullColorTwoSidedImpressions | uint32 |
Description | string | Full color two-sided impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTwoSidedFullColorImps
HighlightColorImpressions | uint32 |
Description | string | Highlight color hardcopy impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImpressionHighlightColorImps
HighlightColorSheets | uint32 |
Description | string | Highlight color media sheets consumed by this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icSheetHighlightColorSheets
HighlightColorTwoSidedImpressions | uint32 |
Description | string | Highlight color two-sided impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTwoSidedHighlightColorImps
MonochromeImages | uint32 |
Description | string | Monochrome images processed by this managed element (e.g., Scanner).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImageMonochromeImages
MonochromeImpressions | uint32 |
Description | string | Monochrome hardcopy impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImpressionMonochromeImps
MonochromeSheets | uint32 |
Description | string | Monochrome media sheets consumed by this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icSheetMonochromeSheets
MonochromeTwoSidedImpressions | uint32 |
Description | string | Monochrome two-sided impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTwoSidedMonochromeImps
OtherWorkType | string |
Description | string | A free-form string that describes the work type when the the value of the WorkType property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_ImagingWorkStatisticalData.WorkType
TotalImages | uint32 |
Description | string | Total images processed by this managed element (e.g., Scanner).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImageTotalImages
TotalImpressions | uint32 |
Description | string | Total hardcopy impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImpressionTotalImps
TotalSheets | uint32 |
Description | string | Total media sheets consumed by this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icSheetTotalSheets
TotalTwoSidedImpressions | uint32 |
Description | string | Total two-sided impressions from this managed element (e.g., Printer or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTwoSidedTotalImps
WorkType | uint16 |
Description | string | Work type of this instance of ImagingWorkStatisticalData. 1 (Other) means vendor-specific work type and should not be used (to avoid interoperability problems). 2 (Unknown) means unknown work type and should not be be used (to avoid amgiguity in accounting applications). 3 (WorkTotals) means total counters across imaging element execution modes (both user and maintenance). 4 (Datastream) means user datastream work (both control and content) while this imaging element is in user mode. 5 (Auxiliary) means hardcopy auxiliary work (e.g., banner sheets) while this imaging element is in user mode. 6 (Waste) means hardcopy waste work (e.g., process runout or paper jams) while this imaging element is in user mode. 7 (Maintenance) means maintenance work (e.g., calibration) while this imaging element is in maintenance mode.
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImageWorkType, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImpressionWorkType, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTwoSidedWorkType, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icSheetWorkType
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Other, Unknown, WorkTotals, Datastream, Auxiliary, Waste, Maintenance, DMTF Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_StatisticalData
OtherPersistenceType | string | CIM_ImagingStatisticalData
PersistenceType | uint16 | CIM_ImagingStatisticalData
RateIntervalEndTime | datetime | CIM_StatisticalData
RateIntervalStartTime | datetime | CIM_StatisticalData
SampleInterval | datetime | CIM_StatisticalData
SNMPKeyId | uint32 | CIM_ImagingStatisticalData
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData