# NAME

rrdgraph_rpn - About RPN Math in rrdtool graph

# SYNOPSIS

RPN expression:=vname|operator|value[,RPN expression]

# DESCRIPTION

If you have ever used a traditional HP calculator you already know RPN (Reverse Polish Notation). The idea behind RPN is that you have a stack and push your data onto this stack. Whenever you execute an operation, it takes as many elements from the stack as needed. Pushing is done implicitly, so whenever you specify a number or a variable, it gets pushed onto the stack automatically.

At the end of the calculation there should be one and only one value left on the stack. This is the outcome of the function and this is what is put into the vname. For CDEF instructions, the stack is processed for each data point on the graph. VDEF instructions work on an entire data set in one run. Note, that currently VDEF instructions only support a limited list of functions.

Example: `VDEF:maximum=mydata,MAXIMUM`

This will set variable "maximum" which you now can use in the rest of your RRD script.

Example: `CDEF:mydatabits=mydata,8,*`

This means: push variable mydata, push the number 8, execute the operator *. The operator needs two elements and uses those to return one value. This value is then stored in mydatabits. As you may have guessed, this instruction means nothing more than mydatabits = mydata * 8. The real power of RPN lies in the fact that it is always clear in which order to process the input. For expressions like `a = b + 3 * 5` you need to multiply 3 with 5 first before you add b to get a. However, with parentheses you could change this order: `a = (b + 3) * 5`. In RPN, you would do `a = b, 3, +, 5, *` without the need for parentheses.

# OPERATORS

Boolean operators

  LT, LE, GT, GE, EQ, NE

  Less than, Less or equal, Greater than, Greater or equal, Equal, Not equal all pop two elements from the stack, compare them for the selected condition and return 1 for true or 0 for false. Comparing an unknown or an infinite value will result in unknown returned ... which will also be treated as false by the IF call.

  UN, ISINF

  Pop one element from the stack, compare this to unknown respectively to positive or negative infinity. Returns 1 for true or 0 for false.

  then,else,condition,IF

  Pops three elements from the stack. If the element popped last is 0 (false), the value popped first is pushed back onto the stack, otherwise the value popped second is pushed back. This does, indeed, mean that any value other than 0 is considered to be true.

  Example: `A,B,C,IF` should be read as `if (A) then (B) else (C)`

Comparing values

  MIN, MAX

  Pops two elements from the stack and returns the smaller or larger, respectively. Note that infinite is larger than anything else. If one of the input numbers is unknown then the result of the operation will be unknown too.

  MINNAN, MAXNAN

  NAN-safe version of MIN and MAX. If one of the input numbers is unknown then the result of the operation will be the other one. If both are unknown, then the result of the operation is unknown.

  lower-limit,upper-limit,LIMIT

  Pops two elements from the stack and uses them to define a range. Then it pops another element and if it falls inside the range, it is pushed back. If not, an unknown is pushed.

  The range defined includes the two boundaries (so: a number equal to one of the boundaries will be pushed back). If any of the three numbers involved is either unknown or infinite this function will always return an unknown

  Example: `CDEF:a=alpha,0,100,LIMIT` will return unknown if alpha is lower than 0 or if it is higher than 100.

Arithmetics

  +, -, *, /, %

  Add, subtract, multiply, divide, modulo

  ADDNAN

  NAN-safe addition. If one parameter is NAN/UNKNOWN it'll be treated as zero. If both parameters are NAN/UNKNOWN, NAN/UNKNOWN will be returned.

  value,power,POW

  Raise value to the power of power.

  SIN, COS, LOG, EXP, SQRT

  Sine and cosine (input in radians), log and exp (natural logarithm), square root.

  ATAN

  Arctangent (output in radians).

  ATAN2

  Arctangent of y,x components (output in radians). This pops one element from the stack, the x (cosine) component, and then a second, which is the y (sine) component. It then pushes the arctangent of their ratio, resolving the ambiguity between quadrants.

  Example: `CDEF:angle=Y,X,ATAN2,RAD2DEG` will convert `X,Y` components into an angle in degrees.

  FLOOR, CEIL

  Round down or up to the nearest integer.

  DEG2RAD, RAD2DEG

  Convert angle in degrees to radians, or radians to degrees.

  ABS

  Take the absolute value.

Set Operations

  count,SORT

  Pop one element from the stack. This is the count of items to be sorted. The top count of the remaining elements are then sorted from the smallest to the largest, in place on the stack.

         4,3,22.1,1,4,SORT -> 1,3,4,22.1

  count,REV

  Reverse the number

  Example: `CDEF:x=v1,v2,v3,v4,v5,v6,6,SORT,POP,5,REV,POP,+,+,+,4,/` will compute the average of the values v1 to v6 after removing the smallest and largest.

  count,AVG

  Pop one element (count) from the stack. Now pop count elements and build the average, ignoring all UNKNOWN values in the process.

  Example: `CDEF:x=a,b,c,d,4,AVG`

  count,SMIN and count,SMAX

  Pop one element (count) from the stack. Now pop count elements and push the minimum/maximum back onto the stack.

  Example: `CDEF:x=a,b,c,d,4,AVG`

  count,MEDIAN

  pop one element (count) from the stack. Now pop count elements and find the median, ignoring all UNKNOWN values in the process. If there are an even number of non-UNKNOWN values, the average of the middle two will be pushed on the stack.

  Example: `CDEF:x=a,b,c,d,4,MEDIAN`

  count,STDEV

  pop one element (count) from the stack. Now pop count elements and calculate the standard deviation over these values (ignoring any NAN values). Push the result back on to the stack.

  Example: `CDEF:x=a,b,c,d,4,STDEV`

  percent,count,PERCENT

  pop two elements (count,percent) from the stack. Now pop count element, order them by size (while the smalles elements are -INF, the largest are INF and NaN is larger than -INF but smaller than anything else. No pick the element from the ordered list where percent of the elements are equal then the one picked. Push the result back on to the stack.

  Example: `CDEF:x=a,b,c,d,95,4,PERCENT`

  count,TREND, TRENDNAN

  Create a "sliding window" average of another data series.

  Usage: CDEF:smoothed=x,1800,TREND

  This will create a half-hour (1800 second) sliding window average of x. The average is essentially computed as shown here:

                       +---!---!---!---!---!---!---!---!--->
                                                           now
                             delay     t0
                       <--------------->
                               delay       t1
                           <--------------->
                                    delay      t2
                               <--------------->

           Value at sample (t0) will be the average between (t0-delay) and (t0)
           Value at sample (t1) will be the average between (t1-delay) and (t1)
           Value at sample (t2) will be the average between (t2-delay) and (t2)

  TRENDNAN is - in contrast to TREND - NAN-safe. If you use TREND and one source value is NAN the complete sliding window is affected. The TRENDNAN operation ignores all NAN-values in a sliding window and computes the average of the remaining values.

  PREDICT, PREDICTSIGMA, PREDICTPERC

  Create a "sliding window" average/sigma/percentil of another data series, that also shifts the data series by given amounts of time as well

  Usage - explicit stating shifts: `CDEF:predict=<shift n>,...,<shift 1>,n,<window>,x,PREDICT` `CDEF:sigma=<shift n>,...,<shift 1>,n,<window>,x,PREDICTSIGMA` `CDEF:perc=<shift n>,...,<shift 1>,n,<window>,<percentil>,x,PREDICTPERC`

  Usage - shifts defined as a base shift and a number of time this is applied `CDEF:predict=<shift multiplier>,-n,<window>,x,PREDICT` `CDEF:sigma=<shift multiplier>,-n,<window>,x,PREDICTSIGMA` `CDEF:sigma=<shift multiplier>,-n,<window>,<percentil>,x,PREDICTPERC`

  Example: CDEF:predict=172800,86400,2,1800,x,PREDICT

  This will create a half-hour (1800 second) sliding window average/sigma of x, that average is essentially computed as shown here:

       +---!---!---!---!---!---!---!---!---!---!---!---!---!---!---!---!---!--->
                                                                           now
                                                        shift 1        t0
                                               <----------------------->
                                     window
                               <--------------->
                                             shift 2
                       <----------------------------------------------->
             window
       <--------------->
                                                            shift 1        t1
                                                   <----------------------->
                                         window
                                   <--------------->
                                                  shift 2
                           <----------------------------------------------->
                 window
           <--------------->

       Value at sample (t0) will be the average between (t0-shift1-window) and (t0-shift1)
                                            and between (t0-shift2-window) and (t0-shift2)
       Value at sample (t1) will be the average between (t1-shift1-window) and (t1-shift1)
                                            and between (t1-shift2-window) and (t1-shift2)

  The function is by design NAN-safe. This also allows for extrapolation into the future (say a few days) - you may need to define the data series whit the optional start= parameter, so that the source data series has enough data to provide prediction also at the beginning of a graph...

  The percentile can be between [-100:+100]. The positive percentiles interpolates between values while the negative will take the closest.

  Example: you run 7 shifts with a window of 1800seconds. Assuming that the rrd-file has a step size of 300 seconds this means we have to do the percentile calculation based on a max of 42 distinct values (less if you got NAN). that means that in the best case you get a step rate between values of 2.4 percent. so if you ask for the 99th percentile, then you would need to look at the 41.59th value. As we only have integers, either the 41st or the 42nd value.

  With the positive percentile a linear interpolation between the 2 values is done to get the effective value.

  The negative returns the closest value distance wise - so in the above case 42nd value, which is effectively returning the Percentile100 or the max of the previous 7 days in the window.

  Here an example, that will create a 10 day graph that also shows the prediction 3 days into the future with its uncertainty value (as defined by avg+-4*sigma) This also shows if the prediction is exceeded at a certain point.

          rrdtool graph image.png --imgformat=PNG \
          --start=-7days --end=+3days --width=1000 --height=200 --alt-autoscale-max \
          DEF:value=value.rrd:value:AVERAGE:start=-14days \
          LINE1:value#ff0000:value \
          CDEF:predict=86400,-7,1800,value,PREDICT \
          CDEF:sigma=86400,-7,1800,value,PREDICTSIGMA \
          CDEF:upper=predict,sigma,3,*,+ \
          CDEF:lower=predict,sigma,3,*,- \
          LINE1:predict#00ff00:prediction \
          LINE1:upper#0000ff:upper\ certainty\ limit \
          LINE1:lower#0000ff:lower\ certainty\ limit \
          CDEF:exceeds=value,UN,0,value,lower,upper,LIMIT,UN,IF \
          TICK:exceeds#aa000080:1 \
          CDEF:perc95=86400,-7,1800,95,value,PREDICTPERC \
          LINE1:perc95#ffff00:95th_percentile

  Note: Experience has shown that a factor between 3 and 5 to scale sigma is a good discriminator to detect abnormal behavior. This obviously depends also on the type of data and how "noisy" the data series is.

  Also Note the explicit use of start= in the CDEF - this is necessary to load all the necessary data (even if it is not displayed)

  This prediction can only be used for short term extrapolations - say a few days into the future.

Special values

  UNKN

  Pushes an unknown value on the stack

  INF, NEGINF

  Pushes a positive or negative infinite value on the stack. When such a value is graphed, it appears at the top or bottom of the graph, no matter what the actual value on the y-axis is.

  PREV

  Pushes an unknown value if this is the first value of a data set or otherwise the result of this CDEF at the previous time step. This allows you to do calculations across the data. This function cannot be used in VDEF instructions.

  PREV(vname)

  Pushes an unknown value if this is the first value of a data set or otherwise the result of the vname variable at the previous time step. This allows you to do calculations across the data. This function cannot be used in VDEF instructions.

  COUNT

  Pushes the number 1 if this is the first value of the data set, the number 2 if it is the second, and so on. This special value allows you to make calculations based on the position of the value within the data set. This function cannot be used in VDEF instructions.

Time

  Time inside RRDtool is measured in seconds since the epoch. The epoch is defined to be `Thu Jan 1 00:00:00 UTC 1970`.

  NOW

  Pushes the current time on the stack.

  STEPWIDTH

  The with of the current step in seconds. You can use this to go back from rate based presentations to absolute numbers

        CDEF:abs=rate,STEPWIDTH,*,PREV,ADDNAN

  NEWDAY,NEWWEEK,NEWMONTH,NEWYEAR

  These three operators will return 1.0 whenever a step is the first of the given period. The periods are determined according to the local timezone AND the `LC_TIME` settings.

        CDEF:mtotal=rate,STEPWIDTH,*,NEWMONTH,0,PREV,IF,ADDNAN

  TIME

  Pushes the time the currently processed value was taken at onto the stack.

  LTIME

  Takes the time as defined by TIME, applies the time zone offset valid at that time including daylight saving time if your OS supports it, and pushes the result on the stack. There is an elaborate example in the examples section below on how to use this.

Processing the stack directly

  DUP, POP, EXC

  Duplicate the top element, remove the top element, exchange the two top elements.

  DEPTH

  pushes the current depth of the stack onto the stack

       a,b,DEPTH -> a,b,2

  n,COPY

  push a copy of the top n elements onto the stack

       a,b,c,d,2,COPY => a,b,c,d,c,d

  n,INDEX

  push the nth element onto the stack.

       a,b,c,d,3,INDEX -> a,b,c,d,b

  n,m,ROLL

  rotate the top n elements of the stack by m

       a,b,c,d,3,1,ROLL => a,d,b,c
       a,b,c,d,3,-1,ROLL => a,c,d,b

# VARIABLES

These operators work only on VDEF statements. Note that currently ONLY these work for VDEF.

MAXIMUM, MINIMUM, AVERAGE

  Return the corresponding value, MAXIMUM and MINIMUM also return the first occurrence of that value in the time component.

  Example: `VDEF:avg=mydata,AVERAGE`

STDEV

  Returns the standard deviation of the values.

  Example: `VDEF:stdev=mydata,STDEV`

LAST, FIRST

  Return the last/first non-nan or infinite value for the selected data stream, including its timestamp.

  Example: `VDEF:first=mydata,FIRST`

TOTAL

  Returns the rate from each defined time slot multiplied with the step size. This can, for instance, return total bytes transferred when you have logged bytes per second. The time component returns the number of seconds.

  Example: `VDEF:total=mydata,TOTAL`

PERCENT, PERCENTNAN

  This should follow a DEF or CDEF vname. The vname is popped, another number is popped which is a certain percentage (0..100). The data set is then sorted and the value returned is chosen such that percentage percent of the values is lower or equal than the result. For PERCENTNAN Unknown values are ignored, but for PERCENT Unknown values are considered lower than any finite number for this purpose so if this operator returns an unknown you have quite a lot of them in your data. Infinite numbers are lesser, or more, than the finite numbers and are always more than the Unknown numbers. (NaN < -INF < finite values < INF)

  Example: `VDEF:perc95=mydata,95,PERCENT` `VDEF:percnan95=mydata,95,PERCENTNAN`

LSLSLOPE, LSLINT, LSLCORREL

  Return the parameters for a Least Squares Line (y = mx +b) which approximate the provided dataset. LSLSLOPE is the slope (m) of the line related to the COUNT position of the data. LSLINT is the y-intercept (b), which happens also to be the first data point on the graph. LSLCORREL is the Correlation Coefficient (also know as Pearson's Product Moment Correlation Coefficient). It will range from 0 to +/-1 and represents the quality of fit for the approximation.

  Example: `VDEF:slope=mydata,LSLSLOPE`

# SEE ALSO

rrdgraph gives an overview of how rrdtool graph works. rrdgraph_data describes DEF,CDEF and VDEF in detail. rrdgraph_rpn describes the RPN language used in the ?DEF statements. rrdgraph_graph page describes all of the graph and print functions.

Make sure to read rrdgraph_examples for tips&tricks.

# AUTHOR

Program by Tobias Oetiker <tobi@oetiker.ch>

This manual page by Alex van den Bogaerdt <alex@vandenbogaerdt.nl> with corrections and/or additions by several people