| # Viewer mode

Index XSane mode: Viewer mode Save mode Copy mode Multipage mode Fax mode E-mail mode Gimp plugin Scan options Medium selection Color management Color correction: Gamma correction Brightness Contrast Threshold RGB default Negative Autoenhancement Default Restore Store Histogram window Pipette functions Standard options window Advanced options window Preview: Pipette white Pipette gray Pipette black Unzoom Zoom out Zoom in Undo zoom Autoselect scanarea Autoraise scanarea Select visible area Delete preview cache Preset area Rotation Aspect ratio RGB values Select scanarea Move scanarea Batch scan: Empty batch list Open batch list Save batch list Add area to list Remove selection Rename selection Rotate image Mirror image Setup: Copy setup Display setup Enhancement setup Fax setup Filetype setup E-mail setup Saving setup Color management setup | In the viewer mode an image is scanned and displayed in the viewer. Select filename: If you press the disk icon a browse dialog is opened where you can select the name of the image file that is suggested for the viewer. You also can enter the filename directly to the text box right to the disk icon. Filename counter step width: When the filename contains a counter at the end then the counter is increased (or decreased) by the selected step width when the scan has been completed. Type: Filetype and fileextension that are suggested for the viewer. The viewer window: When the image is scanned it is displayed in the viewer window: Save image: Save image to disk. If the path, filename and filetype is not defined, a dialog opens that allows selecting path, filename and filetype. OCR: Call OCR program and save created text to file. Clone image: Creates a new viewer window with a copy of the displayed image. Scale image: Change size of the image. Despeckle image: Removes spots from the displayed image that is scanned from a rastered original like a magazine. Blur image: Blur displayed image. Rotate image 90, 180, 270 degree: Rotates the image by 90, 180 or 270 degree (clockwise). Mirror image at vertical or horizontal axis: Mirrors the image at vertical or horizonral axis.

> Author: Oliver Rauch