<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE refentry PUBLIC "-//OASIS//DTD DocBook XML V4.1.2//EN"
               "http://www.oasis-open.org/docbook/xml/4.1.2/docbookx.dtd" [
]>
<refentry id="gdbus-org.freedesktop.NetworkManager.Device.Modem">
  <refmeta>    <refentrytitle role="top_of_page" id="gdbus-interface-org-freedesktop-NetworkManager-Device-Modem.top_of_page">org.freedesktop.NetworkManager.Device.Modem</refentrytitle>
  <indexterm zone="gdbus-interface-org-freedesktop-NetworkManager-Device-Modem.top_of_page"><primary sortas=".Device.Modem">org.freedesktop.NetworkManager.Device.Modem</primary></indexterm>
  </refmeta>  <refnamediv>    <refname>org.freedesktop.NetworkManager.Device.Modem</refname>    <refpurpose>Modem Device</refpurpose>  </refnamediv>  <refsect1 role="properties">
    <title role="properties.title">Properties</title>
    <synopsis>
<link linkend="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.ModemCapabilities">ModemCapabilities</link>    readable   u
<link linkend="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.CurrentCapabilities">CurrentCapabilities</link>  readable   u
<link linkend="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.DeviceId">DeviceId</link>             readable   s
<link linkend="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.OperatorCode">OperatorCode</link>         readable   s
<link linkend="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.Apn">Apn</link>                  readable   s
</synopsis>
  </refsect1>
<refsect1 role="desc" id="gdbus-interface-org-freedesktop-NetworkManager-Device-Modem">
  <title role="desc.title">Description</title>
  <para></para>
</refsect1>
<refsect1 role="details" id="gdbus-properties-org.freedesktop.NetworkManager.Device.Modem">
  <title role="details.title">Property Details</title>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.ModemCapabilities">
  <title>The "ModemCapabilities" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.ModemCapabilities"><primary sortas=".Device.Modem:ModemCapabilities">org.freedesktop.NetworkManager.Device.Modem:ModemCapabilities</primary></indexterm>
<programlisting>
ModemCapabilities  readable   u
</programlisting>
<para>        The generic family of access technologies the modem supports. Not all
        capabilities are available at the same time however; some modems require a
        firmware reload or other reinitialization to switch between eg CDMA/EVDO
        and GSM/UMTS.
</para><para>        Returns: <link linkend="NMDeviceModemCapabilities">NMDeviceModemCapabilities</link>
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.CurrentCapabilities">
  <title>The "CurrentCapabilities" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.CurrentCapabilities"><primary sortas=".Device.Modem:CurrentCapabilities">org.freedesktop.NetworkManager.Device.Modem:CurrentCapabilities</primary></indexterm>
<programlisting>
CurrentCapabilities  readable   u
</programlisting>
<para>        The generic family of access technologies the modem currently supports
        without a firmware reload or reinitialization.
</para><para>        Returns: <link linkend="NMDeviceModemCapabilities">NMDeviceModemCapabilities</link>
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.DeviceId">
  <title>The "DeviceId" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.DeviceId"><primary sortas=".Device.Modem:DeviceId">org.freedesktop.NetworkManager.Device.Modem:DeviceId</primary></indexterm>
<programlisting>
DeviceId  readable   s
</programlisting>
<para>        An identifier used by the modem backend (ModemManager) that aims to
        uniquely identify the a device. Can be used to match a connection to a
        particular device.
</para><para>        Since: 1.20
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.OperatorCode">
  <title>The "OperatorCode" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.OperatorCode"><primary sortas=".Device.Modem:OperatorCode">org.freedesktop.NetworkManager.Device.Modem:OperatorCode</primary></indexterm>
<programlisting>
OperatorCode  readable   s
</programlisting>
<para>        The MCC and MNC (concatenated) of the network the modem is connected to.
        Blank if disconnected or not a 3GPP modem.
</para><para>        Since: 1.20
</para>
</refsect2>
<refsect2 role="property" id="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.Apn">
  <title>The "Apn" property</title>
  <indexterm zone="gdbus-property-org-freedesktop-NetworkManager-Device-Modem.Apn"><primary sortas=".Device.Modem:Apn">org.freedesktop.NetworkManager.Device.Modem:Apn</primary></indexterm>
<programlisting>
Apn  readable   s
</programlisting>
<para>        The access point name the modem is connected to. Blank if disconnected.
</para><para>        Since: 1.20
</para>
</refsect2>
</refsect1>
</refentry>

