## org.freedesktop.NetworkManager.Device.Modem org.freedesktop.NetworkManager.Device.Modem — Modem Device |

## Properties

    ModemCapabilities    readable   u
    CurrentCapabilities  readable   u
    DeviceId             readable   s
    OperatorCode         readable   s
    Apn                  readable   s

## Description

## Property Details

### The "ModemCapabilities" property

    ModemCapabilities  readable   u

The generic family of access technologies the modem supports. Not all capabilities are available at the same time however; some modems require a firmware reload or other reinitialization to switch between eg CDMA/EVDO and GSM/UMTS.

Returns: NMDeviceModemCapabilities

### The "CurrentCapabilities" property

    CurrentCapabilities  readable   u

The generic family of access technologies the modem currently supports without a firmware reload or reinitialization.

Returns: NMDeviceModemCapabilities

### The "DeviceId" property

    DeviceId  readable   s

An identifier used by the modem backend (ModemManager) that aims to uniquely identify the a device. Can be used to match a connection to a particular device.

Since: 1.20

### The "OperatorCode" property

    OperatorCode  readable   s

The MCC and MNC (concatenated) of the network the modem is connected to. Blank if disconnected or not a 3GPP modem.

Since: 1.20

### The "Apn" property

    Apn  readable   s

The access point name the modem is connected to. Blank if disconnected.

Since: 1.20