## NMDeviceVlan NMDeviceVlan |

## Functions

const char * | nm_device_vlan_get_hw_address ()
gboolean | nm_device_vlan_get_carrier ()
NMDevice * | nm_device_vlan_get_parent ()
guint | nm_device_vlan_get_vlan_id ()

## Types and Values

#define | NM_DEVICE_VLAN_HW_ADDRESS
#define | NM_DEVICE_VLAN_CARRIER
#define | NM_DEVICE_VLAN_PARENT
#define | NM_DEVICE_VLAN_VLAN_ID

## Description

## Functions

### nm_device_vlan_get_hw_address ()

    const char *
    nm_device_vlan_get_hw_address (NMDeviceVlan *device);

`nm_device_vlan_get_hw_address` has been deprecated since version 1.24 and should not be used in newly-written code.

Use `nm_device_get_hw_address()` instead.

Gets the hardware (MAC) address of the NMDeviceVlan

[skip]

#### Parameters

device | a NMDeviceVlan |

#### Returns

the hardware address. This is the internal string used by the device, and must not be modified.

### nm_device_vlan_get_carrier ()

    gboolean
    nm_device_vlan_get_carrier (NMDeviceVlan *device);

Whether the device has carrier.

#### Parameters

device | a NMDeviceVlan |

#### Returns

`TRUE` if the device has carrier

### nm_device_vlan_get_parent ()

    NMDevice *
    nm_device_vlan_get_parent (NMDeviceVlan *device);

#### Parameters

device | a NMDeviceVlan |

#### Returns

the device's parent device.

[transfer none]

### nm_device_vlan_get_vlan_id ()

    guint
    nm_device_vlan_get_vlan_id (NMDeviceVlan *device);

#### Parameters

device | a NMDeviceVlan |

#### Returns

the device's VLAN ID

## Types and Values

### NM_DEVICE_VLAN_HW_ADDRESS

    #define NM_DEVICE_VLAN_HW_ADDRESS "hw-address"

### NM_DEVICE_VLAN_CARRIER

    #define NM_DEVICE_VLAN_CARRIER    "carrier"

### NM_DEVICE_VLAN_PARENT

    #define NM_DEVICE_VLAN_PARENT     "parent"

### NM_DEVICE_VLAN_VLAN_ID

    #define NM_DEVICE_VLAN_VLAN_ID    "vlan-id"