Hardware Locality (hwloc) 2.2.0

Functions
Sharing topologies between processes

## Functions
int | hwloc_shmem_topology_get_length (hwloc_topology_t topology, size_t *lengthp, unsigned long flags)
int | hwloc_shmem_topology_write (hwloc_topology_t topology, int fd, hwloc_uint64_t fileoffset, void *mmap_address, size_t length, unsigned long flags)
int | hwloc_shmem_topology_adopt (hwloc_topology_t *topologyp, int fd, hwloc_uint64_t fileoffset, void *mmap_address, size_t length, unsigned long flags)

## Detailed Description

These functions are used to share a topology between processes by duplicating it into a file-backed shared-memory buffer.

The master process must first get the required shared-memory size for storing this topology with hwloc_shmem_topology_get_length().

Then it must find a virtual memory area of that size that is available in all processes (identical virtual addresses in all processes). On Linux, this can be done by comparing holes found in /proc/<pid>/maps for each process.

Once found, it must open a destination file for storing the buffer, and pass it to hwloc_shmem_topology_write() together with virtual memory address and length obtained above.

Other processes may then adopt this shared topology by opening the same file and passing it to hwloc_shmem_topology_adopt() with the exact same virtual memory address and length.

## Function Documentation

## ◆ hwloc_shmem_topology_adopt()

int hwloc_shmem_topology_adopt | ( | hwloc_topology_t * | topologyp,
|  | int | fd,
|  | hwloc_uint64_t | fileoffset,
|  | void * | mmap_address,
|  | size_t | length,
|  | unsigned long | flags
| ) |  |

Adopt a shared memory topology stored in a file.

Map a file in virtual memory and adopt the topology that was previously stored there with hwloc_shmem_topology_write().

The returned adopted topology in `topologyp` can be used just like any topology. And it must be destroyed with hwloc_topology_destroy() as usual.

However the topology is read-only. For instance, it cannot be modified with hwloc_topology_restrict() and object userdata pointers cannot be changed.

The segment of the file pointed by descriptor `fd`, starting at offset `fileoffset`, and of length `length` (in bytes), will be mapped at virtual address `mmap_address`.

The file pointed by descriptor `fd`, the offset `fileoffset`, the requested mapping virtual address `mmap_address` and the length `length` must be identical to what was given to hwloc_shmem_topology_write() earlier.

Note
  Flags `flags` are currently unused, must be 0.
  The object userdata pointer should not be used unless the process that created the shared topology also placed userdata-pointed buffers in shared memory.
  This function takes care of calling hwloc_topology_abi_check().

Returns
  -1 with errno set to EBUSY if the virtual memory mapping defined by `mmap_address` and `length` isn't available in the process.
  -1 with errno set to EINVAL if `fileoffset`, `mmap_address` or `length` aren't page-aligned, or do not match what was given to hwloc_shmem_topology_write() earlier.
  -1 with errno set to EINVAL if the layout of the topology structure is different between the writer process and the adopter process.

## ◆ hwloc_shmem_topology_get_length()

int hwloc_shmem_topology_get_length | ( | hwloc_topology_t | topology,
|  | size_t * | lengthp,
|  | unsigned long | flags
| ) |  |

Get the required shared memory length for storing a topology.

This length (in bytes) must be used in hwloc_shmem_topology_write() and hwloc_shmem_topology_adopt() later.

Note
  Flags `flags` are currently unused, must be 0.

## ◆ hwloc_shmem_topology_write()

int hwloc_shmem_topology_write | ( | hwloc_topology_t | topology,
|  | int | fd,
|  | hwloc_uint64_t | fileoffset,
|  | void * | mmap_address,
|  | size_t | length,
|  | unsigned long | flags
| ) |  |

Duplicate a topology to a shared memory file.

Temporarily map a file in virtual memory and duplicate the topology `topology` by allocating duplicates in there.

The segment of the file pointed by descriptor `fd`, starting at offset `fileoffset`, and of length `length` (in bytes), will be temporarily mapped at virtual address `mmap_address` during the duplication.

The mapping length `length` must have been previously obtained with hwloc_shmem_topology_get_length() and the topology must not have been modified in the meantime.

Note
  Flags `flags` are currently unused, must be 0.
  The object userdata pointer is duplicated but the pointed buffer is not. However the caller may also allocate it manually in shared memory to share it as well.

Returns
  -1 with errno set to EBUSY if the virtual memory mapping defined by `mmap_address` and `length` isn't available in the process.
  -1 with errno set to EINVAL if `fileoffset`, `mmap_address` or `length` aren't page-aligned.