nvme-toshiba-clear-pcie-correctable-errors(1)
=============================================

NAME
----
nvme-toshiba-clear-pcie-correctable-errors - Reset the PCIe correctable errors count to zero.

SYNOPSIS
--------
[verse]
'nvme toshiba clear-pcie-correctable-errors ' <device>


DESCRIPTION
-----------
For the NVMe device given, sends the Toshiba clear PCIe correctable errors
request.

The <device> parameter is mandatory and may be either the NVMe
character device (ex: /dev/nvme0), or a namespace block device (ex:
/dev/nvme0n1). 


EXAMPLES
--------
* Clear the PCIe correctable errors count:
+
------------
# nvme toshiba clear-pcie-correctable-errors /dev/nvme0 
------------

NVME
----
Part of the nvme-user suite
