nvme-wdc-enc-get-log(1)
=======================

NAME
----
nvme-wdc-enc-get-log - Send NVMe WDC enc-get-log Vendor Unique Command, return result.

SYNOPSIS
--------
[verse]
'nvme wdc enc-get-log' <device> [--log-id=<NUM>, -l <NUM>] [--output-file=<FILE>, -o <FILE>] [--transfer-size=<SIZE>, -s <SIZE>]

DESCRIPTION
-----------

For the NVMe device given, send a Vendor Unique WDC enc-get-log command and
output the Enclosure logs.

The <device> parameter is mandatory and may be either the NVMe character
device (ex: /dev/nvme0).

The --log-id=<NUM>, -l <NUM> parameter is mandatory and may be either 0xd1, 0xd2, 0xd3, 0xd4, 0xe2 and 0xe4.

This will only work on WDC devices supporting this feature.
Results for any other device are undefined.

On success it returns the enclosure log data, error code otherwise.

OPTIONS
-------
-o <FILE>::
--output-file=<FILE>::
    Output file pathname

-s <SIZE>::
--transfer-size=<NUM>::
    Data retrieval transfer size, maximum transfer size should be 0x2000 (decimal 8192)

EXAMPLES
--------
* Gets the enclosure log from the device based on the log id(0xd1) with transfer size(0x2000) and saves to defined file in current directory:
+
------------
# nvme wdc enc-get-log /dev/nvme0 -l 0xd1 -o d1_log.bin -s 0x2000
------------
* Gets the enclosure log from the device based on the log id(0xd2) with default transfer size(0x1000) and saves to defined file in current directory:
+
------------
# nvme wdc enc-get-log /dev/nvme0 -l 0xd2 -o d1_log.bin 
------------

NVME
----
Part of the nvme-user suite.
