nvme-lnvm-id-ns(1)
==================

NAME
----
nvme-lnvm-id-ns - Identify Geometry for LightNVM NVMe device

SYNOPSIS
--------
[verse]
'nvme lnvm-id-ns' <device> [--namespace-id=<nsid> | -n <nsid>]
			[--force | -f]
			[--raw-binary | -b]
			[--human-readable | -H]

DESCRIPTION
-----------
Send an Identify Geometry command to the given LightNVM device, returns
properties of the specified namespace in either human-readable or binary
format.

OPTIONS
-------
--namespace-id=<nsid>::
-n <nsid>::
	Retrieve the geometry from the selected namespace.

--force::
-f::
	Try to read the data and assume it is a LightNVM device

--raw-binary::
-b::
	Output the raw output

--human-readable::
-H::
	Output the status in human readable format

EXAMPLES
--------
* Retrieve the geometry from nvme0
------------
# nvme lnvm-id-ns /dev/nvme0 -n 1
------------

NVME
----
Part of the nvme-user suite
